SERVICE MANUAL UPDATE SEC. 6A ENGINE VIN CODE CORRECTION. Geo Prizm 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6A ENGINE VIN CODE CORRECTION

#### Subject: ENGINE VIN CODE CORRECTION

#### Model and Year: 1991 GEO PRIZM WITH 1.6L ENGINE

The VIN engine code designations at the top of Sections 6Al and 6A2 of the 1991 GEO Prizm Service Manual are reversed.

The Base and LSI model Engine Information (VIN 6) is located in Engine Mechanical (Section 6A1). The GSi model Engine Information (VIN 5) is located in Engine Mechanical (Section 6A2).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.