SERVICE MANUAL UPDATE-SEC.6E2 TERMINAL END VIEW REVISION. Geo Sprint 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC.6E2 TERMINAL END VIEW REVISION

#### VEHICLES AFFECTED: 1989-90 "M" 1.0L VIN 6

This bulletin serves to revise page 6E2-A9 "ECM Terminal End View" in Section 6E2 "Driveability And Emissions" in the 1989 and 1990 Sprint/Firefly 1.0L (VIN 6) "M" carline (TBI) Service Manual.

The ECM pin-out omits ECM terminal "B2" ignition signal.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.