PART NUMBERS/APPLICATIONS FOR CANVAS TOP AND WEATHERSTRIPS. Geo Sprint 1993

For 1990-2009 cars

# PART NUMBERS/APPLICATIONS FOR CANVAS TOP AND WEATHERSTRIPS

#### Subject: PART NUMBERS AND APPLICATIONS FOR CANVAS TOP AND WEATHERSTRIPS

#### Model and Year: 1990-93 GEO METRO CONVERTIBLE M-CAR

Should it become necessary to replace convertible top weatherstrips or the canvas top, use the following guidelines:

Before VIN: JGlMR3368NK204042 - If replacing any weatherstrips, all must be replaced.

After VIN: JGlMR3368NK204042 - Weatherstrips can be replaced individually.

Weatherstrip Part Numbers: 96065466 - Side Front #1 RH 96065467 - Side Front #1 LH 96065468 - Front Side Rear Corner #2 RH 96065469 - Front Side Rear Corner #2 LH 96065470 - Rear Side #3 RH 96065471 - Rear Side #3 LH 96067015 - Front Top Header

Canvas Top Part Number: 12344181

Do Not order the complete topstack assembly to fix water leaks as it does not contain the weatherstrips. Order the appropriate weatherstrips or canvas top as listed above.

PART "AVAILABILITY: Parts are expected to be available on 6/07/93.

WARRANTY INFORMATION: Use applicable Labor Operation and Times.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.