CREAKING NOISE FROM FRT. SUSP. REPLACE FRT. STABILIZER BUSH.. Geo Storm 1991

For 1990-2009 cars

# CREAKING NOISE FROM FRT. SUSP. REPLACE FRT. STABILIZER BUSH.

#### Subject: Creaking Noise from Front Suspension in Cold Weather Service Procedure (Replace Front Stabilizer Bar Bushings)

#### Models: 1990-91 Geo Storm 1990-91 Isuzu Impulse

This bulletin is being revised to facilitate distribution to GM of Canada dealers only. Previous divisional publication number was:

GM Canada 91-3-103

#### Condition

Some owners may experience a creaking noise coming from the front suspension especially during cold weather.

#### Cause

Creaking noise is caused by friction created between the outer surface of the stabilizer bar and the inner surface of the bushing.

#### Correction

If normal service procedures do not correct this condition, replace the front stabilizer bar bushings with p/n 97063972 (base coupe) or p/n 97063973 (gsi coupe and hatchback). These new bushings contain a silicone lubricant for superior noise reduction.

#### Parts Information

#### Part Number Description of Part Quantity

97063972 bushing-stab. bar 2 97063973 bushing-stab. bar 2

#### Warranty Information

Use applicable labour code and time

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.