MANUAL UPDATES FOUR SPEED AUTO TRANSAXLE. Geo Storm 1990

For 1990-2009 cars

# MANUAL UPDATES FOUR SPEED AUTO TRANSAXLE

#### Subject: FOUR SPEED AUTOMATIC TRANSAXLE CONTROL VALVE ASSEMBLY

#### Model and Year: 1990 GEO STORM

When performing the Control Valve Assembly procedure on page 7A1-2-3 of the 1990 GEO Storm Service Manual (ST371-90), be sure to install a new Lower Separator Plate Gasket when reassembling the Control Valve Assembly.

Figure 55 on page 7A1-2-14 should be replaced with the new attached figure.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.