SMU - SECTION 6D2 - CRANKING SYSTEM. Geo Tracker - 4WD 1994

For 1990-2009 cars

# SMU - SECTION 6D2 - CRANKING SYSTEM

---------------------------------------------------------------------- SERVICE MANUAL UPDATE ----------------------------------------------------------------------

#### SUBJECT: SECTION 6D2 - CRANKING SYSTEM

#### MODELS: 1993-95 GEO TRACKER

THE INFORMATION CONTAINED IN THIS SERVICE MANUAL UPDATE REPLACES THE INFORMATION FOUND UNDER "SPECIFICATIONS" IN SECTION 6D2 OF THE 1993-95 GEO TRACKER SERVICE MANUALS.

STARTER MOTOR USAGE

STARTER MOTOR CURRENT DRAW NO-LOAD * MANUAL TRANSMISSION ........50 AMPS AT 11 VOLTS * AUTOMATIC TRANSMISSION .....90 AMPS AT 11 VOLTS

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.