Clutch Grabbing. Geo Tracker - 2WD 1996

For 1990-2009 cars

Checks | Causes
--- | ---
Inspect the engine mounts | Loose or worn.

Inspect the pressure plate

- Warped pressure plate surface.
- Burned or smeared resin on pressure plate surface.

Inspect the clutch disc

- Oil contamination (oil soaked).
- Excessively worn, exploded or damaged.
- Worn or broken torsion springs.
- Worn splines in disc hub.

Inspect the flywheel

- Flywheel surface runout.Burned or smeared resin on the flywheel surface.

Transmission input shaft | Worn or damaged splines