Transmission General Specifications. Geo Tracker - 2WD 1996

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Transmission Fluid Capacities: Pan Removal (Approximate) | 2.9 L | 3.1qts
Transmission Fluid Capacities: Overhaul (Approximate) | 6.0 L | 6.3 qts
Transmission Fluid Type | Dextron® lll | Dextron® lll
Transmission Weight: Dry | 53.3 Kg | 117.50 lb
Transmission Weight: With Fluid | 58.6 Kg | 129.08 lb
Converter Size | 245 mm | 9.64 in
6 Position Quadrant | P, R, N,D,2,1 | P,R,N,D,2,1,
Pressure Taps Available | Line Pressure | Line Pressure
Case Materials | Die Cast Aluminum | Die Cast Aluminum