SMU - SECTION 0B - RECOMMENDED LUBRICANT. Geo Tracker - 4WD 1995

For 1990-2009 cars

# SMU - SECTION 0B - RECOMMENDED LUBRICANT

---------------------------------------------------------------------- SERVICE MANUAL UPDATE ----------------------------------------------------------------------

#### SUBJECT: SECTION 0B - RECOMMENDED LUBRICANT FOR TRANSFER CASE, MANUAL TRANSMISSION AND AXLES

#### MODELS: 1991-95 GEO TRACKER

THE FOLLOWING INFORMATION REPLACES THE RECOMMENDED LUBRICANTS SHOWN IN PAST YEAR GEO TRACKER SERVICE MANUALS.

MANUAL TRANSMISSION AND TRANSFER CASE: SAE 75W-90 GL-4 SYNTHETIC LUBRICANT, GM P/N 12346190, OR EQUIVALENT.

FRONT AND REAR AXLES: SAE 80W-90 GL-5 LUBRICANT, GM P/N 12345977, OR EQUIVALENT.

#### PART AVAILABILITY:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.