For 1990-2009 cars

Table 1: | Brake Action Uneven -- Pulls to One Side
Table 2: | Brakes Drag
Table 3: | Brake System Noise

Refer to a symptom diagnostic procedure from the following list in order to diagnose the symptom.

• | Brake Action Uneven -- Pulls to One Side

• | Brakes Drag

• | Brake System Noise

#### Brake Action Uneven -- Pulls to One Side

Checks | Actions
--- | ---
Inoperative Carrier | Replace the carrier.
Stuck Caliper Piston | Repair the caliper piston or replace the caliper assembly, if needed.

#### Brakes Drag

Checks | Actions
--- | ---
Stuck Caliper Piston | Repair the caliper piston or replace the caliper assembly, if needed.

#### Brake System Noise

Checks | Actions
--- | ---
Excessive Rotor Run Out | Replace the rotor.
Interference of the Dust Cover | Repair the dust cover.
Loose Caliper Mounting Bolts | Tighten the mounting bolts.