For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Behind Fascia Screws | 5.5 N·m | 49 lb in
Front Bumper Impact Bar Nuts | 27 N·m | 20 lb ft
Front Wheel Well Screws | 1.5 N·m | 13 lb in
Luggage Compartment Fascia Bolts | 5.5 N·m | 49 lb in
Mud Guard Screws | 1.5 N·m | 13 lb in
Rear Bumper Energy Absorber Nuts | 27 N·m | 20 lb ft
Rear Bumper Impact Bar Nuts | 27 N·m | 20 lb ft
Rear Upper Fascia Screws | 1.5 N·m | 13 lb in
Splash Shield Bolts | 1.5 N·m | 13 lb in
Splash Shield Nuts | 1.5 N·m | 13 lb in
Splash Shield Screws | 1.5 N·m | 13 lb in
Trim Panel Bolts | 10 N·m | 89 lb in