For 1990-2009 cars

## Engine Controls Connector End Views Notchback

Table 1: | Accelerator Pedal Position (APP) Sensor (MT34)
Table 2: | Camshaft Position (CMP) Sensor
Table 3: | Clutch Pedal Position (CPP) Switch (MT34)
Table 4: | Crankshaft Position Sensor (CKP) Sensor
Table 5: | Electronic Throttle Control (MT34)
Table 6: | Engine Coolant Temperature (ECT) Sensor
Table 7: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Table 8: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve (MT34)
Table 9: | Exhaust Gas Recirculation (EGR) Valve
Table 10: | Fuel Injector 1
Table 11: | Fuel Injector 2
Table 12: | Fuel Injector 3
Table 13: | Fuel Injector 4
Table 14: | Fuel Pump/Sender
Table 15: | Fuel Tank Pressure (FTP) Sensor (MT34)
Table 16: | Heated Oxygen Sensor (HO2S) 1
Table 17: | Heated Oxygen Sensor (HO2S) 1 (EURO IV)
Table 18: | Heated Oxygen Sensor (HO2S) 1 (MT34)
Table 19: | Heated Oxygen Sensor (HO2S) 2
Table 20: | Heated Oxygen Sensor (HO2S) 2 (EURO IV)
Table 21: | Heated Oxygen Sensor (HO2S) 2 (MT34)
Table 22: | Idle Air Control (IAC) Valve (MR140)
Table 23: | Ignition Coil (IC) Module
Table 24: | Intake Air Temperature (IAT) Sensor
Table 25: | Intake Manifold Tuning Valve
Table 26: | Intake Manifold Tuning Valve Position Sensor (MT34)
Table 27: | Knock Sensor (KS)
Table 28: | Manifold Absolute Pressure (MAP) Sensor
Table 29: | Octane Selector Switch (MR140)
Table 30: | Rough Road Sensor
Table 31: | Throttle Position (TP) Sensor (MR140)

#### Accelerator Pedal Position (APP) Sensor (MT34)

Connector Part Information |

• | MG 651044

• | 6-Way F

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | APP Sensor 2 Signal
2 | BN | -- | Low Reference
3 | GY | -- | 5-Volt Reference 2
4 | GY | -- | 5-Volt Reference 1
5 | OG/BK | -- | Low Reference
6 | L-BU | -- | APP Sensor 1 Signal

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way F JR Power Timer 3P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK (MR140) | -- | Ignition 1 Voltage
OG (MT34)
2 | BK/WH | -- | Ground
3 | L-BU/BK | -- | Camshaft Position (CMP) Sensor Signal

#### Clutch Pedal Position (CPP) Switch (MT34)

Connector Part Information |

• | KUM PB 625-04027

• | 4-Way F NMWP 02F-B Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Ignition 1 Voltage
2 | BK | -- | Ground
3 | PU | -- | Crank Signal
4 | L-BU | -- | Crank Signal

#### Crankshaft Position Sensor (CKP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way F JR Power Timer 3P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Crankshaft Position (CKP) Sensor Signal
2 | YE/BK | -- | Low Reference
3 | BK (MR140) | -- | Ground
BK/WH (MT34)

#### Electronic Throttle Control (MT34)

Connector Part Information |

• | PED 15326835

• | 8-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | 5-Volt Reference
2 | PU | -- | TPS 2 Signal
3 | L-BU | -- | TPS 1 Signal
4 | D-BU | -- | Low Reference
5 | BN | -- | ETC (-)
6-7 | -- | -- | Not Used
8 | BN | -- | ETC (+)

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | PED 12040753

• | 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | -- | Engine Coolant Temperature (ECT) Sensor Signal
B | BN | -- | Low Reference

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | PED 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN (MR140) | -- | EVAP Canister Purge Valve Solenoid Control
WH (MT34)
B | PK (MR140) | -- | Ignition 1 Voltage
OG (MT34)

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve (MT34)

Connector Part Information |

• | PED 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | -- | EVAP Canister Vent Valve Solenoid Control
B | PK | -- | Ignition 1 Voltage

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | PED 12110790

• | 5-Way F Metri-Pack 150 Series Sealed (GY)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | -- | Exhaust Gas Recirculation Valve Control
B | BN/WH | -- | Low Reference
C | GY | -- | Exhaust Gas Recirculation (EGR) Valve Position Sensor Signal
D | PU | -- | 5-Volt Reference
E | PK (MR140) | -- | Ignition 1 Voltage
OG (MT34)

#### Fuel Injector 1

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU (MR140) | -- | Ignition 1 Voltage
OG/BK (MT34)
2 | L-BU/WH (MR140) | -- | Fuel Injector 1 Control
BU/WH (MT34)

#### Fuel Injector 2

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU (MR140) | -- | Ignition 1 Voltage
OG/BK (MT34)
2 | BN (MR140) | -- | Fuel Injector 2 Control
PK/BK (MT34)

#### Fuel Injector 3

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU (MR140) | -- | Ignition 1 Voltage
OG/BK (MT34)
2 | PU/D-BU (MR140) | -- | Fuel Injector 3 Control
L-GN/BK (MT34)

#### Fuel Injector 4

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU (MR140) | -- | Ignition 1 Voltage
OG/BK (MT34)
2 | L-GN/D-BU (MR140) | -- | Fuel Injector 4 Control
BN (MT34)

#### Fuel Pump/Sender

Connector Part Information |

• | AMP 36159-1

• | 6-Way F Fuel Pump 6 POS Connector Assembly (BN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU | -- | Fuel Level Sensor Signal
2 | BK | -- | Ground
3 | BN | -- | Fuel Pump Supply Voltage
4 | PK | -- | Ignition Voltage
5 | YE | -- | Low Fuel Indicator Control
6 | L-BU | -- | Low Reference

#### Fuel Tank Pressure (FTP) Sensor (MT34)

Connector Part Information |

• | KET MG 620395

• | 3-Way M Series Sealed (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Low Reference
2 | BN/BK | -- | Fuel Tank Pressure Sensor Signal
3 | RD/WH | -- | 5-Volt Reference

#### Heated Oxygen Sensor (HO2S) 1

Connector Part Information |

• | PED 12162144

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | GN/WH | -- | Heated Oxygen Sensor (HO2S) 1 Low Reference
B | BN | -- | Heated Oxygen Sensor (HO2S) 1 Signal
C | BK | -- | Ground
D | PK | -- | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) 1 (EURO IV)

Connector Part Information |

• | PED 12162144

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Heated Oxygen Sensor (HO2S) 1 Signal
B | BK | -- | Ground
C | GN/WH | -- | Heated Oxygen Sensor (HO2S) 1 Low Reference
D | PK | -- | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) 1 (MT34)

Connector Part Information |

• | KUM PB 625-04027

• | 4-Way F NMWP 02F-B Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Heated Oxygen Sensor (HO2S) 1 Signal
2 | GY | -- | Heated Oxygen Sensor (HO2S) 1 Heater Control
3 | D-GN/WH | -- | Heated Oxygen Sensor (HO2S) 1 Low Reference
4 | OG | -- | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) 2

Connector Part Information |

• | PED 12162144

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | -- | Heated Oxygen Sensor (HO2S) 2 Low Reference
B | BN | -- | Heated Oxygen Sensor (HO2S) 2 Signal
C | BN | -- | Heated Oxygen Sensor (HO2S) 2 Heater Control
D | OG | -- | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) 2 (EURO IV)

Connector Part Information |

• | PED 12162144

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Heated Oxygen Sensor (HO2S) 2 Signal
B | BN | -- | Heated Oxygen Sensor (HO2S) 2 Heater Control
C | PU | -- | Heated Oxygen Sensor (HO2S) 2 Low Reference
D | OG | -- | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) 2 (MT34)

Connector Part Information |

• | KUM PB 625-04027

• | 4-Way F NMWP 02F-B Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Heated Oxygen Sensor (HO2S) 1 Signal
2 | BN | -- | Heated Oxygen Sensor (HO2S) 1 Heater Control
3 | PU | -- | Heated Oxygen Sensor (HO2S) 1 Low Reference
4 | OG | -- | Ignition 1 Voltage

#### Idle Air Control (IAC) Valve (MR140)

Connector Part Information |

• | PED 12040754

• | 4-Way Metri-Pack 150 Series (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU/BU | -- | Idle Air Control (IAC) B Low Control
B | D-BU | -- | Idle Air Control (IAC) B High Control
C | L-GN/BK | -- | Idle Air Control (IAC) A Low Control
D | GN | -- | Idle Air Control (IAC) A High Control

#### Ignition Coil (IC) Module

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG (MR140) | -- | Ignition Coil (IC) Timing Control 2 and 3
WH (MT34)
B | PK (MR140) | -- | Ignition 1 Voltage
OG/BK (MT34)
C | OG | -- | Ignition Coil (IC) Timing Control 1 and 4

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | AMP 85202-1

• | 2-Way JR Power Timer 2P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Intake Air Temperature (IAT) Sensor Signal
2 | BN | -- | Low Reference

#### Intake Manifold Tuning Valve

Connector Part Information |

• | AMP 174352-2

• | 2-Way F Econoseal J Mark II + Connector Plug Housing (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK (MR140) | -- | Ignition 1 Voltage
OG (MT34)
2 | YE | -- | Intake Manifold Tuning Valve Solenoid Control

#### Intake Manifold Tuning Valve Position Sensor (MT34)

Connector Part Information |

• | AMP 368215-1

• | 3-Way JPT 3P Assembly for Knock Sensor (GY)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | 5-Volt Reference
2 | D-BU | -- | Intake Manifold Tuning Valve Position Sensor Signal
3 | BN/WH | -- | Low Reference

#### Knock Sensor (KS)

Connector Part Information |

• | AMP 85202-1

• | 2-Way JR Power Timer 2P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Knock Sensor (KS) Signal
2 | L-BU | -- | Low Reference

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN/WH | -- | Low Reference
B | L-GN | -- | Manifold Absolute Pressure Sensor Signal
C | PU | -- | 5-Volt Reference

#### Octane Selector Switch (MR140)

Connector Part Information |

• | KET MG 620395

• | 3-Way M Series Sealed (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | -- | Ground
3 | D-GN | -- | Octane Selection Signal

#### Rough Road Sensor

Connector Part Information |

• | PED 12162185

• | 3-Way F Metri-Pack 150.2 Series Sealed, Pull To Seat (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG/BK | -- | 5-Volt Reference
B | D-GN | -- | Rough Road Sensor Signal
C | L-BU | -- | Low Reference

#### Throttle Position (TP) Sensor (MR140)

Connector Part Information |

• | PED 12078090

• | 3-Way F Metri-Pack 150 Series (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | -- | 5-Volt Reference
B | BN | -- | Low Reference
C | L-BU | -- | Throttle Position (TP) Sensor Signal

## Engine Controls Connector End Views Hatchback

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position (CKP) Sensor
Table 3: | Engine Coolant Temperature (ECT) Sensor
Table 4: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Table 5: | Exhaust Gas Recirculation (EGR) Valve
Table 6: | Fuel Injector 1
Table 7: | Fuel Injector 2
Table 8: | Fuel Injector 3
Table 9: | Fuel Injector 4
Table 10: | Fuel Pump/Sender
Table 11: | Heated Oxygen Sensor (HO2S) 1
Table 12: | Heated Oxygen Sensor (HO2S) 2
Table 13: | Idle Air Control (IAC) Valve
Table 14: | Ignition Coil (IC) Module
Table 15: | Intake Air Temperature (IAT) Sensor
Table 16: | Knock Sensor (KS)
Table 17: | Manifold Absolute Pressure (MAP) Sensor
Table 18: | Octane Selection Switch
Table 19: | Rough Road Sensor
Table 20: | Throttle Position (TP) Sensor

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way F JR Power Timer 3P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | 1748 | Camshaft Position (CMP) Sensor Signal
2 | BK/WH | 51 | Ground
3 | BN | 1733 | Ignition 1 Voltage

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way F JR Power Timer 3P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
2 | YE/BK | 1868 | Low Reference
3 | BK/WH | 51 | Ground

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | PED 12040753

• | 2-Way F Metri-Pack 150 Series Sealed Pull To Seat (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN | 410 | Engine Coolant Temperature (ECT) Sensor Signal
B | D-GN | 808 | Low Reference

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | PED 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 452 | EVAP Canister Purge Valve Solenoid Control
B | BN | 1733 | Ignition 1 Voltage

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | PED 12110790

• | 5-Way F Metri-Pack 150 Series Sealed (GY)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-BU | 436 | Exhaust Gas Recirculation (EGR) Valve Control
B | D-GN | 813 | Low Reference
C | D-GN | 435 | 5-Volt Reference
D | D-GN/WH | 416 | Exhaust Gas Recirculation (EGR) Valve Position Sensor Signal
E | BN | 1733 | Ignition 1 Voltage

#### Fuel Injector 1

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | BN/BK | 1747 | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | L-GN | 1746 | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | BN/WH | 1745 | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | YE | 1744 | Fuel Injector 4 Control

#### Fuel Pump/Sender

Connector Part Information |

• | AMP 936159-1

• | 6-Way F Fuel Pump 6POS Connector Assembly (BN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 1936 | Fuel Level Sensor Signal
2 | BK | 850 | Ground
3 | BN | 1723 | Fuel Pump Supply Voltage
4 | BK | 850 | Ground
5 | PU | 172 | Low Fuel Indicator Control
6 | L-BU | 1937 | Low Reference

#### Heated Oxygen Sensor (HO2S) 1

Connector Part Information |

• | PED 12162144

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 428 | Heated Oxygen Sensor (HO2S) 1 Signal
B | D-BU/BK | 429 | Heated Oxygen Sensor (HO2S) 1 Low Reference
C | BN | 50 | Heated Oxygen Sensor (HO2S) 1 Heater Control
D | BN | 1733 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) 2

Connector Part Information |

• | PED 12162144

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-GN/BK | 1670 | Heated Oxygen Sensor (HO2S) 2 Low Reference
B | L-GN | 413 | Heated Oxygen Sensor (HO2S) 2 Signal
C | BN | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
D | BN | 1733 | Ignition 1 Voltage

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | PED 12040754

• | 4-Way F Metri-Pack 150 Series (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-GN | 415 | Idle Air Control (IAC) B Low Control
B | L-GN | 417 | Idle Air Control (IAC) B High Control
C | WH/D-BU | 533 | Idle Air Control (IAC) A Low Control
D | L-GN | 534 | Idle Air Control (IAC) A High Control

#### Ignition Coil (IC) Module

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 423 | Ignition Coil (IC) Timing Control 2 and 3
B | PK | 539 | Ignition 1 Voltage
C | WH | 406 | Ignition Coil (IC) Timing Control 1 and 4

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | AMP 85202

• | 2-Way F JR Power Timer 2P Housing Assembly (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 468 | Intake Air Temperature (IAT) Sensor Signal
2 | D-GN | 808 | Low Reference

#### Knock Sensor (KS)

Connector Part Information |

• | AMP 368215-1

• | 3-Way F JPT 3P Assembly for Knock Sensor (GY)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | 496 | Knock Sensor (KS) Signal
2 | D-BU/WH | 1876 | Low Reference
3 | D-GN | 808 | Low Reference

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 433 | Low Reference
B | L-BU | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | L-BU | 469 | 5-Volt Reference

#### Octane Selection Switch

Connector Part Information |

• | KET MG 620395

• | 3-Way M Series Sealed (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 892 | Octane Selection Switch
2 | BK/WH | 51 | Ground
3 | -- | -- | Not Used

#### Rough Road Sensor

Connector Part Information |

• | PED 12162185

• | 3-Way F Metri-Pack 150.2 Series Sealed Pull To Seat (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 1937 | Low Reference
B | D-GN | 602 | Rough Road Sensor Signal w/o ABS
C | WH | 1031 | 5-Volt Reference

#### Throttle Position (TP) Sensor

Connector Part Information |

• | PED 12078090

• | 3-Way F Metri-Pack 150 Series (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 427 | 5-Volt Reference
B | D-BU | 426 | Low Reference
C | WH | 425 | Throttle Position (TP) Sensor Signal