For 1990-2009 cars

Figure 1: |

#### Fuel Injection and Air Cleaner

(1) | Air Cleaner
(2) | Intake Air Temperature (IAT) Sensor
(3) | Throttle Body
(4) | Ignition Coil (IC) Module
(5) | Fuel Injector 1
(6) | Fuel Injector 2
(7) | Fuel Injector 3
(8) | Fuel Injector 4
(9) | Fuel Rail
(10) | Engine Control Module (ECM)

Figure 2: |

#### Exhaust Gas Recirculation (EGR) and Knock Sensor (KS)

(1) | Idle Air Control (IAC) Valve
(2) | Throttle Position (TP) Sensor
(3) | Intake Manifold Tuning Valve Solenoid
(4) | Knock Sensor (KS)
(5) | Exhaust Gas Recirculation (EGR) Valve
(6) | Vehicle Speed Sensor (VSS)

Figure 3: |

#### Crankshaft Position (CKP) Sensor, Camshaft Position (CMP) Sensor, and Manifold Absolute Pressure (MAP) Sensor

(1) | Battery
(2) | Manifold Absolute Pressure (MAP) Sensor
(3) | Camshaft Position (CMP) Sensor
(4) | Crankshaft Position (CKP) Sensor
(5) | Rough Road Sensor
(6) | Octane Selection Switch

Figure 4: |

#### Engine Data Sensors

(1) | Engine Coolant Temperature (ECT) Sensor
(2) | Heated Oxygen Sensor (HO2S)1
(3) | Heated Oxygen Sensor (HO2S) 2
(4) | Oil Pressure Switch
(5) | EVAP Canister Purge Solenoid Valve
(6) | Intake Manifold Tuning Valve Solenoid

Figure 5: |

#### Fuel Vapor Recovery System

(1) | Fuel Tank
(2) | Fuel Line to Fuel Rail
(3) | EVAP Canister Purge Vacuum Line to Intake Manifold
(4) | EVAP Canister Purge Solenoid Valve
(5) | EVAP Service Port
(6) | EVAP Canister Vent Solenoid Valve
(7) | EVAP Canister
(8) | Fuel Fill Tube
(9) | Fuel Filler Cap
(10) | Fuel Tank Pressure Sensor
(11) | Fuel Pump/Sender Assembly