For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coupling Flange Pinch Bolt | 22 N·m | 16 lb ft
Ignition Switch Housing Sheer Bolts | 11 N·m | 97 lb in
Ignition Switch Retaining Screw | 2 N·m | 18 lb in
Key Interlock Solenoid Screws | 2 N·m | 18 lb in
Key Reminder Switch Screws | 2 N·m | 18 lb in
Lower Instrument Trim Panel Screws | 3 N·m | 27 lb in
Lower Steering Column Cover Panel Screws | 3 N·m | 27 lb in
Steering Column Jacket Assembly Bracket Nuts | 22 N·m | 16 lb ft
Steering Wheel Nut | 38 N·m | 28 lb ft
Support Housing Screws | 16 N·m | 12 lb ft
Tilt Steering Lever Cap Screw | 4 N·m | 35 lb in
Turn Signal Switch Housing Screws | 3 N·m | 27 lb in
Upper and Lower Steering Column Cover Panel Screws | 3 N·m | 27 lb in