For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Glass Screws | 7 N·m | 62 lb in
Door Hinge-to-Body Bolts | 35 N·m | 26 lb ft
Door Hinge-to-Door Bolts | 15 N·m | 11 lb ft
Door Hold Open Link-to-Body Bolts | 35 N·m | 26 lb ft
Door Hold Open Link-to-Door Bolts | 5 N·m | 44 lb in
Door Lock Screw | 8 N·m | 71 lb in
Door Lock Striker Screws | 24 N·m | 18 lb ft
Door Pull Bracket Screws | 3.5 N·m | 31 lb in
Guide Rail Bolts | 7 N·m | 62 lb in
Inside Door Handle Screw | 3 N·m | 27 lb in
Outside Door Handle Bolts | 4.5 N·m | 40 lb in
Outside Rear View Mirror Screws | 4.5 N·m | 40 lb in
Window Regulator Nuts | 7 N·m | 62 lb in