For 1990-2009 cars

## Fluid and Lubricant Recommendations Except Holden

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | ESSO JWS 3309 or T-IV Automatic Transmission Fluid (GM Part No. U.S. 88900925, in Canada 22689186)
Brake Fluid and Clutch Fluid | DOT-3 or DOT-4
Clutch Linkage Pivot Points | Engine Oil
Engine Coolant | Mixture of water and good quality ethylene glycol base antifreeze (year-round coolant)
Engine Oil | API SJ (ILSAC GF-II) Grade or Better SAE 5W-30, SAE 10W-30, SAE 15W-40 (Cold area: SAE 5W-30, Hot area: SAE 15W-40)
Floor Shift Linkage Points | Engine Oil

#### Hood Latch Assembly

1. Pivots and Spring Anchor
2. Release Pawl

1. Engine Oil
2. Multipurpose type grease meeting requirements NLGI No. 1 or 2

Hood and Door Hinges, Fuel Door Hinge, Rear Compartment Lid Hinges | Engine oil
Key Lock Cylinders | Silicone Lubricant
Manual Transaxle | GM Goodwrench™ Synthetic Manual Transmission Fluid (GM Part No.U.S. 12346190, in Canada 10953477) or equivalent SAE 75W-85 GL-4 gear oil.
Manual Transaxle Shift Linkage | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | DEXRON®-III or DEXRON®-IID
Weatherstrips | Silicone Grease

## Fluid and Lubricant Recommendations Holden

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | ESSO JWS 3309 or conforming to Holden spec HN2414
Brake Fluid and Clutch Fluid | DOT-4
Clutch Linkage Pivot Points | Engine Oil
Engine Coolant | DEX-COOL® (red) or silicate based coolant (blue) Important: Do not mix types of coolant.
Engine Oil |

• | SAE 5W/30 or 10W/30

• | API SL or SM

• | ILSAC GF-3 or GF-4

Floor Shift Linkage Points | Engine Oil
Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges | Engine oil
Hood Latch Assembly

- Pivots and Spring Anchor

Engine Oil

- Release Pawl

Multipurpose type grease meeting requirements NLGI No. 1 or 2

Key Lock Cylinders | Silicone Lubricant
Manual Transaxle | SAE 75W/90
Manual Transaxle Shift Linkage | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | DEXRON®-III
Weatherstrips | Silicone Grease