For 1990-2009 cars

Table 1: | Radio (Base)
Table 2: | Radio (RDS)
Table 3: | Speaker - Left Front
Table 4: | Speaker - Left Rear
Table 5: | Speaker - Right Front
Table 6: | Speaker - Right Rear
Table 7: | Tweeter - Left
Table 8: | Tweeter - Right

#### Radio (Base)

Connector Part Information |

• | 173853-1

• | 18-Way M 070 Series Multilock Plug 18P

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 200 | Right Front Speaker Output (+)
2 | D-BU | 46 | Right Rear Speaker Output (+)
3 | BN/WH | 309 | Right Park Lamp Supply Voltage
4 | YE | 43 | Accessory Voltage
5 | OG | 540 | Battery Positive Voltage
6 | -- | -- | Not Used
7 | GY | 199 | Left Rear Speaker Output (+)
8 | PU | 201 | Left Front Speaker Output (+)
9 | BN | 117 | Right Front Speaker Output (-)
10 | WH | 115 | Right Rear Speaker Output (-)
11 | BK | 450 | Ground
L-GN/RD | 230 | Instrument Panel Lamps Dimming Control (w/Dimmer)
12-13 | -- | -- | Not Used
14 | BK | 450 | Ground
15-16 | -- | -- | Not Used
17 | D-GN | 116 | Left Rear Speaker Output (-)
18 | L-GN | 118 | Left Front Speaker Output (-)

#### Radio (RDS)

Connector Part Information |

• | 936593-2

• | 16-Way

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU | 46 | Right Rear Speaker Output (+)
2 | WH | 115 | Right Rear Speaker Output (-)
3 | BN/WH | 309 | Right Park Lamp Supply Voltage
4 | -- | -- | Not Used
5 | L-BU | 200 | Right Front Speaker Output (+)
6 | BN | 117 | Right Front Speaker Output (-)
7 | -- | -- | Not Used
8 | OG | 540 | Left Rear Speaker Output (-)
9 | PU | 201 | Left Front Speaker Output (+)
10 | L-GN | 118 | Left Front Speaker Output (-)
11 | -- | -- | Not Used
12 | BK | 450 | Ground
L-GN/RD | 230 | IP Lamp Dimming Control
13 | GY | 199 | Left Rear Speaker Output (+)
14 | D-GN | 116 | Left Rear Speaker Output (-)
15 | YE | 43 | Accessory Voltage
16 | BK | 450 | Ground

#### Speaker - Left Front

Connector Part Information |

• | MG610043

• | 2-Way Connector (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 201 | Left Front Speaker Output (+)
2 | L-GN | 118 | Left Front Speaker Output (-)

#### Speaker - Left Rear

Connector Part Information |

• | MG610043

• | 2-Way F 250 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 116 | Left Rear Speaker Output (-)
2 | GY | 199 | Left Rear Speaker Output (+)

#### Speaker - Right Front

Connector Part Information |

• | MG610043

• | 2-Way Connector F (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 200 | Right Front Speaker Output (+)
2 | BN | 117 | Right Front Speaker Output (-)

#### Speaker - Right Rear

Connector Part Information |

• | MG610043

• | 2-Way F 250 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | 115 | Right Rear Speaker Output (+)
2 | D-BU | 46 | Right Rear Speaker Output (-)

#### Tweeter - Left

Connector Part Information |

• | MG610070

• | 2-Way F 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-GN | 118 | Left Front Speaker Output (-)
2 | PU | 201 | Left Front Speaker Output (+)

#### Tweeter - Right

Connector Part Information |

• | MG610070

• | 2-Way F 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 117 | Right Front Speaker Output (-)
2 | L-BU | 200 | Right Front Speaker Output (+)