For 1990-2009 cars

Table 1: | C101 TCM Harness to Engine Harness
Table 2: | C102 Front Harness to Engine Harness
Table 3: | C104 Body Harness to Front Harness
Table 4: | C106 Body Harness to Front Harness (RHD)
Table 5: | C107 Body Harness to Front Harness (RHD)
Table 6: | C113 Front Harness to Left Turn Signal Jumper
Table 7: | C114 Front Harness to Right Turn Signal Jumper
Table 8: | C201 Front Harness to I/P Harness (LHD) Body Harness to Front Harness (RHD)
Table 9: | C202 TCM Harness to I/P Harness
Table 10: | C203 Front Harness to I/P Harness (LHD) I/P Harness to Body Harness (RHD)
Table 11: | C204 Front Harness to I/P Harness
Table 12: | C205 Engine Harness to I/P Harness
Table 13: | C210 I/P Harness to Body Harness
Table 14: | C211 Front Harness to Body Harness
Table 15: | C212 I/P Harness to Body Harness
Table 16: | C213 I/P Harness to Body Harness
Table 17: | C214 Air Bag Harness to I/P Harness (except North America)
Table 18: | C214 Air Bag Harness to I/P Harness (North America)
Table 19: | C215 Engine Harness to I/P Harness
Table 20: | C216 Body Harness to Left Rear Door Harness
Table 21: | C351 Body Harness to Driver Door Harness
Table 22: | C361 Body Harness to Passenger Door Harness
Table 23: | C371 Body Harness to Left Rear Door Harness
Table 24: | C381 Body Harness to Right Rear Door Harness
Table 25: | C401 Body Harness to Tailgate Harness (Hatchback)
Table 26: | C401 Body Harness to Rear Harness (Notchback)
Table 27: | C402 Tailgate Harness to Tailgate Extension Harness (Hatchback)
Table 28: | C402 Rear Harness to Body Harness (Notchback)
Table 29: | C403 Tailgate Harness to Tailgate Extension Harness (Hatchback)
Table 30: | C404 Body Harness to Tailgate Harness (Hatchback)
Table 31: | C415 Body Harness to Left Tail Lamp Jumper (Hatchback)
Table 32: | C415 Rear Harness to Left Tail Lamp Jumper (Notchback)
Table 33: | C416 Body Harness to Left Tail Lamp Jumper (Hatchback)
Table 34: | C416 Rear Harness to Right Tail Lamp Jumper (Notchback)
Table 35: | C417 Rear Harness to Marker Lamp Jumper (Hatchback/Notchback)

#### C101 TCM Harness to Engine Harness

Connector Part Information |

• | AMP 174257-2

• | 4-Way F 070 Series Econoseal-J MK-2 Cap Hsg 4P (BK)

Connector Part Information

• | AMP 174259-2

• | 4-Way M 070 Series Econoseal-J MK-2 Plug Assembly 4P (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK/WH | 251 | Ground | 1 | BK/WH | 251 | Ground
2 | L-GN | 24 | Backup Lamp Supply Voltage | 2 | L-GN | 24 | Backup Lamp Supply Voltage
3 | YE | 710 | CAN Serial Data Low | 3 | YE | 710 | CAN Serial Data Low
4 | PU | 1807 | CAN Serial Data High | 4 | PU | 1807 | CAN Serial Data High

#### C102 Front Harness to Engine Harness

Connector Part Information |

• | PK 145-20017 (KUM)

• | 20-Way F AR 20F-W Assembly (WH)

Connector Part Information

• | PK 141-20017 (KUM)

• | 20-Way M AR 20M-W Assembly (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN | 1977 | Fuel Level Sensor Low Reference | 1 | L-BU | 1937 | Fuel Level Sensor Low Reference
2 | GY | 1936 | Fuel Level Sensor Signal | 2 | GY | 1936 | Fuel Level Sensor Signal
3 | -- | -- | Not Used | 3 | -- | -- | Not Used
4 | L-GN | 24 | Backup Lamp Supply Voltage | 4 | L-GN/BK | 24 | Backup Lamp Supply Voltage
5 | D-GN | 834 | Rough Road Signal (w/ABS) | 5 | WH | 834 | Rough Road Signal (w/ABS)
6 | GY | 473 | High Speed Cooling Fan Relay Control | 6 | GY | 473 | High Speed Cooling Fan Relay Control
7 | GY | 355 | Low Speed Cooling Fan Relay Control | 7 | D-GN | 355 | Low Speed Cooling Fan Relay Control
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BN | 1733 | Ignition 1 Voltage | 9 | BN | 1733 | Ignition 1 Voltage
BN | 1733 | Ignition 1 Voltage (MR-140)
10 | D-GN/BK | 1670 | HO2S 2 Low Reference Sensor | 10 | D-GN/BK | 1670 | HO2S 2 Low Reference Sensor
11 | L-GN | 413 | HO2S 2 High Signal Sensor | 11 | L-GN | 413 | HO2S 2 High Signal Sensor
12 | BN | 1671 | HO2S 2 Heater Low Control Sensor | 12 | BN | 1671 | HO2S 2 Heater Low Control Sensor
13 | -- | -- | Not Used | 13 | -- | -- | Not Used
14 | L-BU | 1030 | Low Reference | 14 | L-BU | 1030 | Low Reference
15 | WH/RD | 1031 | 5-Volt Reference | 15 | WH/D-BU | 1031 | 5-Volt Reference
16 | PK | 1733 | Main Relay Output | 16 | PK | 1733 | Main Relay Output
17 | YE/D-BU | 497 | Fuel Pump Relay Control | 17 | YE/BK | 497 | Fuel Pump Relay Control
18 | D-GN | 67 | A/C Compressor Clutch Coil Supply Voltage | 18 | D-GN | 67 | A/C Compressor Clutch Coil Supply Voltage
19-20 | -- | -- | Not Used | 19-20 | -- | -- | Not Used

#### C104 Body Harness to Front Harness

Connector Part Information |

• | KET MG 651068

• | 15-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641071-1

• | 15-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | GY/D-GN | 711 | Left Headlamp High Beam Supply Voltage | 1 | GY/D-GN | 11 | Left Headlamp High Beam Supply Voltage
2 | WH/BK | 1346 | Headlamp Supply Voltage/Headlamp Control | 2 | WH/BK | 1346 | Headlamp Supply Voltage/Headlamp Control
3 | OG | 140 | Battery Positive Voltage | 3 | -- | -- | Not Used
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | BN | 1080 | Park Lamp Relay Control | 7 | BN | 1080 | Park Lamp Relay Control
8 | WH | 352 | Headlamp Relay Coil Supply Voltage | 8 | WH | 352 | Headlamp Relay Coil Supply Voltage
9 | YE/GN | 712 | Left Headlamp Low Beam Supply Voltage | 9 | YE/GN | 12 | Left Headlamp Low Beam Supply Voltage
10 | -- | -- | Not Used | 10 | -- | -- | Not Used
11 | D-GN/WH | 94 | Windshield Washer Switch Signal | 11 | D-GN/WH | 94 | Windshield Washer Switch Signal
12 | RD | 441 | Ignition 3 Voltage | 12 | RD | 441 | Ignition 3 Voltage
13 | D-GN | 96 | Windshield Washer Switch Pulse Delay Signal | 13 | D-GN | 96 | Windshield Washer Switch Pulse Delay Signal
14 | D-BU | 92 | Windshield Wiper Motor Low Speed | 14 | D-BU | 92 | Windshield Wiper Motor Low Speed
15 | WH | 95 | Windshield Wiper Motor High Speed | 15 | WH | 95 | Windshield Wiper Motor High Speed

#### C106 Body Harness to Front Harness (RHD)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (BK)

Connector Part Information

• | KET MG 641053-2

• | 8-Way M 090-II Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 1 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
2 | WH/YE | 318 | Front Fog Lamp Supply Voltage | 2 | WH/YE | 318 | Front Fog Lamp Supply Voltage
3 | BK | 28 | Horn Relay Control | 3 | BK | 28 | Horn Relay Control
4 | GN | 189 | Headlamp Leveling Motor Supply Voltage | 4 | GN | 189 | Headlamp Leveling Motor Supply Voltage
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | BN/BK | 109 | Hood Ajar Switch Signal | 6 | BN/BK | 109 | Hood Ajar Switch Signal
7 | PU | 239 | Ignition 1 Voltage | 7 | PU | 239 | Ignition 1 Voltage
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

#### C107 Body Harness to Front Harness (RHD)

Connector Part Information |

• | KET MG 651056

• | 10-Way F 090-II Connector (WH)

Connector Part Information

• | KET MG 641059-5

• | 10-Way M 090-II Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | OG | 1142 | Battery Positive Voltage | 1 | OG/GN | 1142 | Battery Positive Voltage
2 | RD | 242 | Ignition 3 Voltage | 2 | RD | 242 | Ignition 3 Voltage
3 | L-GN | 867 | ABS Indicator Control | 3 | L-GN | 867 | ABS Indicator Control
4 | BK/WH | 2051 | Serial Data | 4 | BK/WH | 2051 | Serial Data
5 | L-GN/BK | 392 | Rear Window Washer Pump Control | 5 | L-GN/BK | 392 | Rear Window Washer Pump Control
6 | BN | 33 | Brake Warning Indicator Control | 6 | BN | 33 | Brake Warning Indicator Control
7 | PK | 639 | Ignition 3 Voltage (Mando ABS) | 7 | PK | 639 | Ignition 3 Voltage (Mando ABS)
8 | BN | 1541 | Ignition 1 Voltage | 8 | BN | 1541 | Ignition 1 Voltage
9 | BN/WH | 309 | Right Park Lamp Supply Voltage | 9 | BN/WH | 309 | Right Park Lamp Supply Voltage
10 | -- | -- | Not Used | 10 | -- | -- | Not Used

#### C113 Front Harness to Left Turn Signal Jumper

Connector Part Information |

• | KET MG 641234

• | 3-Way F SSD & 0509 (BK)

Connector Part Information

• | KET MG 611611

• | 3-Way M SSD & 0509 Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | BN | 709 | Left Park Lamp Supply Voltage
2 | BK | 50 | Ground | 2 | BK | 50 | Ground
3 | L/BU | 14 | Left Turn Signal Lamp Supply Voltage | 3 | YE | 14 | Left Turn Signal Lamp Supply Voltage

#### C114 Front Harness to Right Turn Signal Jumper

Connector Part Information |

• | KET MG 641234

• | 3-Way F SSD & 0509 (BK)

Connector Part Information

• | KET MG 611611

• | 3-Way M SSD & 0509 Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN/WH | 309 | Right Park Lamp Supply Voltage | 1 | BN | 709 | Right Park Lamp Supply Voltage
2 | BK | 250 | Ground | 2 | BK | 50 | Ground
3 | D/BU | 15 | Right Turn Signal Lamp Supply Voltage | 3 | YE | 14 | Right Turn Signal Lamp Supply Voltage

#### C201 Front Harness to I/P Harness (LHD) Body Harness to Front Harness (RHD)

Connector Part Information |

• | KET MG 651074-2

• | 18-Way F 090-II Connector (BU)

Connector Part Information

• | KET MG 641077-2

• | 18-Way M 090-II Connector (BU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | OG/D-GN | 1142 | Battery Positive Voltage | 1 | OG/D-GN | 1142 | Battery Positive Voltage
2 | RD | 242 | Ignition 1 Voltage | 2 | RD | 242 | Ignition 1 Voltage
3 | L-GN | 867 | ABS Indicator Control | 3 | L-GN | 867 | ABS Indicator Control
4 | BK/WH | 2051 | Serial Data (w/ABS) | 4 | BK/WH | 2051 | Serial Data (w/ABS)
5 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal (w/ABS) | 5 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal (w/ABS)
6 | WH/YE | 318 | Front Fog Lamp Supply Voltage | 6 | WH/YE | 318 | Front Fog Lamp Supply Voltage
7 | BK | 28 | Horn Relay Control (w/SIR) | 7 | BK | 28 | Horn Relay Control (w/SIR)
BK/WH | 29 | Horn Control (w/o SIR) | BK/WH | 29 | Horn Control (w/o SIR)
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | L-GN/BK | 392 | Rear Window Washer Pump Control (w/Rear Window Washer) | 9 | L-GN/BK | 392 | Rear Window Washer Pump Control (w/Rear Window Washer)
10 | BN | 33 | Brake Warning Indicator Control | 10 | BN | 33 | Brake Warning Indicator Control
BN/WH | 133 | Brake Warning Indicator Control (LHD) | BN/WH | 133 | Brake Warning Indicator Control (LHD)
11 | PK | 639 | Ignition 1 Voltage (Mando ABS) | 11 | PK | 639 | Ignition 1 Voltage (Mando ABS)
12 | BN | 1541 | Ignition 1 Voltage | 12 | BN | 1541 | Ignition 1 Voltage
13 | BN/WH | 309 | Right Park Lamp Supply Voltage | 13 | BN/WH | 309 | Right Park Lamp Supply Voltage
14 | L-BU | 1769 | Fog Lamp Indicator Control (w/Fog Lamps) | 14 | L-BU | 1769 | Fog Lamp Indicator Control
15 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (Except North America) | 15 | D-GN | 189 | Headlamp Leveling Motor Supply Voltage (Except North America)
16 | PU | 172 | Low Fuel Indicator Control | 16 | PU | 172 | Low Fuel Indicator Control
17 | BN/BK | 109 | Hood Ajar Switch Signal | 17 | BN/BK | 109 | Hood Ajar Switch Signal
18 | PK | 239 | Ignition 1 Voltage (HV-240) | 18 | PK | 239 | Ignition 1 Voltage

#### C202 TCM Harness to I/P Harness

Connector Part Information |

• | KET MG 651350

• | 11-Way F 090-II (WH)

Connector Part Information

• | KET MG 641353

• | 11-Way M 090-II (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN | 323 | Park/Neutral Position (PNP) Switch Park Signal | 1 | BN | 323 | Park/Neutral Position (PNP) Switch Park Signal
2-3 | -- | -- | Not Used | 2-3 | -- | -- | Not Used
4 | D-GN/WH | 1135 | Hold Mode Signal | 4 | D-GN/WH | 1135 | Hold Mode Signal
5 | YE | 1481 | Hold Mode Indicator Control | 5 | YE | 1481 | Hold Mode Indicator Control
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 7 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
8 | D-BU | 2051 | Serial Data | 8 | BK/WH | 2051 | Serial Data
9 | D-GN/WH | 817 | Vehicle Speed Signal | 9 | D-GN/WH | 817 | Vehicle Speed Signal
D-GN/WH | 817 | Vehicle Speed Signal
10 | PK | 839 | Ignition 1 Voltage | 10 | PK | 839 | Ignition 1 Voltage
11 | OG | 440 | Battery Positive Voltage | 11 | OG | 440 | Battery Positive Voltage

#### C203 Front Harness to I/P Harness (LHD) I/P Harness to Body Harness (RHD)

Connector Part Information |

• | KET MG 651110-5

• | 14-Way F 090-II Series (BK)

Connector Part Information

• | KET MG 641113-5

• | 14-Way M 090-II Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | OG | 140 | Battery Positive Voltage | 1 | OG | 140 | Battery Positive Voltage
2 | WH/BK | 1346 | Headlamp Supply Voltage/Headlamp Control | 2 | WH/BK | 1346 | Headlamp Supply Voltage/Headlamp Control
3 | GY/D-GN | 11 | Headlamp High Beam Supply Voltage | 3 | GY/D-GN | 11 | Headlamp High Beam Supply Voltage
4 | YE/D-GN | 12 | Headlamp Low Beam Supply Voltage | 4 | YE/D-GN | 12 | Headlamp Low Beam Supply Voltage
5 | WH | 352 | Headlamp Relay Coil Supply Voltage | 5 | WH | 352 | Headlamp Relay Coil Supply Voltage
6 | BN | 1080 | Park Lamp Relay Control | 6 | BN | 1080 | Park Lamp Relay Control
7 | PU | 293 | Rear Defog Element Supply Voltage | 7 | PU | 293 | Rear Defog Element Supply Voltage
8 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 8 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
9 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | 9 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
10 | WH | 95 | Windshield Wiper Motor High Speed | 10 | WH | 95 | Windshield Wiper Motor High Speed
11 | D-BU | 92 | Windshield Wiper Motor Low Speed | 11 | D-BU | 92 | Windshield Wiper Motor Low Speed
12 | D-GN | 96 | Windshield Wiper Switch Pulse Delay Signal | 12 | D-GN | 96 | Windshield Wiper Switch Pulse Delay Signal
13 | RD | 441 | Ignition 3 Voltage | 13 | RD | 441 | Ignition 3 Voltage
14 | D-GN/WH | 94 | Windshield Washer Switch Signal | 14 | D-GN/WH | 94 | Windshield Washer Switch Signal

#### C204 Front Harness to I/P Harness

Connector Part Information |

• | KET MG 651926

• | 4-Way F 312-II Series (WH)

Connector Part Information

• | KET MG 641928

• | 4-Way M 312-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | OG/BK | 142 | Battery Positive Voltage | 1 | OG | 142 | Battery Positive Voltage
2 | RD/BK | 141 | Ignition 3 Voltage | 2 | RD/BK | 141 | Ignition 3 Voltage
3 | YE | 143 | Accessory Voltage | 3 | YE | 143 | Accessory Voltage
4 | RD/BK | 141 | Ignition 3 Voltage | 4 | RD/BK | 141 | Ignition 3 Voltage

#### C205 Engine Harness to I/P Harness

Connector Part Information |

• | KET MG 611810-41

• | 18-Way F Device Connector (GY)

Connector Part Information

• | KET MG 652426

• | 36-Way M Door 36P Hsg (090-II) (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YE | 5 | Crank Voltage (Except Auto Transmission North America) | 1 | YE | 5 | Crank Voltage (Except Auto Transmission North America)
PU | 6 | Starter Solenoid Crank Voltage (Automatic Transmission North America) | 1 | PU | 6 | Starter Solenoid Crank Voltage (Automatic Transmission North America)
2 | PK | 539 | Ignition 1 Voltage | 2 | PK | 539 | Ignition 1 Voltage
3 | WH | 30 | Fuel Level Sensor Signal | 3 | WH | 30 | Fuel Level Sensor Signal
4 | D-BU | 2051 | Serial Data (w/Immobilizer) | 4 | BK/WH | 2051 | Serial Data
BK/WH | 2051 | Serial Data (w/o Immobilizer)
5 | YE | 1578 | EVAP Canister Vent Solenoid Control (North America) | 5 | YE | 1578 | EVAP Canister Vent Solenoid Control (North America)
6 | WH | 135 | ECT Sensor Gage Signal | 6 | WH | 135 | ECT Sensor Gage Signal
7 | D-BU | 25 | Charge Indicator Control/Charge Indicator Signal | 7 | D-BU | 25 | Charge Indicator Control/Charge Indicator Signal
8 | PK | 839 | Ignition 1 Voltage | 8 | PK | 839 | Ignition 1 Voltage
1739 | 1739
9 | D-GN/WH | 762 | A/C Request Signal | 9 | D-GN/WH | 762 | A/C Request Signal
10 | BN | 732 | Evaporator Temperature Sensor Signal (1.2L) | 10 | BN | 732 | Evaporator Temperature Sensor Signal
11 | OG | 440 | Battery Positive Voltage | 11 | OG | 440 | Battery Positive Voltage
12 | L-BU | 733 | Reference Low (1.4L) | 12 | L-BU | 733 | Reference Low (1.4L)
BN | Reference Low (1.2L) | BN | Reference Low (1.2L)
13 | PK/D-BU | 439 | Ignition 1 Voltage (w/Manual Transmission) | 13 | PK | 439 | Ignition 1 Voltage (w/Manual Transmission)
14 | D-GN/WH | 817 | Vehicle Speed Signal (w/Manual Transmission) | 14 | D-GN/WH | 817 | Vehicle Speed Signal
15 | WH | 121 | Engine Speed Signal | 15 | WH | 121 | Engine Speed Signal
16 | BN/BK | 419 | MIL Control | 16 | BN/BK | 419 | Malfunction Indicator Lamp (MIL) Control
17 | D-GN | 31 | Oil Pressure Indicator Control | 17 | D-GN/WH | 31 | Oil Pressure Indicator Control
18 | PU/WH | 821 | Engine Overspeed Indicator Control (w/Overspeed Warning) | 18 | BN/BK | 821 | Engine Overspeed Indicator Control

#### C210 I/P Harness to Body Harness

Connector Part Information |

• | KET MG 651050-2

• | 8-Way F 090-II Series (BU)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (BU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YE | 749 | Security Indicator Control | 1 | YE | 749 | Security Indicator Control
2 | BK/WH | 2051 | Serial Data | 2 | BK/WH | 2051 | Serial Data
3 | PK | 239 | Ignition 1 Voltage | 3 | PK | 239 | Ignition 1 Voltage
4 | RD/WH | 740 | Battery Positive Voltage (LHD) | 4 | RD/WH | 740 | Battery Positive Voltage (LHD)
5 | YE | 1578 | EVAP Canister Vent Solenoid Control | 5 | YE | 1578 | EVAP Canister Vent Solenoid Control
6 | L-GN | 80 | Key in Ignition Switch Signal | 6 | L-GN | 80 | Key in Ignition Switch Signal
7 | BN/BK | 109 | Hood Ajar Switch Signal | 7 | BN/BK | 109 | Hood Ajar Switch Signal
8 | -- | -- | Not Used | 8 | -- | -- | Not Used

#### C211 Front Harness to Body Harness

Connector Part Information |

• | KET MG 651086-3

• | 22-Way F 090-II Series (YE)

Connector Part Information

• | KET MG 641089-3

• | 22-Way M 090-II Series (YE)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN/BK | 885 | Left Rear Wheel Speed Sensor Low Reference (w/ABS) | 1 | BN/BK | 885 | Left Rear Wheel Speed Sensor Low Reference
2 | D-GN/WH | 884 | Left Rear Wheel Speed Sensor Signal (w/ABS) | 2 | D-GN/WH | 884 | Left Rear Wheel Speed Sensor Signal
3 | PU | 883 | Right Rear Wheel Speed Sensor Low Reference (w/ABS) | 3 | PU | 883 | Right Rear Wheel Speed Sensor Low Reference
4 | L-BU | 882 | Right Rear Wheel Speed Sensor Signal (w/ABS) | 4 | L-BU | 882 | Right Rear Wheel Speed Sensor Signal
5 | L-GN | 24 | Backup Lamp Supply Voltage | 5 | L-GN | 24 | Backup Lamp Supply Voltage
6 | L-BU | 1937 | Fuel Level Sensor Low Reference | 6 | L-BU | 1937 | Fuel Level Sensor Low Reference
GY/D-GN | 1029
7 | PU | 709 | Left Park Lamp Supply Voltage | 7 | PU | 709 | Left Park Lamp Supply Voltage
8 | BN/WH | 309 | Right Park Lamp Supply Voltage | 8 | BN/WH | 309 | Right Park Lamp Supply Voltage
9 | BN | 1733 | Ignition 1 Voltage (MR-140) | 9 | BN | 1733 | Ignition 1 Voltage (MR-140)
10 | OG/BK | 540 | Battery Positive Voltage | 10 | BN | 541 | Battery Positive Voltage
11 | PU | 267 | Heated Mirror Element Supply Voltage (LHD) | 11 | PU | 267 | Heated Mirror Element Supply Voltage (Hatchback)
OG | 293 | Heated Mirror Element Supply Voltage (Notchback) | OG | 293 | Heated Mirror Element Supply Voltage (Notchback)
12 | PU | 172 | Low Fuel Indicator Control (LHD) | 12 | PU | 172 | Low Fuel Indicator Control (LHD)
13 | L-GN/BK | 392 | Low Reference | 13 | L-GN/BK | 392 | Low Reference
14 | L-BU | 1030 | Low Reference (MR-140) | 14 | L-BU | 1030 | Low Reference (MR-140)
15 | WH/BU | 1031 | 5-Volt Reference (MR-140) | 15 | WH | 1031 | 5-Volt Reference (MR-140)
16 | L-BU | 1723 | Fuel Pump Supply Voltage | 16 | BN | 1723 | Fuel Pump Supply Voltage
17 | -- | -- | Not Used | 17 | -- | -- | Not Used
18 | BN | 41 | Ignition 3 Voltage (w/Power Windows) | 18 | RD/WH | 41 | Ignition 3 Voltage
19 | GY | 1936 | Fuel Level Sensor Signal | 19 | GY | 1936 | Fuel Level Sensor Signal
20 | -- | -- | Not Used | 20 | -- | -- | Not Used
21 | D-GN/WH | 261 | Arm Alarm Signal | 21 | D-GN/WH | 261 | Arm Alarm Signal
22 | BN | 741 | Ignition 1 Voltage | 22 | BN | 741 | Ignition 1 Voltage

#### C212 I/P Harness to Body Harness

Connector Part Information |

• | KET MG 651056-5

• | 10-Way F 090-II Series (BK)

Connector Part Information

• | KET MG 641059-5

• | 10-Way M 090-II Connector (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | OG | 1340 | Battery Positive Voltage | 1 | OG | 1340 | Battery Positive Voltage
2-3 | -- | -- | Not Used | 2-3 | -- | -- | Not Used
4 | D-GN/WH | 157 | Courtesy Lamp Control | 4 | D-GN/WH | 157 | Courtesy Lamp Control
5 | RD | 441 | Ignition 3 Voltage | 5 | RD | 441 | Ignition 3 Voltage
6 | GY | 393 | Rear Window Wiper Motor Control | 6 | GY | 393 | Rear Window Wiper Motor Control
7 | RD | 122 | Rear Fog Lamp Supply Voltage (Rear Fog Lamps) | 7 | RD | 122 | Rear Fog Lamp Supply Voltage (Rear Fog Lamps)
8 | -- | -- | Not Used | 8 | -- | -- | Not Used
9 | BK/WH | 238 | Seat Belt Switch - Driver | 9 | BK/WH | 238 | Seat Belt Switch - Driver
10 | PU | 126 | Left Front Door Open Switch Signal | 10 | PU | 126 | Left Front Door Open Switch Signal

#### C213 I/P Harness to Body Harness

Connector Part Information |

• | KET MG 651068

• | 15-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641071

• | 15-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | OG | 40 | Battery Positive Voltage | 1 | OG | 40 | Battery Positive Voltage
OG | 40 | Battery Positive Voltage (w/Power Mirrors)
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | PU | 172 | (RHD) | 3 | PU | 172 | (RHD)
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
D-BU | 15 | Right Turn Signal Lamps Supply Voltage (w/Remote Keyless Entry)
5 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | 5 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
L-BU | 14 | Left Turn Signal Lamp Supply Voltage (w/Remote Keyless Entry)
6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
7 | PU | 201 | Left Front Speaker Output (+) | 7 | PU | 201 | Left Front Speaker Output (+)
8 | L-GN | 118 | Left Front Speaker Output (-) | 8 | L-GN | 118 | Left Front Speaker Output (-)
9 | L-BU | 200 | Right Front Speaker Output (+) | 9 | L-BU | 200 | Right Front Speaker Output (+)
10 | BN | 117 | Right Front Speaker Output (-) | 10 | BN | 117 | Right Front Speaker Output (-)
11 | GY | 199 | Left Rear Speaker Output (+) | 11 | GY | 199 | Left Rear Speaker Output (+)
12 | D-GN | 116 | Left Rear Speaker Output (-) | 12 | D-GN | 116 | Left Rear Speaker Output (-)
13 | D-BU | 46 | Right Rear Speaker Output (+) | 13 | D-BU | 46 | Right Rear Speaker Output (+)
14 | WH | 115 | Right Rear Speaker Output (-) | 14 | WH | 115 | Right Rear Speaker Output (-)
15 | BN | 33 | Brake Warning Indicator Control | 15 | BN | 33 | Brake Warning Indicator Control

#### C214 Air Bag Harness to I/P Harness (except North America)

Connector Part Information |

• | KET MG 610396

• | 4-Way F Series Sealed (WH)

Connector Part Information

• | KET MG 620397

• | 4-Way M Series Sealed (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | D-GN/WH | 358 | Air Bag Indicator Control | 1 | D-GN/WH | 358 | Air Bag Indicator Control
2 | -- | -- | Not Used | 2 | -- | -- | Not Used
3 | PK | 139 | Ignition 1 Voltage | 3 | PK | 139 | Ignition 1 Voltage
4 | BN | 337 | SIR Serial Data | 4 | BN | 337 | SIR Serial Data

#### C214 Air Bag Harness to I/P Harness (North America)

Connector Part Information |

• | KET MG 610404

• | 10-Way F 090-II Series (YE)

Connector Part Information

• | KET MG 620405

• | 10-Way M 090-II Connector (YE)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | DG/WH | 6169 | Front Discriminating Sensor -- LH Signal | 1 | DG/WH | 6169 | Front Discriminating Sensor -- LH Signal
2 | PU | 1358 | DIC Switch Signal | 2 | PU | 1358 | DIC Switch Signal
3 | L-GN | 6777 | Front Discriminating Sensor -- RH Signal | 3 | L-GN | 6777 | Front Discriminating Sensor -- RH Signal
4 | PK | 739 | Ignition 1 Voltage | 4 | PK | 739 | Ignition 1 Voltage
5 | YE | 6168 | Front Discriminating Sensor -- LH Signal | 5 | YE | 6168 | Front Discriminating Sensor -- LH Signal
6 | DG/WH | 358 | AIR BAG Indicator Control | 6 | DG/WH | 358 | AIR BAG Indicator Control
7 | PK | 139 | Ignition 1 Voltage | 7 | PK | 139 | Ignition 1 Voltage
8 | BN | 337 | Serial Data | 8 | BN | 337 | Serial Data
9 | BN/WH | 6776 | Front Discriminating Sensor -- RH Signal | 9 | BN/WH | 6776 | Front Discriminating Sensor -- RH Signal
10 | -- | -- | Not Used | 10 | -- | -- | Not Used

#### C215 Engine Harness to I/P Harness

Connector Part Information |

• | KET MG 611810-41

• | 18-Way F Device Connector (GY)

Connector Part Information

• | KET MG 652426

• | 36-Way M Door 36P Hsg (090-II) (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | YE/BK | 183 | Cruise Control Indicator Signal | 1 | YE/BK | 183 | Cruise Control Indicator Signal
2 | L-GN/BU | 474 | 5-Volt Reference | 2 | L-GN | 474 | 5-Volt Reference
3-5 | -- | -- | Not Used | 3-5 | -- | -- | Not Used
6 | D-GN/WH | 397 | Cruise Control ON Switch Output | 6 | D-GN/WH | 397 | Cruise Control ON Switch Output
7 | D-GN/WH | 718 | Accelerator Pedal Sensor Signal Return | 7 | D-GN/WH | 718 | Accelerator Pedal Sensor Signal Return
8 | D-BU | 1161 | Electronic Throttle-Pedal Position Signal 1 | 8 | D-BU | 1161 | Electronic Throttle-Pedal Position Signal 1
9 | GY/BK | 596 | 5-Volt Reference | 9 | GY | 596 | 5-Volt Reference
10 | L-BU | 645 | Accelerator Pedal Sensor Signal Return | 10 | L-BU | 645 | Accelerator Pedal Sensor Signal Return
11 | WH | 1162 | Electronic Throttle-Pedal Position Signal 2 | 11 | WH | 1162 | Electronic Throttle-Pedal Position Signal 2
12 | GY | 474 | 5-Volt Reference | 12 | GY | 474 | 5-Volt Reference
13-18 | -- | -- | Not Used | 13-18 | -- | -- | Not Used

#### C216 Body Harness to Left Rear Door Harness

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090 II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | BN/WH | 6776 | SIR Inflator Feed - Right Side | 3 | BN/WH | 6776 | SIR Inflator Feed - Right Side
4 | L-GN | 6777 | SIR Inflator Output - Right Side | 4 | L-GN | 6777 | SIR Inflator Output - Right Side
5 | YE | 6168 | SIR Inflator Feed - Left Side | 5 | YE | 6168 | SIR Inflator Feed - Left Side
6 | GY/WH | 6169 | SIR Inflator Output - Left Side | 6 | GY/WH | 6169 | SIR Inflator Output - Left Side

#### C351 Body Harness to Driver Door Harness

Connector Part Information |

• | KET MG 610692

• | 29-Way F Door (WH)

Connector Part Information

• | KET MG 620693

• | 29-Way M Door Connector (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | RD/WH | 41 | Ignition 3 Voltage | 1 | RD/WH | 41 | Ignition 3 Voltage
2 | BN/OG | 1307 | Power Window Master Switch Lockout Control | 2 | BN/OG | 1307 | Power Window Master Switch Lockout Control
3 | D-GN | 166 | Power Window Master Switch Passenger Front Up Signal | 3 | D-GN | 166 | Power Window Master Switch Passenger Front Up Signal
4 | BN | 167 | Power Window Master Switch Passenger Front Down Signal | 4 | BN | 167 | Power Window Master Switch Passenger Front Down Signal
5 | L-GN/RD | 668 | Power Window Motor Left Rear Up Control | 5 | L-GN/RD | 668 | Power Window Motor Left Rear Up Control
6 | GY/D-GN | 169 | Power Window Master Switch Left Rear Down Signal | 6 | GY/D-GN | 169 | Power Window Master Switch Left Rear Down Signal
7 | BK | 650 | Ground | 7 | BK | 650 | Ground
8 | WH | 81 | Mirror Motor Right Control | 8 | WH | 81 | Mirror Motor Right Control
9 | L-GN | 89 | Mirror Motor Up/Down Control | 9 | L-GN | 89 | Mirror Motor Down Control
10 | GY | 90 | Mirror Motor Left Control | 10 | GY | 90 | Mirror Motor Left Control
11 | -- | -- | Not Used | 11 | -- | -- | Not Used
12 | OG | 267 | Heated Mirror Element Supply Voltage | 12 | OG | 267 | Heated Mirror Element Supply Voltage
13 | L-BU | 170 | Power Window Master Switch Right Rear Up Signal | 13 | L-BU | 170 | Power Window Master Switch Right Rear Up Signal
14 | PU | 171 | Power Window Master Switch Right Rear Down Signal | 14 | PU | 171 | Power Window Master Switch Right Rear Down Signal
15-17 | -- | -- | Not Used | 15-17 | -- | -- | Not Used
18 | D-BU | 49 | Door Latch Switch Signal | 18 | PU/D-BU | 49 | Door Latch Switch Signal
19 | L-GN | 118 | Left Front Speaker Output (-) (LHD) | 19 | L-GN | 118 | Left Front Speaker Output (-) (LHD)
BN | 117 | Right Front Speaker Output (-) (RHD) | BN | 117 | Right Front Speaker Output (-) (RHD)
20 | PU | 201 | Left Front Speaker Output (+) (LHD) | 20 | PU | 201 | Left Front Speaker Output (+) (LHD)
L-BU | 200 | Left Front Speaker Output (+) (RHD) | L-BU | 200 | Left Front Speaker Output (+) (RHD)
21-23 | -- | -- | Not Used | 21-23 | -- | -- | Not Used
24 | L-GN | 194 | Door Unlock Control (w/o Dimming) | 24 | L-GN | 194 | Door Unlock Control (w/o Dimming)
25 | GY | 195 | Door Lock Control | 25 | GY | 195 | Door Lock Control
26 | D-BU | 294 | Door Lock Actuator Unlock Control | 26 | D-BU | 294 | Door Lock Actuator Unlock Control
27 | WH | 295 | Door Lock Actuator Lock Control | 27 | WH | 295 | Door Lock Actuator Lock Control
28 | -- | -- | Not Used | 28 | -- | -- | Not Used
29 | OG | 40 | Battery Positive Voltage | 29 | OG | 40 | Battery Positive Voltage

#### C361 Body Harness to Passenger Door Harness

Connector Part Information |

• | KET MG 610692

• | 29-Way F Door (WH)

Connector Part Information

• | KET MG 620693

• | 29-Way M Door Connector (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | -- | -- | Not Used | 1 | -- | -- | Not Used
2 | BN/OG | 1307 | Power Window Master Switch Lockout Control | 2 | BN/OG | 1307 | Power Window Master Switch Lockout Control
RD/WH | 41 | RD/WH | 41
3 | D-GN | 166 | Power Window Master Switch Passenger Front Up Signal | 3 | D-GN | 166 | Power Window Master Switch Passenger Front Up Signal
4 | BN | 167 | Power Window Master Switch Passenger Front Down Signal | 4 | BN | 167 | Power Window Master Switch Passenger Front Down Signal
5-6 | -- | -- | Not Used | 5-6 | -- | -- | Not Used
7 | BK | 150 | Ground | 7 | BK | 150 | Ground
8 | WH | 81 | Mirror Motor Right Control | 8 | WH | 81 | Mirror Motor Right Control
9 | L-GN | 89 | Mirror Motor Up/Down Control | 9 | L-GN | 89 | Mirror Motor Up/Down Control
10 | GY | 90 | Mirror Motor Left Control | 10 | GY | 90 | Mirror Motor Left Control
11 | BK | 1150 | Ground | 11 | BK | 1150 | Ground
12 | OG | 267 | Heater Mirror Element Supply Voltage | 12 | OG | 267 | Heater Mirror Element Supply Voltage
13-17 | -- | -- | Not Used | 13-17 | -- | -- | Not Used
18 | D-BU | 49 | Door Latch Switch Signal | 18 | D-BU | 49 | Door Latch Switch Signal
19 | BN | 117 | Right Front Speaker Output (-) | 19 | BN | 117 | Right Front Speaker Output (-)
L-GN | 118 | Left Front Speaker Output (-) (RHD) | L-GN | 118 | Left Front Speaker Output (-) (RHD)
20 | L-BU | 200 | Right Front Speaker Output (+) | 20 | L-BU | 200 | Right Front Speaker Output (+)
PU | 201 | Left Front Speaker Output (+) (RHD) | PU | 201 | Left Front Speaker Output (+) (RHD)
21-25 | -- | -- | Not Used | 21-25 | -- | -- | Not Used
26 | D-BU | 294 | Door Lock Actuator Unlock Control | 26 | D-BU | 294 | Door Lock Actuator Unlock Control
27 | WH | 295 | Door Lock Actuator Lock Control | 27 | WH | 295 | Door Lock Actuator Lock Control
28-29 | -- | -- | Not Used | 28-29 | -- | -- | Not Used

#### C371 Body Harness to Left Rear Door Harness

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090 II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | WH | 295 | Door Lock Actuator Lock Control | 1 | WH | 295 | Door Lock Actuator Lock Control
2 | D-BU | 294 | Door Lock Actuator Unlock Control | 2 | D-BU | 294 | Door Lock Actuator Unlock Control
3 | GY/D-GN | 169 | Power Window Master Switch Left Rear Down Signal | 3 | GY/RD | 169 | Power Window Master Switch Left Rear Down Signal
4 | L-GN/RD | 668 | Power Window Motor Left Rear Up Control | 4 | L-GN/BK | 168 | Power Window Motor Left Rear Up Control
5 | BN/OG | 1307 | Power Window Master Switch Lockout Control | 5 | BN/OG | 1307 | Power Window Master Switch Lockout Control
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

#### C381 Body Harness to Right Rear Door Harness

Connector Part Information |

• | KET MG 651044

• | 6-Way F 090 II Series (WH)

Connector Part Information

• | KET MG 641047

• | 6-Way M 090 II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | WH | 295 | Door Lock Actuator Lock Control | 1 | WH | 295 | Door Lock Actuator Lock Control
2 | D-BU | 294 | Door Lock Actuator Unlock Control | 2 | D-BU | 294 | Door Lock Actuator Unlock Control
3 | PU | 171 | Power Window Master Switch Left Rear Down Signal | 3 | GY/OG | 169 | Power Window Master Switch Right Rear Down Signal
4 | L-BU | 170 | Power Window Master Switch Right Rear Up Signal | 4 | L-GN/BK | 168 | Power Window Master Switch Right Rear Up Signal
5 | BN/OG | 1307 | Power Window Master Switch Lockout Control | 5 | BN/OG | 1307 | Power Window Master Switch Lockout Control
6 | -- | -- | Not Used | 6 | -- | -- | Not Used

#### C401 Body Harness to Tailgate Harness (Hatchback)

Connector Part Information |

• | KET MG 610402

• | 8-Way F Series Sealed (WH)

Connector Part Information

• | KET MG 620403

• | 8-Way M Series Sealed (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | BK | 293 | Rear Defog Element Supply Voltage | 2 | BK | 293 | Rear Defog Element Supply Voltage
3 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 3 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
4 | RD | 441 | Ignition 3 Voltage | 4 | RD | 441 | Ignition 3 Voltage
5 | GY | 393 | Rear Window Wiper Motor Control | 5 | GY | 393 | Rear Window Wiper Motor Control
6 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal | 6 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal
7 | D-BU | 49 | Tamper Switch Signal | 7 | D-BU | 49 | Tamper Switch Signal
8 | BK | 850 | Ground | 8 | BK | 850 | Ground

#### C401 Body Harness to Rear Harness (Notchback)

Connector Part Information |

• | KET MG 651050

• | 8-Way F 090-II Series (WH)

Connector Part Information

• | KET MG 641053

• | 8-Way M 090-II Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 309 | Right Park Lamp Supply Voltage | 1 | PU | 309 | Right Park Lamp Supply Voltage
2 | BK | 24 | Backup Lamp Supply Voltage | 2 | PU | 24 | Backup Lamp Supply Voltage
3 | BN | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps) | 3 | BN | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps)
4 | RD | 709 | Left Park Lamp Supply Voltage | 4 | PU | 709 | Left Park Lamp Supply Voltage
5 | GY | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 5 | GY | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
6 | OG/BK | 14 | Left Turn Signal Lamps Supply Voltage | 6 | OG/BK | 14 | Left Turn Signal Lamps Supply Voltage
7 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 7 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
8 | BK | -- | Not Used | 8 | BK | -- | Not Used

#### C402 Tailgate Harness to Tailgate Extension Harness (Hatchback)

Connector Part Information |

• | KET MG 630680

• | 4-Way F 090-II M Series (WH)

Connector Part Information

• | KET MG 620160

• | 4-Way M 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal | 2 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal
3 | BK | 850 | Ground | 3 | BK | 850 | Ground
4 | D-BU | 49 | Tamper Switch Signal | 4 | D-BU | 49 | Tamper Switch Signal

#### C402 Rear Harness to Body Harness (Notchback)

Connector Part Information |

• | KET MG 651038

• | 4-Way 090-II F Series (WH)

Connector Part Information

• | KET MG 641041

• | 4-Way 090-II M Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Left Park Lamp Supply Voltage | 1 | PU | 709 | Left Park Lamp Supply Voltage
2 | D-BU | 49 | Tamper Switch Signal | 2 | D-BU | 49 | Tamper Switch Signal
3 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal | 3 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal
4 | BK | 450 | Ground | 4 | BK | 850 | Ground

#### C403 Tailgate Harness to Tailgate Extension Harness (Hatchback)

Connector Part Information |

• | KET MG 620395

• | 3-Way F 090 (2.3 MM) Series (WH)

Connector Part Information

• | KET MG 610394

• | 3-Way M 090 (2.3 MM) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | GY | 393 | Rear Window Wiper Motor Control | 1 | GY | 393 | Rear Window Wiper Motor Control
2 | RD | 441 | Ignition 3 Voltage | 2 | RD | 441 | Ignition 3 Voltage
3 | L-GN/BK | 392 | Not Used | 3 | -- | -- | Not Used

#### C404 Body Harness to Tailgate Harness (Hatchback)

Connector Part Information |

• | KET MG 610489

• | 2-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620490

• | 2-Way M 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | D-BU | 294 | Door Lock Actuator Unlock Control | 1 | D-BU | 294 | Door Lock Actuator Unlock Control
2 | WH | 295 | Door Lock Actuator Lock Control | 2 | WH | 295 | Door Lock Actuator Lock Control

#### C415 Body Harness to Left Tail Lamp Jumper (Hatchback)

Connector Part Information |

• | KET MG 610152

• | 6-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620153

• | 6-Way M 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 850 | Ground | 1 | BK | 450 | Ground
2 | BK | 850 | Ground | 2 | BK/YE | 450 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage (w/Backup Lamp) | 3 | WH | 24 | Backup Lamp Supply Voltage
4 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 4 | YE | 14 | Left Turn Signal Lamps Supply Voltage
5 | PU | 709 | Left Park Lamp Supply Voltage | 5 | D-BU | 709 | Left Park Lamp Supply Voltage
PU | 709 | Left Park Lamp Supply Voltage | D-BU | 709 | Left Park Lamp Supply Voltage
6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C415 Rear Harness to Left Tail Lamp Jumper (Notchback)

Connector Part Information |

• | KET MG 610152

• | 6-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620153

• | 6-Way M 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 450 | Ground | 1 | BK | 450 | Ground
2 | BK | 450 | Ground | 2 | BK/YE | 450 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage (w/Backup Lamp) | 3 | WH | 24 | Backup Lamp Supply Voltage
RD | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp (RHD) | WH | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp
4 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | 4 | YE | 14 | Left Turn Signal Lamps Supply Voltage
5 | PU | 709 | Left Park Lamp Supply Voltage | 5 | D-BU | 709 | Left Park Lamp Supply Voltage
6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C416 Body Harness to Left Tail Lamp Jumper (Hatchback)

Connector Part Information |

• | KET MG 610152

• | 6-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620153

• | 6-Way M 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 950 | Ground | 1 | BK | 450 | Ground
2 | BK | 950 | Ground | 2 | BK/YE | 450 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage (w/Backup Lamp) | 3 | WH | 24 | Backup Lamp Supply Voltage
RD | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp (RHD) | WH | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | YE | 15 | Right Turn Signal Lamps Supply Voltage
5 | BN/WH | 309 | Right Park Lamp Supply Voltage | 5 | D-BU | 709 | Right Park Lamp Supply Voltage
6 | BN | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C416 Rear Harness to Right Tail Lamp Jumper (Notchback)

Connector Part Information |

• | KET MG 610152

• | 6-Way F 090 (2.3 mm) Series (WH)

Connector Part Information

• | KET MG 620153

• | 6-Way M 090 (2.3 mm) Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 450 | Ground | 1 | BK | 450 | Ground
2 | BK | 450 | Ground | 2 | BK/YE | 450 | Ground
3 | L-GN | 24 | Backup Lamp Supply Voltage (w/Backup Lamp) | 3 | WH | 24 | Backup Lamp Supply Voltage
RD | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp (RHD) | WH | 122 | Rear Fog Lamp Supply Voltage w/Rear Fog Lamp
4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | 4 | YE | 15 | Right Turn Signal Lamps Supply Voltage
5 | PU/BK | 309 | Right Park Lamp Supply Voltage | 5 | D-BU | 709 | Right Park Lamp Supply Voltage
6 | YE | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal | 6 | RD | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal

#### C417 Rear Harness to Marker Lamp Jumper (Hatchback/Notchback)

Connector Part Information |

• | KET MG 610320

• | 2-Way F SWP Series (BK)

Connector Part Information

• | KET MG 640322

• | 2-Way M SWP Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PU | 709 | Park Lamp Supply Voltage | 1 | BN | 709 | Park Lamp Supply Voltage
2 | BK | 250 | Ground | 2 | BK | 250 | Ground