For 1990-2009 cars

Table 1: | Automatic Transmission Connector
Table 2: | Input Shaft Speed (ISS) Sensor
Table 3: | Park/Neutral Position (PNP) Switch (1.2L)
Table 4: | Park/Neutral Position (PNP) Switch (1.4L, 1.5L, 1.6L)
Table 5: | Shift Program Switch
Table 6: | Transmission Control Module (TCM) - A
Table 7: | Transmission Control Module (TCM) B
Table 8: | Vehicle Speed Sensor (VSS)

#### Automatic Transmission Connector

Connector Part Information |

• | Yazaki 7283-1407-40

• | 10-Way (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 898 | Transmission Fluid Temperature Sensor Signal
2 | PK | 1224 | Timing Valve Control
3 | RD | 1226 | Pressure Control Solenoid Control
4 | D-BU | 1225 | Torque Converter Clutch Solenoid Control
5 | L-GN | 1222 | Shift Solenoid 1 Valve Control
6 | OG/BK | 586 | Transmission Fluid Temperature Sensor Low Reference
7 | -- | -- | Not Used
8 | YE/BK | 1227 | Low Reference
9 | -- | -- | Not Used
10 | YE/BK | 1223 | Shift Solenoid 2 Valve Control

#### Input Shaft Speed (ISS) Sensor

Connector Part Information |

• | Yazaki 7283-8125-90

• | 2-Way F (BU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE/BK | 1297 | Input Shaft Speed (ISS) Sensor Low Signal
2 | D-BU/WH | 1296 | Input Shaft Speed (ISS) Sensor High Signal

#### Park/Neutral Position (PNP) Switch (1.2L)

Connector Part Information |

• | Yazaki 7283-1909-40

• | 9-Way F (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 323 | Park/Neutral Position (PNP) Switch Signal
2 | GY | 2380 | Park/Neutral Position (PNP) Switch Low Gear Signal
3 | WH | 2377 | Park/Neutral Position (PNP) Switch Drive Signal
4 | BK | 51 | Ground
5 | YE | 2381 | Park/Neutral Position (PNP) Switch Neutral Signal
6 | PK | 2384 | Park/Neutral Position (PNP) Switch 2nd Gear Signal
7 | PK | 839 | Ignition 1 Voltage
8 | D-GN/WH | 2383 | Park/Neutral Position (PNP) Switch Reverse Signal
9 | D-GN/YE | 2382 | Park/Neutral Position (PNP) Switch Park Signal

#### Park/Neutral Position (PNP) Switch (1.4L, 1.5L, 1.6L)

Connector Part Information |

• | Yazaki 7283-1909-40

• | 9-Way F (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/YE | 2382 | Park/Neutral Position (PNP) Switch Park Signal
2 | D-GN/WH | 2383 | Park/Neutral Position (PNP) Switch Reverse Signal
3 | PK | 839 | Ignition 1 Voltage
4 | PK | 2384 | Park/Neutral Position (PNP) Switch 2nd Gear Signal
5 | YE | 2381 | Park/Neutral Position (PNP) Switch Neutral Signal
6 | BK | 51 | Ground
7 | WH | 2377 | Park/Neutral Position (PNP) Switch Drive Signal
8 | GY | 2380 | Park/Neutral Position (PNP) Switch Low Gear Signal
9 | BN | 323 | Park/Neutral Position (PNP) Switch Signal

#### Shift Program Switch

Connector Part Information |

• | KET MG 610366

• | 4-Way F PCB 040 Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | 1135 | Transmission Hold Signal
2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | BK | 450 | Ground
4 | BK | 450 | Ground

#### Transmission Control Module (TCM) - A

Connector Part Information |

• | AMP 1318756-1

• | 24-Way F 025/090 SER 26POS PLUG ASSY (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK/WH | 51 | Ground
2 | YE/BK | 1227 | Low Reference
3 | -- | -- | Not Used
4 | RD | 1226 | Pressure Control Solenoid Control
5 | D-BU | 1225 | Torque Converter Clutch Solenoid Control
6 | PK | 839 | Ignition 1 Voltage
7 | YE | 710 | CAN Serial Data Low
8-10 | -- | -- | Not Used
11 | PU | 898 | Transmission Fluid Temperature Sensor Signal
12 | OG/BK | 586 | Transmission Fluid Temperature Sensor Low Reference
13 | -- | -- | Not Used
14 | PK | 1224 | Timing Valve Control
15 | YE/BK | 1223 | Shift Solenoid 2 Valve Control
16 | L-GN | 1222 | Shift Solenoid 1 Valve Control
17 | PU | 1807 | CAN Serial Data High
18-22 | -- | -- | Not Used
23 | BK/WH | 51 | Ground
24 | OG | 440 | Battery Positive Voltage

#### Transmission Control Module (TCM) B

Connector Part Information |

• | AMP 1318757-1

• | 26-Way F 025/090 SER 24POS PLUG ASSY (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | 2383 | Park/Neutral Position (PNP) Switch Reverse Signal
L-GN | 24 | Back-Up Lamps Supply Voltage
2 | -- | -- | Not Used
3 | YE | 1481 | Hold Motor Indicator Control
4 | D-GN/WH | 1135 | Transmission Hold Signal
5 | -- | -- | Not Used
6 | D-BU/WH | 1296 | Input Shaft Speed (ISS) Sensor High Signal
7 | WH | 2377 | Park/Neutral Position (PNP) Switch Drive Signal
8 | YE | 2381 | Park/Neutral Position (PNP) Switch Neutral Signal
9-15 | -- | -- | Not Used
16 | YE/BK | 1297 | Input Shaft Speed (ISS) Sensor Low Signal
17 | -- | -- | Not Used
18 | GY | 2380 | Park/Neutral Position (PNP) Switch Low Gear Signal
19 | PK | 2384 | Park/Neutral Position (PNP) Switch 2nd Gear Signal
20 | D-GN/YE | 2382 | Park/Neutral Position (PNP) Switch Park Signal
21 | -- | -- | Not Used
22 | L-BU | 20 | Stop Lamp Supply Voltage/Stop Lamp Switch Signal
23 | D-BU | 2051 | Serial Data
24 | -- | -- | Not Used
25 | D-GN/WH | 817 | Vehicle Speed Signal
26 | -- | -- | Not Used

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | Yazaki 7283-1232

• | 3-Way F (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 839 | Ignition 1 Voltage
2 | BK/WH | 51 | Ground
3 | D-GN/WH | 817 | Vehicle Speed Signal