For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fuel Filler Door Screws | 2 N·m | 18 lb in
Gas Support Assembly Studs | 8 N·m | 71 lb in
Hatchback Door Hinge Bolts | 20 N·m | 15 lb ft
Hatchback Door Lock Screws | 6 N·m | 53 lb in
Hatchback Door Lock Striker Screws | 20 N·m | 15 lb ft
Luggage Compartment Lock Cylinder Nuts | 3 N·m | 27 lb in
Luggage Compartment Lock Screws | 6 N·m | 53 lb in
Luggage Compartment Lock Striker Bolts | 8 N·m | 71 lb in
Rear Deck Lid Bolts | 10 N·m | 89 lb in
Remote Cable Handle Bolt | 8 N·m | 71 lb in