For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Child Seat Anchor | 25 N·m | 18 lb ft
Front Bucket Seat Bolts | 25 N·m | 18 lb ft
Front Seat Back Bolts | 25 N·m | 18 lb ft
Front Seat Belt Buckle Bolt | 38 N·m | 28 lb ft
Front Seat Cover Screw | 12 N·m | 106 lb in
Front Seat Cushion Bolts | 25 N·m | 18 lb ft
Front Seat Recliner Knob Screw (Lever Type) | 12 N·m | 106 lb in
Lock Assembly Screws | 20 N·m | 15 lb ft
Lock Striker Bolts | 24 N·m | 18 lb ft
Lower Rear Seat Belt Anchor Bolt | 38 N·m | 28 lb ft
Rear Seat Back Bolts | 25 N·m | 18 lb ft
Rear Seat Bolts | 25 N·m | 18 lb ft
Rear Seat Cushion Bolt | 25 N·m | 18 lb ft