For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Child Seat Tether Anchor Bolt (Except 4-Door North America Vehicles) | 25 N·m | 18 lb ft
Child Seat Tether Anchor Bolt (4-Door North America Vehicles) | 38 N·m | 28 lb ft
Seat Belt Anchor Bolt | 38 N·m | 28 lb ft
Seat Belt Buckle Bolt | 38 N·m | 28 lb ft
Seat Belt Height Adjuster Bolts | 27 N·m | 20 lb ft
Seat Belt Retractor Bolt | 38 N·m | 28 lb ft