For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
CHMSL Mounting Screws | 3 N·m | 27 lb in
Cupholder Screws | 2 N·m | 18 lb in
Daytime Running Lamp Module Screws | 2.5 N·m | 22 lb in
Door Jamb Switch Screw | 4.5 N·m | 40 lb in
Headlamp Assembly Bolts | 6 N·m | 53 lb in
Interior Courtesy Lamp Housing Screws | 2 N·m | 18 lb in
License Plate Lamp Screws | 1.5 N·m | 13 lb in
Tail Lamp Assembly Screws | 3 N·m | 27 lb in