For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Automatic Transaxle - 1.2 L and 1.4/1.5 L SOHC | 5.6 liters | 5.9 quarts
Automatic Transaxle - 1.4 L/1.6 L DOHC | 5.8 liters | 6.2 quarts
Automatic Transaxle Shift Linkage | As Required
Brake Fluid and Clutch Fluid | 0.5 liters | 0.5 quarts
Clutch Linkage Pivot Points | As Required
Engine Oil - 1.4/1.5 L SOHC and 1.4/1.6 L DOHC | 3.75 liters | 4 quarts
Engine Oil - 1.2 L SOHC | 3.2 liters | 3.4 quarts
Engine Coolant - 1.4/1.5 L SOHC and 1.4 DOHC | 6.0 liters | 6.3 quarts
Engine Coolant - 1.2 L SOHC | 4.2 liters | 4.4 quarts
Engine Coolant - 1.6 L DOHC | 6.0 liters | 6.3 quarts
Floor Shift Linkage Points | As Required
Hood Latch Assembly, Pivots and Spring Anchor, Release Pawl | As Required
Hood and Door Hinges, Fuel Door Hinge, Rear Compartment Lid Hinges | As Required
Key Lock Cylinders | As Required
Manual Transaxle - 1.4/1.5 L SOHC and 1.4 L/1.6 L DOHC | 1.8 liters | 2 quarts
Manual Transaxle - 1.2 L SOHC | 2.1 liters | 2.2 quarts
Manual Transaxle Shift Linkage | As Required
Power Steering System | 1.1 liters | 1.2 quarts
Weatherstrips | As Required