For 1990-2009 cars

## Antilock Brake System Connector End Views Notchback

Table 1: | Electronic Brake Control Module (EBCM)
Table 2: | Lamp Driver Module
Table 3: | Oil Feed Connector
Table 4: | Wheel Speed Sensor - Left Front
Table 5: | Wheel Speed Sensor - Left Rear
Table 6: | Wheel Speed Sensor - Right Front
Table 7: | Wheel Speed Sensor - Right Rear

#### Electronic Brake Control Module (EBCM)

Connector Part Information |

• | 368482-1

• | 25-Way F Plug Assembly for ABS (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 872 | Right Front Wheel Speed Sensor Low Reference
2 | BN | 833 | Right Front Wheel Speed Sensor
3 | BN | 834 | Rough Road Signal
4 | PK | 639 | Ignition 1 Voltage
5 | BN | 884 | Left Rear Wheel Speed Signal
6 | OG | 885 | Left Rear Wheel Speed Sensor Return
7 | BK/WH | 2051 | Ground
8 | BK | 50 | Ground
9 | RD | 42 | Battery Positive Voltage
10-15 | -- | -- | Not Used
16 | L-GN/BK | 875 | Base Brake Failure Signal
17 | -- | -- | Not Used
18 | L-BU | 20 | Stop Lamp Supply Voltage
19 | L-BU | 830 | Left Front Wheel Speed Sensor Signal
20 | YE | 873 | Left Front Wheel Speed Sensor Return
21 | -- | -- | Not Used
22 | WH | 883 | Right Rear Wheel Speed Sensor Return
23 | BN | 882 | Right Rear Wheel Speed Sensor Signal
24 | BK | 50 | Ground
25 | RD | 42 | Battery Positive Voltage

#### Lamp Driver Module

Connector Part Information |

• | AK 368530-1

• | 6-Way F Econoseal J-Mark II (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | RD | 242 | Battery Positive Voltage
3 | BN | 33 | Brake Warning Indicator Control
4 | -- | -- | Not Used
5 | GY | 875 | Base Brake Failure Signal
6 | L-GN | 867 | ABS Failure Indicator Signal

#### Oil Feed Connector

Connector Part Information |

• | MG640329-5

• | 3-Way F (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 50 | Ground
2 | BK/WH | 242 | DLC Signal
3 | BK | 33 | Ignition + Voltage

#### Wheel Speed Sensor - Left Front

Connector Part Information |

• | 174354-2

• | 2-Way M Econoseal J-Mark II + Connector Cap Hsg (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 830 | Left Front Wheel Speed Sensor Signal
2 | YE | 873 | Left Front Wheel Speed Sensor Return

#### Wheel Speed Sensor - Left Rear

Connector Part Information |

• | 174354-2

• | 2-Way M Econoseal J-Mark II + Connector Cap Hsg (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 884 | Left Rear Wheel Speed Sensor Signal
2 | OG | 885 | Left Rear Wheel Speed Sensor Return

#### Wheel Speed Sensor - Right Front

Connector Part Information |

• | 174354-2

• | 2-Way M Econoseal J-Mark II + Connector Cap Hsg (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 872 | Right Front Wheel Speed Sensor Return
2 | D-GN | 833 | Right Front Wheel Speed Sensor Signal

#### Wheel Speed Sensor - Right Rear

Connector Part Information |

• | 174354-2

• | 2-Way M Econoseal J-Mark II + Connector Cap Hsg (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 882 | Right Rear Wheel Speed Sensor Signal
2 | WH | 883 | Right Rear Wheel Speed Sensor Return

## Antilock Brake System Connector End Views Hatchback

Table 1: | Electronic Brake Control Module (EBCM)
Table 2: | Lamp Driver Module
Table 3: | Wheel Speed Sensor - Left Front
Table 4: | Wheel Speed Sensor - Left Rear
Table 5: | Wheel Speed Sensor - Right Front
Table 6: | Wheel Speed Sensor - Right Rear

#### Electronic Brake Control Module (EBCM)

Connector Part Information |

• | AMP 368482-1

• | 25-Way PLUG ASSY FOR 25P ABS (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 872 | Right Front Wheel Speed Sensor Low Reference
2 | WH | 833 | Right Front Wheel Speed Sensor
3 | WH | 834 | Rough Road Signal
4 | PK | 639 | Ignition 1 Voltage
5 | D-GN/WH | 884 | Left Rear Wheel Speed Signal
6 | BN/BK | 885 | Left Rear Wheel Speed Sensor Return
7 | BK/WH | 2051 | Ground
8 | BK | 50 | Ground
9 | RD | 42 | Battery Positive Voltage
10-15 | -- | -- | Not Used
16 | GY | 875 | Base Brake Failure Signal
17 | -- | -- | Not Used
18 | BN | 20 | Stop Lamp Supply Voltage
19 | D-BU | 830 | Left Front Wheel Speed Sensor Signal
20 | L-GN | 873 | Left Front Wheel Speed Sensor Return
21 | -- | -- | Not Used
22 | PU | 883 | Right Rear Wheel Speed Sensor Return
23 | L-BU | 882 | Right Rear Wheel Speed Sensor Signal
24 | BK | 50 | Ground
25 | RD | 42 | Battery Positive Voltage

#### Lamp Driver Module

Connector Part Information |

• | AK 368530-1

• | 6-Way F Econoseal J-Mark II + 6P (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | RD | 242 | Battery Positive Voltage
3 | BN | 33 | Brake Warning Indicator Control
4 | -- | -- | Not Used
5 | GY | 875 | Base Brake Failure Signal
6 | L-GN | 867 | ABS Failure Indicator Signal

#### Wheel Speed Sensor - Left Front

Connector Part Information |

• | AMP 174354-2

• | 2-Way M Econoseal J-Mark II+ Connector Cap Hsg (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 830 | Left Front Wheel Speed Sensor Signal
2 | L-GN | 873 | Left Front Wheel Speed Sensor Return

#### Wheel Speed Sensor - Left Rear

Connector Part Information |

• | AMP 174354-2

• | 2-Way M Econoseal J-Mark II+ Connector Cap Hsg (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 884 | Left Rear Wheel Speed Sensor Signal
2 | BN/BK | 885 | Left Rear Wheel Speed Sensor Return

#### Wheel Speed Sensor - Right Front

Connector Part Information |

• | AMP 174354-2

• | 2-Way M Econoseal J-Mark II+ Connector Cap Hsg (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 833 | Right Front Wheel Speed Sensor Return
2 | BN | 872 | Right Front Wheel Speed Sensor Signal

#### Wheel Speed Sensor - Right Rear

Connector Part Information |

• | AMP 174354-2

• | 2-Way M Econoseal J-Mark II+ Connector Cap Hsg (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 882 | Right Rear Wheel Speed Sensor Signal
2 | PU | 883 | Right Rear Wheel Speed Sensor Return