For 1990-2009 cars

#### Performance - Manual Transaxle

Application | Specification
--- | ---
Metric | English
Final Drive Ratio (1.4L SOHC) | 4.176:1
Final Drive Ratio (1.4L DOHC) | 3.944:1
Final Drive Ratio (1.5L) | 3.722:1
Gradeability | 0.47 | (tan O)
1st Gear Ratio | 3.545:1
2nd Gear Ratio | 1.952:1
3rd Gear Ratio | 1.276:1
4th Gear Ratio (1.4L DOHC/1.5L) | 0.971:1
4th Gear Ratio (1.4L SOHC) | 0.892:1
5th Gear Ratio (1.4L DOHC/1.5L) | 0.763:1
5th Gear Ratio (1.4L SOHC) | 0.707:1
Reverse Gear Ratio | 3.333:1
Maker | DWMC
Maximum Speed | 170 km/H | (105.6 mph)
Minimum Turning Radius | 4.8 m | (15.7 ft)
Oil Capacity | 1.8 liters | 2 quarts
Transaxle Type and Model | D-16