For 1990-2009 cars

## Heated/Cooled Seat Connector End Views C100/Long Body

Connector 1: | Power Seat Switch
Connector 2: | Heated Seat Switch - Left
Connector 3: | Heated Seat Switch - Right
Connector 4: | Heated Seat - Left
Connector 5: | Heated Seat - Right

### Power Seat Switch

#### Connector Part Information

- OEM: MG 610267
- Service: N/A
- Description: 4-Way F 250 Unsealed

#### Power Seat Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | -- | Heated Seat Switch Signal
2 | RD/WH | -- | Battery Positive Voltage
3 | BK | -- | Ground
4 | BK | -- | Ground

### Heated Seat Switch - Left

#### Connector Part Information

- OEM: PED 15499928
- Service: N/A
- Description: 6-Way F 064 Unsealed

#### Heated Seat Switch - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | -- | Backlight Lamp Control
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | L-BU | -- | Signal
5 | BN | -- | Ignition 3 Voltage
6 | BK | -- | Ground

### Heated Seat Switch - Right

#### Connector Part Information

- OEM: PED 15499928
- Service: N/A
- Description: 6-Way F 064 Unsealed

#### Heated Seat Switch - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | -- | Backlight Lamp Control
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | L-BU/BK | -- | Signal
5 | BN | -- | Ignition 3 Voltage
6 | BK | -- | Ground

### Heated Seat - Left

#### Connector Part Information

- OEM: MG 610207
- Service: N/A
- Description: 2-Way F Unsealed

#### Heated Seat - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Heated Seat Switch Signal
2 | BK | -- | Ground

### Heated Seat - Right

#### Connector Part Information

- OEM: MG 610207
- Service: N/A
- Description: 2-Way F Unsealed

#### Heated Seat - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Heated Seat Switch Signal
2 | BK | -- | Ground

## Heated/Cooled Seat Connector End Views C105/Short Body

Connector 1: | Heated Seat Switch - Left
Connector 2: | Heated Seat Switch - Right

### Heated Seat Switch - Left

#### Connector Part Information

- OEM: PED 15406141
- Service: N/A
- Description: 8-Way F 064 Unsealed

#### Heated Seat Switch - Left

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | -- | Backlight Lamp Control
2 | BK | -- | Ground
3 | BN | -- | Ignition 3 Voltage
4 | BU | -- | Left Heated Seat Back Switch Signal
5 | PU/WH | -- | LED Dimming Signal
6 | L-BU | -- | Left Heated Seat Low Indicator
7 | WH/BK | -- | Left Heated Seat Medium Indicator
8 | GN | -- | Left Heated Seat High Indicator

### Heated Seat Switch - Right

#### Connector Part Information

- OEM: PED 15406141
- Service: N/A
- Description: 8-Way F 064 Unsealed

#### Heated Seat Switch - Right

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | -- | Backlight Lamp Control
2 | BK | -- | Ground
3 | BN | -- | Ignition 3 Voltage
4 | PU | -- | Right Heated Seat Back Switch Signal
5 | PU/WH | -- | Led Dimming Signal
6 | YE | -- | Right Heated Seat High Indicator
7 | WH/BK | -- | Right Heated Seat Medium Indicator
8 | BN | -- | Right Heated Seat Low Indicator