For 1990-2009 cars

Important:

• | To initiate, this procedures requires that a learned master key be available.

• | A total of 10 master keys or valet keys may be programmed to a single vehicle.

• | This procedure adds keys only. The procedure does not erase previously learned keys.

• | The keys to be learned must duplicate the mechanical cut of the current key.

• | If more than one valet key is to be learned, immediately precede each valet key with a learned master key.

1. With a previously learned master key, turn ON the ignition, with the engine OFF.
2. Turn OFF the ignition and remove the key.
3. Within 4 seconds insert the key to be learned.

Turn ON the ignition with the engine OFF. The vehicle has now learned the new key.