For 1990-2009 cars

#### Harsh Feel During Acceleration or Deceleration

Condition | Action
--- | ---
DEFINITION: Harsh feel without causing an upshift or downshift. Concern is most noticeable with light acceleration or deceleration.
Engine and or Transaxle mounts | Inspect the engine and or transaxle for loose, damaged or missing mounts. Repair as necessary.
Base Engine | Inspect the engine for any base level concerns. Repair as necessary.
Drive Axles | Inspect both drive axles for proper installation and/or damage. Repair as necessary.