For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Turn ON the ignition, with the engine OFF.
2. Observe the security indicator.

Does the security indicator come ON for approximately 5 seconds and then turn OFF?

--

Go to Testing for Intermittent Conditions and Poor Connections

Go to Step 3

3 | Inspect for poor connections at the clock. Did you find and correct the condition? | -- | Go to Step 5 | Go to Step 4
4 | Replace the clock. Did you complete the replacement? | -- | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2