For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B1101 | Battery Voltage High | SDM | DTC B1101
B1102 | Battery Voltage Low | SDM | DTC B1102
B1103 | SIR Serial Communications Fault | SDM | DTC B1103
B1346 | Driver Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1346
B1347 | Driver Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1347
B1348 | Driver Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1348
B1349 | Driver Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1349
B1352 | Passenger Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1352
B1353 | Passenger Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1353
B1354 | Passenger Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1354
B1355 | Passenger Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1355
B1361 | Driver Pretensioner Deployment Loop Resistance High | SDM | DTC B1361
B1362 | Driver Pretensioner Deployment Loop Resistance Low | SDM | DTC B1362
B1363 | Driver Pretensioner Deployment Loop Short to Ground | SDM | DTC B1363
B1364 | Driver Pretensioner Deployment Loop Short to Battery | SDM | DTC B1364
B1367 | Passenger Pretensioner Deployment Loop Resistance High | SDM | DTC B1367
B1368 | Passenger Pretensioner Deployment Loop Resistance Low | SDM | DTC B1368
B1369 | Passenger Pretensioner Deployment Loop Short to Ground | SDM | DTC B1369
B1370 | Passenger Pretensioner Deployment Loop Short to Battery | SDM | DTC B1370
B1378 | LF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1378
B1379 | LF Side Deployment Loop Resistance Low | SDM | DTC B1379
B1380 | LF Side Deployment Loop Short To Ground | SDM | DTC B1380
B1381 | LF Side Deployment Loop Short to Battery | SDM | DTC B1381
B1382 | RF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1382
B1383 | RF Side Deployment Loop Resistance Low | SDM | DTC B1383
B1384 | RF Side Deployment Loop Short to Ground | SDM | DTC B1384
B1385 | RF Side Deployment Loop Short to Battery | SDM | DTC B1385
B1395 | Deployment Loops Interconnect Circuit | SDM | DTC B1395
B1400 | Driver SIS Malfunction | SDM | DTC B1400
B1401 | LF Side Impact Sensor Short to Ground | SDM | DTC B1401
B1402 | LF Side Impact Sensor Short to Battery | SDM | DTC B1402
B1403 | Passenger SIS Malfunction | SDM | DTC B1403
B1404 | RF Side Impact Sensor Short to Ground | SDM | DTC B1404
B1405 | RF Side Impact Sensor Short to Battery | SDM | DTC B1405
B1406 | PPD/SBR Malfunction | SDM | DTC B1406
B1407 | PPD/SBR Communication Error | SDM | DTC B1407
B1409 | LF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1409
B1410 | RF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1410
B1414 | LF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1414
B1415 | RF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1415
B1453 | Vehicle Speed Signal | SDM | DTC B1453
B1473 | Left Roof Rail Deployment Loop Resistance Above Threshold | SDM | DTC B1473
B1474 | Left Roof Rail Deployment Loop Resistance Low | SDM | DTC B1474
B1475 | Left Roof Rail Deployment Loop Short to Ground | SDM | DTC B1475
B1476 | Left Roof Rail Deployment Loop Short to Battery | SDM | DTC B1476
B1477 | Right Roof Rail Deployment Loop Resistance Above Threshold | SDM | DTC B1477
B1478 | Right Roof Rail Deployment Loop Resistance Low | SDM | DTC B1478
B1479 | Right Roof Rail Deployment Loop Short to Ground | SDM | DTC B1479
B1480 | Right Roof Rail Deployment Loop Short to Battery | SDM | DTC B1480
B1620 | ECU Performance | SDM | DTC B1620
B1650 | Frontal Stage 1 Deployment Commanded | SDM | DTC B1650
B1651 | LH Side Air Bag Deployment Commanded | SDM | DTC B1651
B1652 | RH Side Air Bag Deployment Commanded | SDM | DTC B1652
B1657 | Deployment Commanded Pretensioner | SDM | DTC B1657
B2500 | Inflatable Restraint System Indicator Circuit | SDM | DTC B2500
B2502 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2502
C1101 | Battery Voltage High | EBCM | DTC C1101
C1102 | Battery Voltage Low | EBCM | DTC C1102
C1200 | Left Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1200
C1201 | Left Front Wheel Speed Circuit Range Performance | EBCM | DTC C1201
C1202 | Left Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1202
C1203 | Right Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1203
C1204 | Right Front Wheel Speed Circuit Range Performance | EBCM | DTC C1204
C1205 | Right Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1205
C1206 | Left Rear Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1206
C1207 | Left Rear Wheel Speed Sensor Circuit Range Performance | EBCM | DTC C1207
C1208 | Left Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1208
C1209 | Right Rear Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1209
C1210 | ECU Malfunction | EBCM | DTC C1210
C1211 | Right Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1211
C1503 | Traction Control Switch Circuit | EBCM | DTC C1503
C1604 | ECU Malfunction | EBCM | DTC C1604
C1605 | CAN Bus Error | EBCM | DTC C1605, C1611, C1612, or C1616
C1611 | CAN Bus Error | EBCM | DTC C1605, C1611, C1612, or C1616
C1612 | CAN Bus Error | EBCM | DTC C1605, C1611, C1612, or C1616
C1616 | CAN Bus OFF Failure | EBCM | DTC C1605, C1611, C1612, or C1616
C2112 | Solenoid Valve Relay Circuit | EBCM | DTC C2112 or C2380
C2380 | Solenoid Valve Circuit | EBCM | DTC C2112 or C2380
C2402 | Pump Motor Circuit | EBCM | DTC C2402
P0218 | Transmission Fluid Overtemperature | TCM |
P0562 | System Voltage Low | TCM |
P0563 | System Voltage High | TCM |
P0601 | TCM Memory - ROM | TCM |
P0603 | Transmission Control Module (TCM) Long Term Memory Reset | TCM |
P0604 | Control Module Random Access Memory (RAM) | TCM |
P0606 | Control Module Internal Performance | TCM |
P0703 | Brake Switch Circuit | TCM |
P0705 | Transmission Range Sensor Circuit | TCM |
P0706 | Transmission Range Switch Performance | TCM |
P0710 | -- | TCM |
P0711 | -- | TCM |
P0715 | -- | TCM |
P0716 | Input Speed Sensor Performance | TCM |
P0717 | Input Speed Sensor - No Signal | TCM |
P0720 | -- | TCM |
P0721 | Output Speed Sensor Performance | TCM |
P0722 | Output Speed Sensor Circuit No Signal | TCM |
P0725 | -- | TCM |
P0726 | Engine Speed Input Circuit Performance | TCM |
P0727 | Engine Speed Signal Circuit | TCM |
P0731 | -- | TCM |
P0732 | -- | TCM |
P0733 | -- | TCM |
P0734 | -- | TCM |
P0741 | TCC Stuck Off | TCM |
P0742 | TCC Stuck On | TCM |
P0781 | -- | TCM |
P0782 | -- | TCM |
P0783 | -- | TCM |
P1604 | -- | TCM |
P1606 | -- | TCM |
P1671 | Lost Communications With Transmission Control Module (TCM) | TCM |
P1672 | Controller Area Network (CAN) Bus Communication | TCM |
P1673 | High Speed CAN Communication Bus | TCM |
P1779 | -- | TCM |
P1780 | Engine Torque Reduction Signal Circuit | TCM |
P1791 | Throttle Position (TP) Sensor Circuit | TCM |
P1839 | EDS3 Output Shortage to Ground | TCM |
P1840 | EDS3 Output Shortage to Battery | TCM |
P1841 | EDS3 Output Open | TCM |
P1850 | Solenoid 1 Output Shortage To Ground | TCM |
P1851 | Solenoid 1 Output Shortage To Battery | TCM |
P1852 | Solenoid 1 Output Open | TCM |
P1853 | Solenoid 2 Output Shortage To Ground | TCM |
P1854 | Solenoid 2 Output Shortage To Battery | TCM |
P1855 | Solenoid 2 Output Open | TCM |
P1861 | EDS4 Output Shortage to Ground | TCM |
P1862 | EDS4 Output Shortage to Battery | TCM |
P1863 | EDS4 Output Open | TCM |
P1864 | EDS5 Output Shortage to Ground | TCM |
P1865 | EDS5 Output Shortage to Battery | TCM |
P1866 | EDS5 Output Open | TCM |
P1867 | EDS6 Output Shortage to Ground | TCM |
P1868 | EDS6 Output Shortage to Battery | TCM |
P1869 | EDS6 Output Open | TCM |
P1870 | -- | TCM |
P1871 | -- | TCM |
P1873 | Solenoid Valve Power Supply Circuit Shortage To Ground | TCM |
P1874 | Solenoid Valve Power Supply Circuit Shortage To Battery | TCM |
P1881 | -- | TCM |
P1883 | -- | TCM |
P1884 | -- | TCM |
P1885 | -- | TCM |
P1886 | -- | TCM |

### 2.0L Engine

DTC | Diagnostic Procedure | Modules
--- | --- | ---
012 | DTC 012 | ECM
013 | DTC 013, 044, or 045 | ECM
014 | DTC 014 or 015 | ECM
015 | DTC 014 or 015 | ECM
016 | DTC 016 or 018 | ECM
017 | DTC 017 | ECM
018 | DTC 016 or 018 | ECM
019 | DTC 019 | ECM
021 | DTC 021 or 022 | ECM
022 | DTC 021 or 022 | ECM
023 | DTC 023 or 025 | ECM
024 | DTC 024 | ECM
025 | DTC 023 or 025 | ECM
029 | DTC 029 or 032 | ECM
032 | DTC 029 or 032 | ECM
033 | DTC 033 or 034 | ECM
034 | DTC 033 or 034 | ECM
035 | DTC 035 | ECM
041 | DTC 041, 042, 063, or 064 | ECM
042 | DTC 041, 042, 063, or 064 | ECM
044 | DTC 013, 044, or 045 | ECM
045 | DTC 013, 044, or 045 | ECM
049 | DTC 049 | ECM
051 | DTC 051 or 055 | ECM
055 | DTC 051 or 055 | ECM
061 | DTC 061 or 062 | ECM
062 | DTC 061 or 062 | ECM
063 | DTC 041, 042, 063, or 064 | ECM
064 | DTC 041, 042, 063, or 064 | ECM
P0106 | DTC P0106 | ECM
P0107 | DTC P0107 or P0108 | ECM
P0108 | DTC P0107 or P0108 | ECM
P0112 | DTC P0112 or P0113 | ECM
P0113 | DTC P0112 or P0113 | ECM
P0117 | DTC P0117 or P0118 | ECM
P0118 | DTC P0117 or P0118 | ECM
P0122 | DTC P0122 or P0123 | ECM
P0123 | DTC P0122 or P0123 | ECM
P0131 | DTC P0131 or P0132 | ECM
P0132 | DTC P0131 or P0132 | ECM
P0133 | DTC P0133, P1133, or P1134 | ECM
P0134 | DTC P0134 or P0140 | ECM
P0135 | DTC P0135 or P0141 | ECM
P0137 | DTC P0137 or P0138 | ECM
P0138 | DTC P0137 or P0138 | ECM
P0140 | DTC P0134 or P0140 | ECM
P0141 | DTC P0135 or P0141 | ECM
P0171 | DTC P0171 or P0172 | ECM
P0172 | DTC P0171 or P0172 | ECM
P0201 | DTC P0201-P0204 | ECM
P0202 | DTC P0201-P0204 | ECM
P0203 | DTC P0201-P0204 | ECM
P0204 | DTC P0201-P0204 | ECM
P0300 | DTC P0300 | ECM
P0313 | DTC P0313 | ECM
P0317 | DTC P0317 | ECM
P0325 | DTC P0325 | ECM
P0327 | DTC P0327 | ECM
P0335 | DTC P0335, P0336, or P0337 | ECM
P0336 | DTC P0335, P0336, or P0337 | ECM
P0337 | DTC P0335, P0336, or P0337 | ECM
P0341 | DTC P0341 or P0342 | ECM
P0342 | DTC P0341 or P0342 | ECM
P0351 | DTC P0351 or P0352 | ECM
P0352 | DTC P0351 or P0352 | ECM
P0400 | DTC P0400, P0401, P0402, or P1402 | ECM
P0401 | DTC P0400, P0401, P0402, or P1402 | ECM
P0402 | DTC P0400, P0401, P0402, or P1402 | ECM
P0404 | DTC P0404, P0405, P0406, or P1404 | ECM
P0405 | DTC P0404, P0405, P0406, or P1404 | ECM
P0406 | DTC P0404, P0405, P0406, or P1404 | ECM
P0420 | DTC P0420 | ECM
P0443 | DTC P0443 | ECM
P0461 | DTC P0461 | ECM, IPC
P0462 | DTC P0462 | ECM, IPC
P0463 | DTC P0463 | ECM, IPC
P0502 | DTC P0502 | ECM, TCM
P0506 | DTC P0506 or P0507 | ECM
P0507 | DTC P0506 or P0507 | ECM
P0532 | DTC P0532 or P0533 for the manual system or DTC P0532 for the automatic system | ECM
P0533 | DTC P0532 or P0533 for the manual system or DTC P0533 for the automatic system | ECM
P0600 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P0601 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P0602 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P0603 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P0604 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P0605 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P0606 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P0607 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P0646 | DTC P0646 or P0647 for the manual system or DTC P0646 for the automatic system | ECM
P0647 | DTC P0646 or P0647 for the manual system or DTC P0647 for the automatic system | ECM
P0700 | DTC P0700 | ECM, TCM
P1106 | DTC P1106 or P1107 | ECM
P1107 | DTC P1106 or P1107 | ECM
P1111 | DTC P1111 or P1112 | ECM
P1112 | DTC P1111 or P1112 | ECM
P1114 | DTC P1114 or P1115 | ECM
P1115 | DTC P1114 or P1115 | ECM
P1121 | DTC P1121 or P1122 | ECM
P1122 | DTC P1121 or P1122 | ECM
P1133 | DTC P0133, P1133, or P1134 | ECM
P1134 | DTC P0133, P1133, or P1134 | ECM
P1167 | DTC P1167 | ECM
P1171 | DTC P1171 | ECM
P1336 | DTC P1336 | ECM
P1380 | DTC P1380 or P1381 | ECM, EBCM
P1381 | DTC P1380 or P1381 | ECM, EBCM
P1391 | DTC P1391, P1392, or P1393 | ECM, EBCM
P1392 | DTC P1391, P1392, or P1393 | ECM, EBCM
P1393 | DTC P1391, P1392, or P1393 | ECM, EBCM
P1404 | DTC P0404, P0405, P0406, or P1404 | ECM
P1601 | DTC P1601 | ECM, TCM
P1607 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P1650 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM
P1655 | DTC P0600-P0607, P1607, P1650, P1655, or P2610 | ECM

### 2.5L Engine

DTC | Diagnostic Procedure | Module(s)
--- | --- | ---
P0030 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0031 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0032 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0036 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0037 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0038 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0050 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0051 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0052 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0056 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0057 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0058 | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058 | ECM
P0101 | DTC P0101, P0102, or P0103 | ECM
P0102 | DTC P0101, P0102, or P0103 | ECM
P0103 | DTC P0101, P0102, or P0103 | ECM
P0106 | DTC P0106 | ECM
P0107 | DTC P0107 or P0108 | ECM
P0108 | DTC P0107 or P0108 | ECM
P0111 | DTC P0111 | ECM
P0112 | DTC P0112 or P0113 | ECM
P0113 | DTC P0112 or P0113 | ECM
P0116 | DTC P0116 | ECM
P0117 | DTC P0117 or P0118 | ECM
P0118 | DTC P0117 or P0118 | ECM
P0119 | DTC P0119 | ECM
P0121 | DTC P0121, P0122, P0123, P0222, or P0223 | ECM
P0122 | DTC P0121, P0122, P0123, P0222, or P0223 | ECM
P0123 | DTC P0121, P0122, P0123, P0222, or P0223 | ECM
P0125 | DTC P0125 or P0128 | ECM
P0128 | DTC P0125 or P0128 | ECM
P0131 | DTC P0131 or P0151 | ECM
P0132 | DTC P0132 or P0152 | ECM
P0133 | DTC P0133 or P0153 | ECM
P0134 | DTC P0134 or P0154 | ECM
P0136 | DTC P0136 or P0156 | ECM
P0137 | DTC P0137 or P0157 | ECM
P0138 | DTC P0138 or P0158 | ECM
P0139 | DTC P0139 or P0159 | ECM
P0140 | DTC P0140 or P0160 | ECM
P0151 | DTC P0131 or P0151 | ECM
P0152 | DTC P0132 or P0152 | ECM
P0153 | DTC P0133 or P0153 | ECM
P0154 | DTC P0134 or P0154 | ECM
P0157 | DTC P0137 or P0157 | ECM
P0158 | DTC P0138 or P0158 | ECM
P0159 | DTC P0139 or P0159 | ECM
P0160 | DTC P0140 or P0160 | ECM
P0171 | DTC P0171, P0172, P0174, or P0175 | ECM
P0172 | DTC P0171, P0172, P0174, or P0175 | ECM
P0174 | DTC P0171, P0172, P0174, or P0175 | ECM
P0175 | DTC P0171, P0172, P0174, or P0175 | ECM
P0221 | DTC P0121, P0122, P0123, P0221, P0222, or P0223 | ECM
P0222 | DTC P0121, P0122, P0123, P0222, or P0223 | ECM
P0223 | DTC P0121, P0122, P0123, P0222, or P0223 | ECM
P0230 | DTCP0230 or P1231 | ECM
P0261 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0262 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0264 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0265 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0267 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0268 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0270 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0271 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0273 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0274 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0276 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0277 | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, or P0277 | ECM
P0300 | DTC P0300, P0301, P0302, P0303, P0304, P0305, or P0306 | ECM
P0301 | DTC P0300, P0301, P0302, P0303, P0304, P0305, or P0306 | ECM
P0302 | DTC P0300, P0301, P0302, P0303, P0304, P0305, or P0306 | ECM
P0303 | DTC P0300, P0301, P0302, P0303, P0304, P0305, or P0306 | ECM
P0304 | DTC P0300, P0301, P0302, P0303, P0304, P0305, or P0306 | ECM
P0305 | DTC P0300, P0301, P0302, P0303, P0304, P0305, or P0306 | ECM
P0306 | DTC P0300, P0301, P0302, P0303, P0304, P0305, or P0306 | ECM
P0317 | DTC P0317 | ECM
P0324 | DTC P0324 | ECM
P0329 | DTC P0329 or P0334 | ECM
P0334 | DTC P0329 or P0334 | ECM
P0335 | DTC P0335, P0336, or P0337 | ECM
P0336 | DTC P0335, P0336, or P0337 | ECM
P0337 | DTC P0335, P0336, or P0337 | ECM
P0340 | DTC P0340, P0341 or P0342 | ECM
P0341 | DTC P0340, P0341 or P0342 | ECM
P0342 | DTC P0340, P0341 or P0342 | ECM
P0351 | DTC P0351-P0356 | ECM
P0352 | DTC P0351-P0356 | ECM
P0353 | DTC P0351-P0356 | ECM
P0354 | DTC P0351-P0356 | ECM
P0355 | DTC P0351-P0356 | ECM
P0356 | DTC P0351-P0356 | ECM
P0400 | DTC P0400, P0401, or P0402 | ECM
P0401 | DTC P0400, P0401, or P0402 | ECM
P0402 | DTC P0400, P0401, or P0402 | ECM
P0403 | DTC P0403, P0404, P0405, P0406, P1403, or P1404 | ECM
P0404 | DTC P0403, P0404, P0405, P0406, P1403, or P1404 | ECM
P0405 | DTC P0403, P0404, P0405, P0406, P1403, or P1404 | ECM
P0406 | DTC P0403, P0404, P0405, P0406, P1403, or P1404 | ECM
P0420 | DTC P0420 or P0430 | ECM
P0430 | DTC P0420 or P0430 | ECM
P0441 | DTC P0441 | ECM
P0442 | DTC P0442 or P0456 | ECM
P0443 | DTC P0443, P0458, or P0459 | ECM
P0444 | DTC P0444 or P0445 | ECM
P0445 | DTC P0444 or P0445 | ECM
P0446 | DTC P0446 | ECM
P0447 | DTC P0447 or P0448 | ECM
P0448 | DTC P0447 or P0448 | ECM
P0451 | DTC P0451 or P0454 | ECM
P0452 | DTC P0452 or P0453 | ECM
P0453 | DTC P0452 or P0453 | ECM
P0454 | DTC P0451 or P0454 | ECM
P0455 | DTC P0455 or P0457 | ECM
P0456 | DTC P0442 or P0456 | ECM
P0457 | DTC P0455 or P0457 | ECM
P0461 | DTC P0461 | ECM, IPC
P0462 | DTC P0462 | ECM, IPC
P0463 | DTC P0463 | ECM, IPC
P0480 | DTC P0480 or P0481 | ECM
P0481 | DTC P0480 or P0481 | ECM
P0496 | DTC P0496 | ECM
P0498 | DTC P0498 or P0499 | ECM
P0499 | DTC P0498 or P0499 | ECM
P0500 | DTC P0500 | ECM
P0501 | DTC P0501 | ECM, TCM
P0506 | DTC P0506 or P0507 | ECM
P0507 | DTC P0506 or P0507 | ECM
P0510 | DTC P0510 | ECM
P0532 | DTC P0532 or P0533 for the manual system or DTC P0532 for the automatic system | ECM
P0533 | DTC P0532 or P0533 for the manual system or DTC P0533 for the automatic system | ECM
P0601 | DTC P0601-P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 | ECM
P0604 | DTC P0601-P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 | ECM
P0605 | DTC P0601-P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 | ECM
P0638 | DTC P0638, P2111, P2112, or P2119 | ECM
P0642 | DTC P0642, P0643, P0698, or P0699 | ECM
P0643 | DTC P0642, P0643, P0698, or P0699 | ECM
P0646 | DTC P0646 or P0647 for the manual system or DTC P0646 for the automatic system | ECM
P0647 | DTC P0646 or P0647 for the manual system or DTC P0647 for the automatic system | ECM
P0650 | DTC P0650 or P1650 | ECM
P0660 | DTC P0660, P0661, or P0662 | ECM
P0661 | DTC P0660, P0661, or P0662 | ECM
P0662 | DTC P0660, P0661, or P0662 | ECM
P0689 | DTC P0689 or P0690 | ECM
P0690 | DTC P0689 or P0690 | ECM
P0700 | DTC P0700 | ECM, TCM
P1171 | DTC P1171 or P1174 | ECM
P1172 | DTC P1172 or P1175 | ECM
P1174 | DTC P1171 or P1174 | ECM
P1175 | DTC P1172 or P1175 | ECM
P1231 | DTC P1230 or P1231 | ECM
P1319 | DTC P1319 | ECM
P1320 | DTC P1320 | ECM
P1321 | DTC P1321 | ECM
P1382 | DTC P1382 | ECM
P1504 | DTC P1504 | ECM
P1562 | DTC P1562 or P1563 | ECM
P1563 | DTC P1562 or P1563 | ECM
P1610 | DTC P1610 or P1611 | ECM
P1611 | DTC P1610 or P1611 | ECM
P1648 | Theft Deterrent Security Code Incorrect | ECM
P2070 | DTC P2070 or P2071 | ECM
P2071 | DTC P2070 or P2071 | ECM
P2077 | DTC P2077 or P2078 | ECM
P2078 | DTC P2077 or P2078 | ECM
P2096 | DTC P2096 or P2098 | ECM
P2098 | DTC P2096 or P2098 | ECM
P2101 | DTC P2101, P2118, or P2119 | ECM
P2110 | DTC P2110 | ECM
P2111 | DTC P0638, P2111, P2112, or P2119 | ECM
P2118 | DTC P2101, P2118, or P2119 | ECM
P2119 | DTC P2101, P2118, or P2119 | ECM
P2122 | DTC P2122, P2123, P2127, P2128, or P2138 | ECM
P2123 | DTC P2122, P2123, P2127, P2128, or P2138 | ECM
P2127 | DTC P2122, P2123, P2127, P2128, or P2138 | ECM
P2128 | DTC P2122, P2123, P2127, P2128, or P2138 | ECM
P2138 | DTC P2122, P2123, P2127, P2128, or P2138 | ECM
P2159 | DTC P2159 | ECM
P2422 | DTC P2422 | ECM