For 1990-2009 cars

### Removal Procedure

1. Remove the rear transmission mount. Refer to Transmission Rear Mount Replacement .
2. Remove the transmission mount bracket to frame bolts (1).
3. Remove the transmission mount bracket (2).

### Installation Procedure

1. Install the transmission mount bracket (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the transmission bracket to frame bolts (1).

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

3. Install the rear transmission mount. Refer to Transmission Rear Mount Replacement .