For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Automatic Transaxle Fluid - Aisin 55-51LE with a Diesel Engine | 6.94 ± 0.15 L | 7.33 ± 0.15 qt
Automatic Transaxle Fluid - Aisin 55-51LE with a Gasoline Engine | 7.14 ± 0.15 L | 7.5 ± 0.15 qt
Automatic Transaxle Fluid - 6T40/45 with a Diesel Engine | 8.66 ± 0.12 L | 9.15 ± 0.12 qt
Automatic Transaxle Fluid - 6T40/45 with a Gasoline Engine | 8.16 ± 0.12 L | 8.6 ± 0.12 qt
Brake Fluid and Clutch Fluid | 0.5 L | 0.53 qt
Engine Coolant | 8.0 L | 8.4 qt
Engine Oil for a Diesel Engine | 6.2 L | 6.6 qt
Engine Oil for a Gasoline Engine | 6.4 L | 6.7 qt
Manual Transaxle Lubricant with a Diesel Engine | 2.1 L | 2.2 qt
Manual Transaxle Lubricant with a Gasoline Engine | 1.6 L | 1.78 qt
Power Steering System Fluid | 1.1 L | 1.2 qt