For 1990-2009 cars

## Clutch Pedal Hard to Push D33 Manual Transaxle

Checks | Actions
--- | ---
Check for bad lubrication of clutch pedal shaft. | Apply the grease or repair it.
Check for a clogged pipe. | Inspect or replace the clogged pipe.
Check for a stuck concentric slave cylinder. | Replace the concentric slave cylinder. Refer to Clutch Concentric Actuator Cylinder Replacement.

## Clutch Pedal Hard to Push D24 Manual Transaxle

Checks | Actions
--- | ---
Check for binding in the linkage. | Lubricate and free-up the binding linkage.
Check for a worn driven plate. | Replace the worn driven plate.