For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch Fluid Passage Seal
2 | 1-2-3-4 Clutch Fluid Passage Seal
3 | Control Valve Body Spacer Plate Assembly
4 | Control Valve Body Assembly
5 | Control Valve Body Bolt M6 x 60 (Qty: 9) Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten in sequence to 12 N·m (106 lb in).
6 | Control Valve Body Bolt M6 x 53) (Qty: 2) Tighten Tighten in sequence to 12 N·m (106 lb in).
7 | Manual Shaft Detent Lever Spring Assembly
8 | Manual Shaft Detent Spring Bolt M6 x 16 (Qty: 1) Tighten Tighten to 12 N·m (106 lb in).
9 | Fluid Level Control Valve Gasket
10 | Fluid Level Control Valve