For 1990-2009 cars

#### Tools Required

J 21104-B (KM-475-B) Weatherstrip Remover Universal or equivalent

### Removal Procedure

1. Remove the luggage compartment rear panel cover. Refer to Rear Compartment Trim Panel Replacement .
2. Remove the plastic retaining clips using the J 21104-B and reposition the luggage compartment rear trim panel.

### Installation Procedure

1. Install the wheelhouse trim panel with the plastic clips.
2. Install the luggage compartment rear panel cover. Refer to Rear Compartment Trim Panel Replacement .