For 1990-2009 cars

Connector 1: | Accelerator Pedal Position (APP) Sensor
Connector 2: | Camshaft Position (CMP) Sensor
Connector 3: | Clutch Switch
Connector 4: | Crankshaft Position (CKP) Sensor
Connector 5: | Engine Coolant Temperature (ECT) Sensor
Connector 6: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve
Connector 7: | Evaporative Emissions (EVAP) Canister Vent Solenoid Valve
Connector 8: | Exhaust Gas Recirculation (EGR) Valve
Connector 9: | Fuel Injector 1
Connector 10: | Fuel Injector 2
Connector 11: | Fuel Injector 3
Connector 12: | Fuel Injector 4
Connector 13: | Fuel Injector 5
Connector 14: | Fuel Injector 6
Connector 15: | Fuel Pump
Connector 16: | Fuel Tank Pressure (FTP) Sensor
Connector 17: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1
Connector 18: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2
Connector 19: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1
Connector 20: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2
Connector 21: | Ignition Coil Module 1
Connector 22: | Ignition Coil Module 2
Connector 23: | Ignition Coil Module 3
Connector 24: | Ignition Coil Module 4
Connector 25: | Ignition Coil Module 5
Connector 26: | Ignition Coil Module 6
Connector 27: | Intake Air Temperature (IAT) Sensor
Connector 28: | Intake Manifold Tuning Valve Solenoid
Connector 29: | Knock Sensor (KS) 1
Connector 30: | Knock Sensor (KS) 2
Connector 31: | Manifold Absolute Pressure (MAP) Sensor
Connector 32: | Mass Air Flow (MAF) Sensor
Connector 33: | Rough Road Wheel Speed Sensor
Connector 34: | Throttle Body

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: AMP 174923
- Service: N/A
- Description: 6-Way F (BK)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | 5-Volt Reference 1
2 | WH/BK | -- | 5-Volt Reference 2
3 | BN | -- | Low Reference
4 | BU | -- | APP Sensor 1 Signal
5 | PU | -- | Low Reference
6 | L-BU | -- | APP Sensor 2 Signal

### Camshaft Position (CMP) Sensor

#### Connector Part Information

- OEM: AMP 85205-1
- Service: N/A
- Description: 3-Way F JR Power Timer 3P Hsg Assembly (BK)

#### Camshaft Position (CMP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN/WH | -- | Camshaft Position (CMP) Sensor Signal
2 | PK/BK | -- | Low Reference
3 | PK | -- | Ignition 1 Voltage

### Clutch Switch

#### Connector Part Information

- OEM: PE 107545
- Service: N/A
- Description: Delphi Micro HVT 4-Way F

#### Clutch Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | YE | -- | Clutch Switch Signal
4 | BK | -- | Ground

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: AMP 85205-1
- Service: N/A
- Description: 3-Way F JR Power Timer 3P Hsg Assembly (BK)

#### Crankshaft Position (CKP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE/BK | -- | Crankshaft Position (CKP) Sensor Signal
2 | BU/WH | -- | Low Reference
3 | BN/WH | -- | Ground

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: AK 0442
- Service: N/A
- Description: 2-Way Connector F (BK)

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | -- | Engine Coolant Temperature (ECT) Sensor Signal
2 | BK/WH | -- | Ground

### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | D-GN/WH | -- | EVAP Canister Purge Valve Solenoid Control

### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve

#### Connector Part Information

- OEM: AK 32229
- Service: N/A
- Description: 2-Way F (BN)

#### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | -- | EVAP Canister Vent Solenoid Control
B | PK/BK | -- | Ignition 1 Voltage

### Exhaust Gas Recirculation (EGR) Valve

#### Connector Part Information

- OEM: PED 12129946
- Service: N/A
- Description: 5-Way F Metri-Pack 150 Series, Sealed (GY)

#### Exhaust Gas Recirculation (EGR) Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GY | -- | Exhaust Gas Recirculation (EGR) Solenoid Control
B | BN | -- | Low Reference
C | GY | -- | Exhaust Gas Recirculation (EGR) Valve Position Sensor Signal
D | OG/BK | -- | 5-Volt Reference
E | PK | -- | Ignition 1 Voltage

### Fuel Injector 1

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way F JR Power Timer 2P Hsg Assembly (BK)

#### Fuel Injector 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | BN | -- | Fuel Injector 1 Control

### Fuel Injector 2

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way F JR Power Timer 2P Hsg Assembly (BK)

#### Fuel Injector 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-GN/BK | -- | Fuel Injector 2 Control

### Fuel Injector 3

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way F JR Power Timer 2P Hsg Assembly (BK)

#### Fuel Injector 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | PK/BK | -- | Fuel Injector 3 Control

### Fuel Injector 4

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way F JR Power Timer 2P Hsg Assembly (BK)

#### Fuel Injector 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-BU/BK | -- | Fuel Injector 4 Control

### Fuel Injector 5

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way F JR Power Timer 2P Hsg Assembly (BK)

#### Fuel Injector 5

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | BN/WH | -- | Fuel Injector 5 Control

### Fuel Injector 6

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way F JR Power Timer 2P Hsg Assembly (BK)

#### Fuel Injector 6

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | YE/BK | -- | Fuel Injector 6 Control

### Fuel Pump

#### Connector Part Information

- OEM: KAFUS B06009A
- Service: N/A
- Description: 6-Way F

#### Fuel Pump

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU | -- | Low Fuel Indicator Signal
2 | BK | -- | Ground
3 | GY | -- | Fuel Pump Supply Voltage
4 | PK | -- | Ignition 1 Voltage
5 | YE | -- | Fuel Level Sensor Signal
6 | BN | -- | Low Reference 2.5L
PU | -- | Low Reference 2.0Ll

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: AK 32311
- Service: N/A
- Description: 3-Way Connector F (BK)

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | -- | Low Reference
2 | D-GN | -- | Fuel Tank Pressure (FTP) Signal
3 | GY | -- | 5-Volt Reference

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1

#### Connector Part Information

- OEM: AMP 174257-2
- Service: N/A
- Description: 4-Way M 070 Series Econoseal J MK-2 Plug Assembly 4P (BK)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU/WH | -- | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 Signal
2 | PK | -- | Ignition 1 Voltage
3 | GN/WH | -- | Low Reference
4 | GY | -- | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 Heater Control

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2

#### Connector Part Information

- OEM: KUM PB 625-04027
- Service: N/A
- Description: 4-Way F NMWP 02F-B Ass'y (BK)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GN/WH | -- | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 Signal
2 | PK | -- | Ignition 1 Voltage
3 | BU/WH | -- | Low Reference
4 | GY/WH | -- | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 Heater Control

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1

#### Connector Part Information

- OEM: AMP 174257-2
- Service: N/A
- Description: 4-Way M 070 Series Econoseal J MK-2 Plug Ass'y 4P (BK)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | -- | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 Signal
2 | PK | -- | Ignition 1 Voltage
3 | GN | -- | Low Reference
4 | L-GN/WH | -- | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 Heater Control

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2

#### Connector Part Information

- OEM: KUM PB 625-04027
- Service: N/A
- Description: 4-Way F NMWP 02F-B Ass'y (BK)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 Signal
2 | PK | -- | Ignition 1 Voltage
3 | BU | -- | Low Reference
4 | L-GN | -- | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 Heater Control

### Ignition Coil Module 1

#### Connector Part Information

- OEM: AK 32325
- Service: N/A
- Description: 3-Way Connector F (GY)

#### Ignition Coil Module 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | -- | Ignition Coil 1 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 2

#### Connector Part Information

- OEM: AK 32325
- Service: N/A
- Description: 3-Way Connector F (GY)

#### Ignition Coil Module 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | OG | -- | Ignition Coil 2 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 3

#### Connector Part Information

- OEM: AK 32325
- Service: N/A
- Description: 3-Way Connector F (GY)

#### Ignition Coil Module 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE | -- | Ignition Coil 3 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 4

#### Connector Part Information

- OEM: AK 32325
- Service: N/A
- Description: 3-Way Connector F (GY)

#### Ignition Coil Module 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BU | -- | Ignition Coil 4 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 5

#### Connector Part Information

- OEM: AK 32325
- Service: N/A
- Description: 3-Way Connector F (GY)

#### Ignition Coil Module 5

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GN | -- | Ignition Coil 5 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 6

#### Connector Part Information

- OEM: AK 32325
- Service: N/A
- Description: 3-Way Connector F (GY)

#### Ignition Coil Module 6

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GY | -- | Ignition Coil 6 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way F JR Power Timer 2P Hsg Ass'y (BK)

#### Intake Air Temperature (IAT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | -- | Intake Air Temperature (IAT) Sensor Signal
2 | YE/BK | -- | Low Reference

### Intake Manifold Tuning Valve Solenoid

#### Connector Part Information

- OEM: AMP 174352-2
- Service: N/A
- Description: 2-Way F Econoseal J Mark II + Connector Plug Housing (BK)

#### Intake Manifold Tuning Valve Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | WH/BK | -- | Intake Manifold Tuning Valve Solenoid Control

### Knock Sensor (KS) 1

#### Connector Part Information

- OEM: AMP 368215-1
- Service: N/A
- Description: 3-Way F JPT 3P Ass'y for Knock Sensor (GY)

#### Knock Sensor (KS) 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU/WH | -- | Knock Sensor (KS) 1 Signal
2 | YE/BK | -- | Low Reference
3 | GY | -- | Shield Ground

### Knock Sensor (KS) 2

#### Connector Part Information

- OEM: AMP 368215-1
- Service: N/A
- Description: 3-Way F JPT 3P Ass'y for Knock Sensor (GY)

#### Knock Sensor (KS) 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BU/WH | -- | Knock Sensor (KS) 2 Signal
2 | YE/BK | -- | Low Reference
3 | GY | -- | Shield Ground

### Manifold Absolute Pressure (MAP) Sensor

#### Connector Part Information

- OEM: PED 12129946
- Service: N/A
- Description: 3-Way F Metri-Pack 150 Series, Sealed (GY)

#### Manifold Absolute Pressure (MAP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | -- | Low Reference
B | L-GN | -- | Manifold Absolute Pressure (MAP) Sensor Signal
C | OG/BK | -- | 5-Volt Reference

### Mass Air Flow (MAF) Sensor

#### Connector Part Information

- OEM: AMP 85205-1
- Service: N/A
- Description: 3-Way F JR Power Timer 3P Hsg Ass'y (BK)

#### Mass Air Flow (MAF) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY/BK | -- | Low Reference
2 | YE | -- | Mass Air Flow (MAF) Sensor Signal
3 | PK | -- | Ignition 1 Voltage

### Rough Road Wheel Speed Sensor

#### Connector Part Information

- OEM: PED 12052644
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series, Sealed (L-GY)

#### Rough Road Wheel Speed Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | -- | Ground
B | L-GN | -- | Rough Road Wheel Speed Sensor Signal

### Throttle Body

#### Connector Part Information

- OEM: KAFUS B06009A
- Service: N/A
- Description: 6-Way F

#### Throttle Body

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | -- | 5-Volt Reference 3
2 | PU | -- | Throttle Position (TP) Sensor 2 Signal
3 | BK | -- | Low Reference
4 | BU | -- | Throttle Position (TP) Sensor 1 Signal
5 | BU | -- | TAC Motor Control 1
6 | L-BU | -- | TAC Motor Control 2