For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.
2. Remove the screws and the digital clock.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the digital clock with the screws and tighten to 2.5 N·m (22 lb in).
2. Install the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.