For 1990-2009 cars

Table 1: | Control Valve Body Cover Removal
Table 2: | Control Solenoid (w/Body and TCM) Valve Assembly Removal
Table 3: | Control Valve Body Assembly Removal

### Control Valve Body Cover Removal

Callout | Component Name
--- | ---
1 | Control Valve Body Cover Bolts M6 x 30 (Qty: 13)
2 | Control Valve Body Cover
3 | Control Valve Body Gasket Tip Discard the seal. It is not reusable.
4 | Control Valve Body Cover Wiring Connector Hole Seal Caution: Support the control solenoid valve assembly around the connector when removing the seal. Excessive pulling force can damage the internal electrical connections. Tip Discard the seal. It is not reusable.
5 | Shift Position Switch Connector
6 | Output Speed Sensor Connector
7 | Input Speed Sensor Connector

### Control Solenoid (w/Body and TCM) Valve Assembly Removal

Callout | Component Name
--- | ---
1 | Control Valve Body M5 x 40.5 (Qty: 3)
2 | Control Valve Body Bolt M6 x 30 (Qty: 12)
3 | Control Solenoid (w/Body and TCM) Valve Assembly
4 | Control Solenoid Valve Assembly Filter Plate Caution: Use care when removing or installing the filter plate assembly. A broken or missing retaining tab may not adequately secure the filter plate to the control solenoid valve assembly, resulting in possible damage or contamination.

Tip

• | Discard the filter plate. It is not reusable.

• | Inspect the pressure switch seals for damage or contamination. Replace the control solenoid valve assembly as necessary.

### Control Valve Body Assembly Removal

Callout | Component Name
--- | ---
1 | Fluid Level Control Valve
2 | Fluid Level Control Valve Gasket
3 | Control Valve Body Bolt M6 x 60 (Qty: 9)
4 | Control Valve Body Bolt M6 x 53 (Qty: 2)
5 | Control Valve Body Assembly
6 | Control Valve Body Spacer Plate Assembly
7 | Manual Shaft Detent Spring Bolt M6 x 16 (Qty: 1)
8 | Manual Shaft Detent Lever Spring Assembly
9 | 1-2-3-4 Clutch Fluid Passage Seal Tip Discard the seal. It is not reusable.
10 | Low/Reverse Clutch Fluid Passage Seal Tip Discard the seal. It is not reusable.