For 1990-2009 cars

RPO | Description
--- | ---
11U | Galaxy White (Solid)
13U | White Pearl (Mica)
19U | Granada Black (Mica)
2G0 | Singapore - Mandatory
2G1 | Israel - Mandatory
47U | Poseidon Blue (Mica)
52U | Highway Yellow (TBD)
53U | Kandinsky Red (Mica)
55U | Linen Beige (Metallic)
5TI | Ukraine - Mandatory
60I | Interior Color - Two Tone (Charcoal + Beige)
6G2 | Reinforcement - Roof Panel
79U | Sanddrift Grey (Metallic)
81I | Interior Color - Charcoal + Charcoal
88U | Dark Denim Grey (Mica)
91U | Oak Green (Mica)
92U | Poly Silver (Metallic)
A02 | Windshield - Tinted, Shaded Upper
A11 | Window - Tinted, All
A36 | Solar Control Glass
A69 | DR and Pretensioner and Load Limiter / Co-DR Pretensioner
A70 | DR and Co-DR Pretensioner and Load Limiter
AA7 | Front and RR, DR-Side One Touch (Down Only)
AAR | Knee Bolster, DR/Co-DR Side - EPP Foam Type
ABZ | Front and RR, DR-Side One Touch W/Safety
AG4 | Adjuster FRT ST Manual, 2 Way, Vert, Driver
AH5 | Power Seat (8 Way), Driver Side
AJ3 | Air Bag - SIR - FRT DR
AJ7 | Air Bag - SIR - FRT DR & Co-DR, Side
AK5 | Air Bag - SIR FRT DR and Co-DR
AL5 | Sensored Deactivated Air Bag (Co-DR)
ALU | Rear Seat - Headrest-Separated (3EA)
AM1 | Control Seat, Manual Lumbar, Driver
AM2 | Control Seat, Manual Lumbar, Pass
AMA | Rear Seat - Headrest-Separated (2EA)
AME | Auto Door Lock - w/Emergency
ANK | Rear Seat - Fixed w/Semi HI-BK
AQ2 | Trunk Net
AR1 | Air Bag Delete
ARB | Reinf-Structure,Body (for IIHS)
AT2 | Restraint Head, FRT Seat, Cloth, 2 Way Adjust
AT3 | Child Seat Tether Anchorage Provision
AT7 | 3 Point ELR and 3 Point LH/CTR/RH
AU4 | Auto Door Lock - Speed Sensitive
AWB | 3 Point ELR and 2 Point CTR Lap Belt
AWU | DR and Co-DR Side - ELR
AY0 | SIR - FRT DR and Co-DR Side, Curtain Air Bag
B02 | South Africa - Mandatory
B04 | Taiwan - Mandatory
B07 | India - Mandatory
B12 | Russia - Mandatory
B13 | Australia - Mandatory
B37 | Car Mat w/o logo and w/o Heel Pad (Hook Type)
B6G | Stainless Door Scuff
BAH | Equipment Security System, Immobilization, Step Two
BCC | Key Hole (Passenger)
BD6 | Molding - Roof Molding : Black Color
BF2 | Floor Carpet - Deluxe
BIH | Insulation - Hood
BKI | Rear Garnish - Body Color
BKJ | Rear Garnish - Chrome Coating
BLQ | I.D Plate - Type "A"
BLS | I.D Plate - Type "B"
BLV | I.D Plate - Type "D"
BLW | Plate Inscription Type 'E'
BMC | I.D Plate - Type "H-1"
BMG | Badge - GMDAT
BMS | I.D Plate - Type "Delete I.D Plate"
BPZ | I.D Plate - Type "T"
BRI | Kit - Body Kit, Exhaust Tip
BS1 | NVH Reduction Items
BV3 | Inst Panel - Black
BYR | Wood Grain-II (Level II)
C1V | Wood Grain-II (Level II, Silver Metallic)
C37 | Heating Mat, DR Side
C38 | Heating Mat, Co-DR Side
C50 | Windshield Heated Function
C60 | HVAC - Air Conditioner (Push Button Type)
C66 | HVAC - Uncompleted Air Con For Manual
C68 | HVAC - Full Auto Air Con
C71 | Door Step Lamp - FRT Door (2 Way Courtesy Lamp)
CB7 | Colombia - Mandatory
CE1 | Wiper - Rain Sensing
CF2 | Latvia - Mandatory
CF5 | Sun Roof, Power In-Sliding and Tilt
CF6 | Lithuania - Mandatory
CGK | Libya - Mandatory
CK1 | Pakistan - Mandatory
CL3 | Slovak - Mandatory
CUV | UK - Mandatory
CUX | Estonia - Mandatory
D31 | Inside Rear View Mirror - Manual Day and Night Mirror
D6H | Sunvisor - Sunshade, DR/Co-DR Side, W/Vanity Mirror
D6I | Sunshade, DR/Co-DR Side, w/Vanity Mirror and Illumination
D75 | Grip Type Outside Door Handle - Body Color
D8Q | Czech - Mandatory
D8T | Iran - Mandatory
D8U | Jordan - Mandatory
D8W | Latin America - Mandatory
D8X | Lebanon - Mandatory
D8Y | Macedonia - Mandatory
D8Z | Slovenia - Mandatory
D94 | Touch-Up Paint
DA1 | Rear Seat - Center Armrest w/Deposit
DA5 | Rear Seat - Center Armrest w/o Deposit
DAB | Sunvisor - Covering-Cloth
DAC | Sunvisor - Extension
DH0 | Inside Rear View Mirror - ECM Mirror
DL6 | Outside Rear View Mirror - Manual Folding and Elec. Control
DL7 | Power Folding and Control
DP8 | OSRVM w/Tilting for Reversing (Passenger)
DQA | Mirror Provisions Aux WFOV
DZ0 | Croatia - Mandatory
DZ3 | Malta - Mandatory
DZ5 | CIS - Mandatory
E17 | Front I 2.5 mph / Rear 2.5 mph
E20 | Grip Type Outside Door Handle - Chrome Color
E2U | Trim Level : LS
E46 | Equipment Additional Ecuador
E4V | Equipment CKD - China
E4W | Equipment CKD - Veitnam
E6W | Equipment - East Europe
E6X | Trunk - Trunk Lid Trim
E7W | Fire Extinguisher
E90 | Seat Back Pocket - DR Side
E91 | Seat Back Pocket - Co-DR Side
ECK | Lever - Auto, Straight, TUTD (LHD Only)
ECN | Straight
ERI | Battery Saver
ET8 | Syria - Mandatory
F29 | Final Axle Ratio A/T-2.819 (Fam I, 2.0LPG)
F40 | Suspension - High MTG Type
F45 | Chassis Continuously Variable Real Time Damping
F65 | Final Axle Ratio A/T-2.396 (2.5 GSL)
F67 | Final Axle Ratio A/T-2.700 (2.0 GSL)
F73 | Final Axle Ratio A/T - Final Axle Ratio A/T
F82 | Ratio Transaxle Final Drive 3.23
FG3 | Gas Shock Absorber
FR8 | Ratio Transaxle Final Drive 4.17
FRC | Final Axle Ratio M/T-3.947 (D24)
FV2 | Final Axle Ratio M/T-4.176 (D16)
FW6 | Final Axle Ratio M/T -3.42 (D33)
FXJ | Ratio Transaxle Final Drive 2.64
FXK | Ratio Transaxle Final Drive 2.89
GFM | Regional General Country
GFP | Regional Australia
GFS | Gulf States - Mandatory
GFX | Complete Knock Down (CKD)
GH3 | Saudi Arabia - Mandatory
HDN | Badge - Holden
J65 | Brake - FRT and RR, Disc (non-ABS)
JL9 | Brake - FRT and RR, ABS
JTP | Iridium Spark Plug
K11 | HVAC - Air Filter - Particle
K15 | HVAC - Air Filter - Combi
K34 | Cruise Control (Max. 180 km/h Over) - Included Cancel Function
K35 | Module Electronic Control, High ALT
K36 | Module Electronic Control, Low Volatility Fuel
KAA | T/M Knob - Leather and SGM Local Wood Grain
KC0 | HVAC - Defroster-Interlocking
KE1 | Chile - Mandatory
KEI | HVAC - VAPS
KH1 | T/M Knob - Leather and Silver Metallic Grain
KIX | Trim Level : Lettering (Rear) - SX
KIY | Trim Level : CDX
KKD | Control Localization (CKD Country)
KOC | Car Name : Tosca
KQZ | General - CRC, Hydraulic
KRC | Fuel Rating Octane No. 87
KRD | Fuel Rating Octane No. 91
KRE | Fuel Rating Octane No. 95
LBK | 2.5 L6 DOHC MPI
LBM | 2.0 L6 DOHC MPI
LDA | 1.8 Fam I DOHC MPI
LHD | Left - Hand Drive
LLW | VM 2.0L
M98 | Automatic T/M, 5 Speed - Aisin 55-51E
MFB | 5 Speed S/R (D24)
MFN | 5 Speed S/R (D33)
MH7 | Transmission Auto 6 SPD, HMD, X23FHD
MH8 | Transmission Auto 6 SPD, HMD, X23F
MLM | Manual T/M-5 Speed SW/R (D16)
MLS | Automatic T/M, 4 Speed - Aisin 50-40E
MPN | General - CRC, Hydraulic
N12 | Muffler - Standard (Warranty 2 Years)
N33 | Manual Tilting Steering Column
N37 | Manual Telescope Steering Column
N40 | Steering - Power
N44 | Steering Wheel - 4 Spoke STD
NC0 | EEC/ECE Equipment
NPH | Muffler - Heavy Duty (Warranty 3 Years)
NQL | Emission System Korean, LEV
NQT | Emission System Open Loop, Leaded (GMDAT)
NR0 | Steering Wheel - Leather
NT2 | Emission System EEC 96
NT3 | Emission System EEC 00
NT4 | Emission System EEC 05
NU2 | Emission System California, ULEV2
NV3 | 6.0J X 16", Alloy-Silver Coating
NV8 | Steering - Speed Sensitive Power (SSPS)
NW9 | Traction Control System (TCS)
PB1 | Cover, Wheel 15 Inch
PFB | Interior Flocking
PFE | Wheel 17 X 7, Aluminum
PG1 | Temporary Spare Tire
PG9 | 6.0J X 15", Steel (Silver)
QBP | Tire All 215/50R17 BW PE/ST TL ALS
QCR | Tire All 205/65R15 BW NY/ST TL ALS
QI2 | Trim Level Name : Trim Level #2
QI3 | Trim Level Name : Trim Level #3
QQ4 | Tire and Wheel Spare, Full Size, Aluminum
QQ5 | Tire and Wheel Spare, Full Size, Steel
QQ6 | Temporary Spare Tire
QRI | Tire All P205/60R16-91S BW TL AL2
RHD | Right - Hand Drive
SBW | Head Lamp - Projection New I
T2C | Cold Area Pack
T2Y | Child Seat Fix Provision
T37 | Fog Lamp, Front (Projection Type)
T44 | Speed Warning Device
T79 | Fog Lamp, Rear (Separate)
T82 | Headlamps Control Automatic On-Off
T84 | Head Lamp Regulation ECE Type, LHD
T85 | Head Lamp Regulation ECE Type, RHD
T89 | Rear And Trunk Combination Lamp - ECE Type
T90 | Side Turn Signal, OSRVM
T96 | Fog Lamp, Front (MFR Type)
TDW | Heavy Duty Corrosion Spec.
TFK | Alarm - Seat Belt Warning, LH
TFM | Alarm - Seat Belt Warning, LH
TQE | Day Time Running Light
TR1 | Rear And Trunk Combination Lamp - SAE Type
TR6 | Head Lamp Leveling Device
TS6 | CHMSL
TUK | Turn Signal Lamp - ECE Type
U05 | Horn - Conventional Type
U07 | Horn - Trumpet Horn Type
U17 | Analog Cluster - STD
U18 | Meter Cluster - Kilometers
U27 | Glove Box Lamp
U63 | Speaker - 9EA (FRT and RR DR and LP Tweeter L/R and RR Tweeter L/R and Sub Woofer)
U68 | Driver Info Display
U77 | Antenna - Back Glass - Radio
UA5 | Keyless Entry - Anti Theft Alarm w/Door and Trunk Opening
UAY | Audio - Radio and 6 INDASH CDC w/MP3
UAZ | Audio - Radio and 6 INDASH CDC (w/RDS) w/MP3
UC1 | Meter Cluster - Miles
UD7 | Obstacle Detection System (RR Only)
UGB | License Plate Lamp - ECE Type
UPK | Radio and CDP (w/MP3)
UPR | Audio - Cassette and Radio and CDP (w/MP3)
UPT | Audio - Cassette and Radio Logic Deck
UQD | Audio - Cassette and Radio and 6 INDASH CDC
UQE | Audio - Radio and CDP (w/RDS) w/MP3
UW6 | Speaker - 6EA (FRT and RR DR and IP Tweeter L/R)
UX8 | Speaker - Radio and 6 INDASH CDC (w/RDS) w/MP3
VA8 | Label - Spanish
VFT | Standard Corrosion Spec.
VGC | Wrap Guard
VHD | Door Impact Pad
VIX | Visible VIN
VIY | Asterisk Mark
VK8 | Sunglass Holder
VNR | VIN Model Year 2007
VNS | VIN Model Year 2008
VNT | VIN Model Year 2009
VNU | I.D Body - US Type
VNW | I.D Body - EU (ISO) Type
VRP | Africa - Mandatory
VTW | Deposit - IP, w/LID
VXC | Audio Power Amplifier 4-CH
VY7 | Leather T/M Knob
W1I | Seat Covering - Leather Covering I (Havana)
W1Y | Leather Covering I (Havana)
W2V | Trim Level : No Lettering
W36 | Trim Level : Lettering (Rear): CDXI
W6C | Seat Covering - Cloth Type II
W6E | Seat Covering - Cloth Type I
W6R | Seat Covering - Leather Covering
WBR | Car Name : Epica
WCM | Trim Level : Lettering (Rear) : LT
WU5 | Dimmer - Inst. Cluster
XA1 | China - Mandatory
XX6 | Audio - Radio Blank (w/Harness)
XZ1 | Hot Area Pack
Y9Y | Badge - Chevrolet
Z5U | Heating
Z5V | Blue Mirror