For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Drive Link Lube Scoop
2 | Drive Link Lube Scoop Seals
3 | Driven Sprocket Assembly, Drive Sprocket and Park Gear Assembly and Drive Link Tip

1. The drive link, drive and driven sprocket assemblies must be removed at the same time.
2. The driven sprocket ball bearing inner race has a slight interference fit with the case. Pull straight up to ease removal.

4 | Driven Sprocket Bearing Assembly Tip The driven sprocket bearing may be stuck to the driven sprocket.
5 | Front Differential Carrier Baffle Bolts M6 x 16 (Qty: 2)
6 | Front Differential Carrier Baffle
7 | Park Pawl Shaft
8 | Park Pawl Spring
9 | Park Pawl