For 1990-2009 cars

#### Range Reference Table

Range | Park | Reverse | Neutral | Drive
--- | --- | --- | --- | ---
1st Braking | 1st | 2nd | 3rd | 4th | 5th | 6th
1-2-3-4 Clutch | -- | -- | -- | Applied | Applied | Applied | Applied | Applied | -- | --
3-5 Reverse Clutch | -- | Applied | -- | -- | -- | -- | Applied | -- | Applied | --
4-5-6 Clutch | -- | -- | -- | -- | -- | -- | -- | Applied | Applied | Applied
2-6 Clutch | -- | -- | -- | -- | -- | Applied | -- | -- | -- | Applied
Low and Reverse Clutch | Applied* | Applied | Applied* | Applied | -- | -- | -- | -- | -- | --
Low Clutch Assembly (OWL) | -- | -- | -- | Holding | Holding | -- | -- | -- | -- | --
* = Applied with NO load