For 1990-2009 cars

Connector 1: | Input Speed Sensor
Connector 2: | Output Speed Sensor
Connector 3: | Park/Neutral Position Switch
Connector 4: | Transaxle
Connector 5: | Transmission Control Module (TCM) A
Connector 6: | Transmission Control Module (TCM) (B)
Connector 7: | Winter Mode Switch

### Input Speed Sensor

#### Connector Part Information

- OEM: YZK 7283-8125-30
- Service: N/A
- Description: 2-Way F 090II Type Sealed

#### Input Speed Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-GN/BK | -- | Input Shaft Speed Sensor Low
2 | PU/WH | -- | Input Shaft Speed Sensor High

### Output Speed Sensor

#### Connector Part Information

- OEM: YZK 7283-8125-30
- Service: N/A
- Description: 2-Way F 090II Type Sealed

#### Output Speed Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | -- | Input Shaft Speed Sensor Low
2 | YE | -- | Input Shaft Speed Sensor High

### Park/Neutral Position Switch

#### Connector Part Information

- OEM: YZK 7223-6508-30
- Service: N/A
- Description: 10-Way F DMS+RV Sealed

#### Park/Neutral Position Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-GN | -- | Reverse Signal
3 | BK/WH | -- | Ground
4 | PK/BK | -- | Park/Neutral Signal
5 | GY | -- | C Signal
6 | YE | -- | B Signal
7 | -- | -- | Not Used
8 | WH | -- | PA Signal
9 | PK | -- | Ignition 1 Voltage
10 | BN/WH | -- | A Signal

### Transaxle

#### Connector Part Information

- OEM: YZK 7223-6509-40
- Service: N/A
- Description: 14-Way F 050 Sealed

#### Transaxle

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG/BK | -- | Transmission Fluid Temperature Sensor Low Reference
2 | BU/WH | -- | Shift Pressure Control Solenoid Control
3 | PU/WH | -- | TCC Clutch Solenoid Control
4 | WH | -- | Line Pressure Control Solenoid Control
5 | -- | -- | Not Used
6 | WH | -- | Shift Solenoid 4 Supply Voltage
7 | YE | -- | Shift Solenoid 2 Supply Voltage
8 | BN/WH | -- | Transmission Fluid Temperature Sensor Signal
9 | PK/BK | -- | Shift Pressure Control Solenoid Supply Voltage
10 | GN | -- | TCC Clutch Solenoid Supply Voltage
11 | BU | -- | Line Pressure Control Solenoid Supply Voltage
12 | OG/WH | -- | Shift Solenoid 5 Supply Voltage
13 | WH | -- | Shift Solenoid 3 Supply Voltage
14 | L-GN | -- | Shift Solenoid 1 Supply Voltage

### Transmission Control Module (TCM) A

#### Connector Part Information

- OEM: TYCO 1318756-2
- Service: N/A
- Description: 24-Way F 025/090III Hybrid Unsealed

#### Transmission Control Module (TCM) A

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | WH | -- | Line Pressure Control Solenoid Control
3 | PU/WH | -- | TCC Clutch Solenoid Control
4 | BU | -- | Line Pressure Control Solenoid Supply Voltage
5 | GN | -- | TCC Clutch Solenoid Supply Voltage
6 | PK | -- | Ignition 1 Voltage
7 | BN | -- | High Speed GMLAN Serial Data (-)
8-10 | -- | -- | Not Used
11 | BN/WH | -- | Transmission Fluid Temperature Sensor Signal
12 | OG/BK | -- | Transmission Fluid Temperature Sensor Low Reference
13 | WH | -- | Shift Solenoid 4 Supply Voltage
14 | WH | -- | Shift Solenoid 3 Supply Voltage
15 | YE/BK | -- | Shift Solenoid 2 Supply Voltage
16 | L-GN | -- | Shift Solenoid 1 Supply Voltage
17 | BN/BK | -- | High Speed GMLAN Serial Data (+)
18 | -- | -- | Not Used
19 | BU/WH | -- | Shift Pressure Control Solenoid Control
20 | -- | -- | Not Used
21 | PK/BK | -- | Shift Pressure Control Solenoid Supply Voltage
22 | OG/WH | -- | Shift Solenoid 5 Supply Voltage
23 | BK/WH | -- | Ground
24 | OG | -- | Battery Positive Voltage (RHD)
RD/WH | -- | Battery Positive Voltage (LHD)

### Transmission Control Module (TCM) (B)

#### Connector Part Information

- OEM: TYCO 1318757-2
- Service: N/A
- Description: 26-Way F 025/090III Hybrid Unsealed

#### Transmission Control Module (TCM) (X2)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | -- | Tap Up Signal
2 | -- | -- | Not Used
3 | L-GN | -- | Winter Mode Indicator Control
4 | L-GN/WH | -- | Winter Mode Switch Signal
5 | PU | -- | Output Shaft Speed Sensor Signal Low
6 | L-GN/BK | -- | Input Shaft Speed Sensor Signal Low
7 | YE | -- | B Signal
8 | BN/WH | -- | A Signal
9 | BN | -- | Driver Shift Control
10-13 | -- | -- | Not Used
14 | YE | -- | Output Shaft Speed Sensor Signal High
15 | GN | -- | Vehicle Speed Signal
GN/WH | -- | Vehicle Speed Signal (Holden, RHD Diesel, Euro/Gen)
16 | PU/WH | -- | Input Shaft Speed Sensor Signal High
17 | GN | -- | Serial Data
18 | BN | -- | Tap Down Signal
19 | WH | -- | PA Signal
20 | GY | -- | C Signal
21 | -- | -- | Not Used
22 | L-BU | -- | Stop Lamp Switch Signal
23-26 | -- | -- | Not Used

### Winter Mode Switch

#### Connector Part Information

- OEM: KET MG652999
- Service: N/A
- Description: 4-Way F 040 Unsealed

#### Winter Mode Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-GN | -- | Winter Mode Switch Signal
3 | BN/WH | -- | Illumination Control
4 | GN | -- | Ground