For 1990-2009 cars

Connector 1: | Door Latch Switch - Driver
Connector 2: | Door Latch Switch - Passenger
Connector 3: | Door Latch Switch - LR
Connector 4: | Door Latch Switch - RR
Connector 5: | Door Lock Actuator - Driver
Connector 6: | Door Lock Actuator - Passenger
Connector 7: | Door Lock Actuator - LR
Connector 8: | Door Lock Actuator - RR
Connector 9: | Door Tamper Switch - Driver
Connector 10: | Trunk Latch
Connector 11: | Trunk Release Switch
Connector 12: | Window/Door Lock Switch A - Driver
Connector 13: | Window/Door Lock Switch B - Driver
Connector 14: | Window/Door Lock Switch - Passenger

### Door Latch Switch - Driver

#### Connector Part Information

- OEM: PKI 15011-04F, PKI 832419
- Service: N/A
- Description: 4-Way F Connector

#### Door Latch Switch - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | -- | All Contact Input
2 | GY | -- | Door Ajar Signal
3 | BN | -- | Driver Front Door Contact Input
4 | BK | -- | Ground

### Door Latch Switch - Passenger

#### Connector Part Information

- OEM: PKI 15011-04F, PKI 832419
- Service: N/A
- Description: 4-Way F Connector

#### Door Latch Switch - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | -- | -- | Not Used
3 | BN | -- | Door Ajar Signal
4 | WH | -- | All Contact Input

### Door Latch Switch - LR

#### Connector Part Information

- OEM: PKI 15011-04F, PKI 832419
- Service: N/A
- Description: 4-Way F Connector

#### Door Latch Switch - LR

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | -- | All Contact Input
2 | -- | -- | Not Used
3 | BN | -- | Door Ajar Signal
4 | WH | -- | Courtesy Lamp Control

### Door Latch Switch - RR

#### Connector Part Information

- OEM: PKI 15011-04F, PKI 832419
- Service: N/A
- Description: 4-Way F Connector

#### Door Latch Switch - RR

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | -- | -- | Not Used
3 | BN | -- | Door Ajar Signal
4 | WH | -- | All Contact Input

### Door Lock Actuator - Driver

#### Connector Part Information

- OEM: AK 6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | -- | Door Lock Actuator Unlock Control
B | GY | -- | Door Lock Actuator Lock Control

### Door Lock Actuator - Passenger

#### Connector Part Information

- OEM: AK 6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | -- | Door Lock Actuator Unlock Control
B | GY | -- | Door Lock Actuator Lock Control

### Door Lock Actuator - LR

#### Connector Part Information

- OEM: AK 6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - LR

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | -- | Door Lock Actuator Unlock Control
B | GY | -- | Door Lock Actuator Lock Control

### Door Lock Actuator - RR

#### Connector Part Information

- OEM: AK 6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - RR

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | -- | Door Lock Actuator Unlock Control
B | GY | -- | Door Lock Actuator Lock Control

### Door Tamper Switch - Driver

#### Connector Part Information

- OEM: PKI 15011-04F, PKI 832419
- Service: N/A
- Description: 4-Way F Connector

#### Door Tamper Switch - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | -- | Door Lock Control
2 | BK | -- | Ground
3 | WH | -- | Door Unlock Control
4 | L-BU | -- | Ajar Switch Signal

### Trunk Latch

#### Connector Part Information

- OEM: KET MG 651032
- Service: N/A
- Description: 3-Way F

#### Trunk Latch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-BU | -- | Trunk Latch Actuator Supply Voltage
3 | OG/BK | -- | Trunk Open Switch Signal

### Trunk Release Switch

#### Connector Part Information

- OEM: KET MG 651201-4
- Service: N/A
- Description: 2-Way F

#### Trunk Release Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Ignition Voltage
2 | RD | -- | Trunk Latch Actuator Supply Voltage

### Window/Door Lock Switch A - Driver

#### Connector Part Information

- OEM: KET MG 651056
- Service: N/A
- Description: 10-Way F 090-II Series (WH)

#### Window/Door Lock Switch A - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-GN | -- | Power Window Master Switch Right Rear Up Signal
2 | PU | -- | Power Window Master Switch Right Rear Down Signal
3 | D-GN | -- | Power Window Master Switch Left Rear Up Signal
4 | PU | -- | Power Window Master Switch Left Rear Down Signal
5 | L-BU | -- | Power Window Master Switch Passenger Front Down Signal
5 | BN | -- | Power Window Motor Driver Front Down Control (Holden, RHD Diesel, Euro/Gen)
6 | OG | -- | Power Window Supply Voltage
6 | BK | -- | Ground (Holden, RHD Diesel, Euro/Gen)
7 | OG | -- | Power Window Supply Voltage (Holden, RHD Diesel, Euro/Gen)
7 | BN | -- | Power Window Master Switch Passenger Front Down Signal
8 | BN | -- | Power Window Motor Driver Front Down Control
8 | L-BU | -- | Power Window Master Switch Passenger Front Down Signal (Holden, RHD Diesel, Euro/Gen)
9 | PK | -- | Power Window Master Switch Lockout Control
9 | BN | -- | Power Window Master Switch Passenger Front Down Signal (Holden, RHD Diesel, Euro/Gen)
10 | BK | -- | Ground
10 | PK/BK | -- | Power Window Master Switch Lockout Control (Holden, RHD Diesel, Euro/Gen)

### Window/Door Lock Switch B - Driver

#### Connector Part Information

- OEM: KET MG 651044
- Service: N/A
- Description: 6-Way F 090 II Series (WH)

#### Window/Door Lock Switch B - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG/BK | -- | Power Window Motor Driver Front Up Control
2 | BU/WH | -- | Power Window Switch Driver Front Express Down Signal
3 | -- | -- | Not Used
4 | L-BU | -- | Door Lock Control
5 | WH | -- | Door Unlock Control
6 | OG/BU | -- | Auto Up

### Window/Door Lock Switch - Passenger

#### Connector Part Information

- OEM: KET MG 651050
- Service: N/A
- Description: 8-Way F 090-II Series (WH)

#### Window/Door Lock Switch - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | -- | Power Window Master Switch Passenger Front Down Signal
2 | PK | -- | Power Window Master Switch Lockout Control
3 | L-BU | -- | Power Window Master Switch Passenger Front Up Signal
4 | D-BU | -- | Power Window Motor Passenger Front Up Control
5 | L-BU | -- | Door Llock Control
6 | BK | -- | Ground
7 | WH | -- | Door Unlock Control
8 | BN/RD | -- | Power Window Motor Passenger Front Down Control