For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
3. Press the clips down and remove the instrument cluster lens.
4. Remove the tachometer from the instrument cluster.

### Installation Procedure

1. Install the tachometer to the instrument cluster.
2. Install the instrument cluster lens.
3. Install the instrument cluster. Refer to Instrument Cluster Replacement .
4. Connect the negative battery cable.