For 1990-2009 cars

Connector 1: | A/C Compressor Clutch
Connector 2: | A/C Refrigerant Pressure Sensor
Connector 3: | Accelerator Pedal Position (APP) Sensor (LBM/LBK)
Connector 4: | Accelerator Pedal Position Sensor (LLW)
Connector 5: | Air Temperature Actuator
Connector 6: | Ambient Air Temperature Sensor (C68)
Connector 7: | Ashtray Lamp
Connector 8: | Automatic Transmission (M98)
Connector 9: | Automatic Transmission (MH7/MH8)
Connector 10: | Automatic Transmission Control Indicator (MH7/MH8)
Connector 11: | Automatic Transmission Shift Lever (M98)
Connector 12: | Auxiliary Power Outlet
Connector 13: | Backup Lamp - Left
Connector 14: | Backup Lamp - Right
Connector 15: | Backup Lamp Switch (MFB/MFN)
Connector 16: | Blower Motor
Connector 17: | Blower Motor Resistor (C60/C66)
Connector 18: | Blower Motor Switch (C60/C66)
Connector 19: | Body Control Module X1
Connector 20: | Body Control Module X2
Connector 21: | Body Control Module X3
Connector 22: | Body Control Module X4
Connector 23: | Body Control Module X5
Connector 24: | Boost Pressure Actuator (LLW)
Connector 25: | Boost Pressure Sensor (LLW)
Connector 26: | Brake Fluid Level Switch
Connector 27: | Camshaft Position (CMP) Sensor
Connector 28: | CAN Test Connector (MH7/MH8)
Connector 29: | Center Dome Lamp
Connector 30: | Center High Mounted Stop Lamp (CHMSL)
Connector 31: | Cigar Lighter
Connector 32: | Clock
Connector 33: | Clutch Switch (LBM/LBK w/MFB/MFN)
Connector 34: | Cooling Fan - Auxiliary
Connector 35: | Cooling Fan - Main
Connector 36: | Crankshaft Position (CKP) Sensor
Connector 37: | Data Link Connector (DLC)
Connector 38: | Diesel Particulate Filter Pressure Sensor (LLW)
Connector 39: | Diode
Connector 40: | Door Latch Switch - Driver
Connector 41: | Door Latch Switch - Left Rear
Connector 42: | Door Latch Switch - Passenger
Connector 43: | Door Latch Switch - Right Rear
Connector 44: | Door Lock Actuator - Driver
Connector 45: | Door Lock Actuator - Left Rear
Connector 46: | Door Lock Actuator - Passenger
Connector 47: | Door Lock Actuator - Right Rear
Connector 48: | Door Step Lamp - Driver
Connector 49: | Door Step Lamp - Passenger
Connector 50: | Door Tamper Switch - Driver
Connector 51: | Door Tamper Switch - Passenger
Connector 52: | Driver Information Center (DIC)
Connector 53: | Electronic Brake Control Module (EBCM) (JL9/NW9)
Connector 54: | Electronic Brake Control Module (EBCM) (F45)
Connector 55: | Electronic Brake Control Module (EBCM) (JL9/NW9-F45)
Connector 56: | Electronic Stability Control Switch (F45)
Connector 57: | Engine Control Module (ECM) X1
Connector 58: | Engine Control Module (ECM) X2
Connector 59: | Engine Coolant Temperature (ECT) Sensor (LBK/LBM)
Connector 60: | Engine Coolant Temperature (ECT) Sensor (LLW)
Connector 61: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LBK/LBM)
Connector 62: | Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LBK/LBM)
Connector 63: | Exhaust Gas Recirculation (EGR) Valve (LBK/LBM)
Connector 64: | Exhaust Gas Recirculation (EGR) Valve (LLW)
Connector 65: | Exhaust Gas Temperature Sensor 1 (LLW)
Connector 66: | Exhaust Gas Temperature Sensor 2 (LLW)
Connector 67: | Fog Lamp - Left Front
Connector 68: | Fog Lamp - Left Rear
Connector 69: | Fog Lamp - Right Front
Connector 70: | Fog Lamp - Right Rear
Connector 71: | Front Defogger
Connector 72: | Fuel Filter Heater/Temperature Sensor (LLW)
Connector 73: | Fuel Injector 1 (LBK/LBM)
Connector 74: | Fuel Injector 1 (LLW)
Connector 75: | Fuel Injector 2 (LBK/LBM)
Connector 76: | Fuel Injector 2 (LLW)
Connector 77: | Fuel Injector 3 (LBK/LBM)
Connector 78: | Fuel Injector 3 (LLW)
Connector 79: | Fuel Injector 4 (LBK/LBM)
Connector 80: | Fuel Injector 4 (LLW)
Connector 81: | Fuel Injector 5 (LBK/LBM)
Connector 82: | Fuel Injector 6 (LBK/LBM)
Connector 83: | Fuel Pump (LBM/LBK)
Connector 84: | Fuel Pump Module (LLW)
Connector 85: | Fuel Rail Pressure Control Valve (LLW)
Connector 86: | Fuel Rail Pressure Sensor (LLW)
Connector 87: | Fuel Tank Pressure (FTP) Sensor (LBK/LBM)
Connector 88: | Generator
Connector 89: | Glow Plug Control Unit (LLW)
Connector 90: | Hazard Switch
Connector 91: | Headlamp - Left (TR6)
Connector 92: | Headlamp - Left (-TR6)
Connector 93: | Headlamp - Right (TR6)
Connector 94: | Headlamp - Right (-TR6)
Connector 95: | Headlamp Switch
Connector 96: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LBK/LBM)
Connector 97: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LBK/LBM)
Connector 98: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LBK/LBM)
Connector 99: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LBK/LBM)
Connector 100: | Heated Seat - Driver (C37)
Connector 101: | Heated Seat - Passenger (C38)
Connector 102: | Heated Seat Switch - Driver (C37)
Connector 103: | Heated Seat Switch - Passenger (C38)
Connector 104: | High Pressure Pump (LLW)
Connector 105: | High Speed Blower Motor Relay (C68)
Connector 106: | Hood Ajar Switch
Connector 107: | Horn - High
Connector 108: | Horn - Low
Connector 109: | HVAC Control Module (C60/C66)
Connector 110: | HVAC Control Module X1 (C68)
Connector 111: | HVAC Control Module X2 (C68)
Connector 112: | Ignition Coil Module 1 (LBK/LBM)
Connector 113: | Ignition Coil Module 2 (LBK/LBM)
Connector 114: | Ignition Coil Module 3 (LBK/LBM)
Connector 115: | Ignition Coil Module 4 (LBK/LBM)
Connector 116: | Ignition Coil Module 5 (LBK/LBM)
Connector 117: | Ignition Coil Module 6 (LBK/LBM)
Connector 118: | Ignition Switch
Connector 119: | Immobilizer
Connector 120: | Inflatable Restraint I/P Module
Connector 121: | Inflatable Restraint Roof Rail Module - Left (AY0)
Connector 122: | Inflatable Restraint Roof Rail Module - Right (AY0)
Connector 123: | Inflatable Restraint Sensing and Diagnostic Module (SDM)
Connector 124: | Inflatable Restraint Side Impact Module - Driver (AY0)
Connector 125: | Inflatable Restraint Side Impact Module - Passenger (AY0)
Connector 126: | Inflatable Restraint Side Impact Sensor - Left (AY0)
Connector 127: | Inflatable Restraint Side Impact Sensor - Right (AY0)
Connector 128: | Inflatable Restraint Steering Wheel Module
Connector 129: | Inflatable Restraint Steering Wheel Module Coil X1
Connector 130: | Inflatable Restraint Steering Wheel Module Coil X2
Connector 131: | Input Speed Sensor (M98)
Connector 132: | Inside Rearview Mirror
Connector 133: | Instrument Panel Cluster (IPC) X1
Connector 134: | Instrument Panel Cluster (IPC) X2
Connector 135: | Instrument Panel Cluster (IPC) X3
Connector 136: | Instrument Panel Cluster (IPC) X4 (M98)
Connector 137: | Instrument Panel Cluster (IPC) X4 (MH7/MH8)
Connector 138: | Intake Air Temperature (IAT) Sensor (LBK/LBM)
Connector 139: | Intake Manifold Tuning Valve Solenoid (LBK/LBM)
Connector 140: | I/P Compartment Lamp
Connector 141: | I/P Compartment Lamp Switch
Connector 142: | Key Reminder Switch
Connector 143: | Knock Sensor (KS) 1 (LBK/LBM)
Connector 144: | Knock Sensor (KS) 2 (LBK/LBM)
Connector 145: | License Lamp
Connector 146: | Magnetic Steering Actuator (N40/NV8)
Connector 147: | Manifold Absolute Pressure (MAP) Sensor (LBK/LBM)
Connector 148: | Mass Air Flow (MAF) Sensor (LBK/LBM)
Connector 149: | Mass Air Flow (MAF) Sensor (LLW)
Connector 150: | Mode Actuator
Connector 151: | Multifunction Control Module X1
Connector 152: | Multifunction Control Module X2
Connector 153: | Multifunction Control Module X3
Connector 154: | Multifunction Switch
Connector 155: | Multifunction/Turn Signal Switch
Connector 156: | Object Detection Alarm (UD7)
Connector 157: | Object Detection Module (UD7)
Connector 158: | Object Detection Sensor - Left Corner (UD7)
Connector 159: | Object Detection Sensor - Left Middle (UD7)
Connector 160: | Object Detection Sensor - Right Corner (UD7)
Connector 161: | Object Detection Sensor - Right Middle (UD7)
Connector 162: | Oil Feeding Connector (JL9-F45)
Connector 163: | Oil Feeding Connector (JL9+F45)
Connector 164: | Oil Pressure Switch
Connector 165: | Output Speed Sensor (M98)
Connector 166: | Outside Rearview Mirror - Driver
Connector 167: | Outside Rearview Mirror - Passenger
Connector 168: | Park/Neutral Position Switch (M98)
Connector 169: | Park Brake Switch
Connector 170: | Passenger Airbag/Seat Belt Warning Lamp
Connector 171: | Passenger Presence System Sensor (AL5)
Connector 172: | Power Amplifier (U63)
Connector 173: | Power Seat Switch (AH5)
Connector 174: | Power Seat Test Connector (AH5)
Connector 175: | Power Steering Control Module (N40/NV8)
Connector 176: | PRNDL Lamp
Connector 177: | PTC Heater (LLW)
Connector 178: | Radio X1
Connector 179: | Radio X2
Connector 180: | Radio Antenna Module
Connector 181: | Rain Sensor (CEI)
Connector 182: | Rear Compartment Lamp
Connector 183: | Rear Compartment Release Switch
Connector 184: | Rear Window Defogger Grid X1
Connector 185: | Rear Window Defogger Grid X2
Connector 186: | Recirculation Actuator
Connector 187: | Seat Belt Pretensioner - Driver
Connector 188: | Seat Belt Pretensioner - Passenger
Connector 189: | Seat Belt Switch - Driver
Connector 190: | Seat Belt Switch - Passenger
Connector 191: | Speaker - Left Front
Connector 192: | Speaker - Left Rear
Connector 193: | Speaker - Right Front
Connector 194: | Speaker - Right Rear
Connector 195: | Steering Angle Sensor (F45)
Connector 196: | Stop Lamp Switch
Connector 197: | Subwoofer Speaker
Connector 198: | Sunload Sensor (C68/T82)
Connector 199: | Sunroof Module (CF5)
Connector 200: | Sunroof Switch/Reading Lamp (CF5)
Connector 201: | Tail Lamp - Left
Connector 202: | Tail Lamp - Right
Connector 203: | Theft Deterrent Alarm
Connector 204: | Throttle Body (LBK/LBM)
Connector 205: | Throttle Plate Actuator (LLW)
Connector 206: | Traction Control Switch (NW9)
Connector 207: | Transmission Control Module (TCM) X1 (M98)
Connector 208: | Transmission Control Module (TCM) X2 (M98)
Connector 209: | Trunk Latch
Connector 210: | Trunk Tamper Switch
Connector 211: | Turn Signal Lamp - Left Front (TR6)
Connector 212: | Turn Signal Lamp - Right Front (TR6)
Connector 213: | Turn Signal/Park Lamp - Left Front (-TR6)
Connector 214: | Turn Signal/Park Lamp - Right Front (-TR6)
Connector 215: | Tweeter - Left Front
Connector 216: | Tweeter - Left Rear
Connector 217: | Tweeter - Right Front
Connector 218: | Tweeter - Right Rear
Connector 219: | Vanity Lamp - Left
Connector 220: | Vanity Lamp - Right
Connector 221: | Vehicle Speed Sensor (MFB/MFN)
Connector 222: | Water In Fuel Sensor (LLW)
Connector 223: | Wheel Speed Sensor (WSS) - Left Front (JL9/NW9)
Connector 224: | Wheel Speed Sensor (WSS) - Left Rear (JL9/NW9)
Connector 225: | Wheel Speed Sensor (WSS) - Right Front (JL9/NW9)
Connector 226: | Wheel Speed Sensor (WSS) - Right Rear (JL9/NW9)
Connector 227: | Window/Door Lock Switch - Driver X1
Connector 228: | Window/Door Lock Switch - Driver X2
Connector 229: | Window/Door Lock Switch - Passenger
Connector 230: | Window Motor - Driver (AA7)
Connector 231: | Window Motor - Driver (ABZ)
Connector 232: | Window Motor - Left Rear
Connector 233: | Window Motor - Passenger
Connector 234: | Window Motor - Right Rear
Connector 235: | Window Switch - Left Rear
Connector 236: | Window Switch - Right Rear
Connector 237: | Windshield Washer Fluid Pump - Front
Connector 238: | Windshield Washer Fluid Switch
Connector 239: | Windshield Wiper Motor
Connector 240: | Windshield Wiper/Washer Switch X1
Connector 241: | Windshield Wiper/Washer Switch X2
Connector 242: | Winter Mode Switch (M98)
Connector 243: | Yaw Rate Sensor (F45)

### A/C Compressor Clutch

#### Connector Part Information

- OEM: AK32232
- Service: N/A
- Description: GY

#### A/C Compressor Clutch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-GN | -- | A/C Compressor Clutch Supply Voltage
B | BK | -- | Ground

### A/C Refrigerant Pressure Sensor

#### Connector Part Information

- OEM: AK32316
- Service: N/A
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### A/C Refrigerant Pressure Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | 5-Volt Reference (LHD)
L-BU | -- | 5-Volt Reference (RHD)
2 | BN | -- | Ground
3 | OG/BK | -- | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position (APP) Sensor (LBM/LBK)

#### Connector Part Information

- OEM: 174923-2
- Service: N/A
- Description: 6-Way F Multilock 070 Series (BK)

#### Accelerator Pedal Position (APP) Sensor (LBM/LBK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | 5-Volt Reference 1
2 | WH/BK | -- | 5-Volt Reference 2
3 | BN | -- | Low Reference
4 | BU | -- | APP Sensor 1 Signal
5 | PU | -- | Low Reference
6 | L-BU | -- | APP Sensor 2 Signal

### Accelerator Pedal Position Sensor (LLW)

#### Connector Part Information

- OEM: 936394-2
- Service: N/A
- Description: 6-Way F 2.8mm Series Sealed (BK)

#### Accelerator Pedal Position Sensor (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1274 | Accelerator Pedal Position 5-Volt Reference 2
2 | WH/BK | 543 | Accelerator Pedal Position 5-Volt Reference 1
3 | BN | 1271 | Accelerator Pedal Position Low Reference 1
4 | D-BU | 1161 | Accelerator Pedal Position Signal 1
5 | PU | 1272 | Accelerator Pedal Position Low Reference 2
6 | L-BU | 1162 | Accelerator Pedal Position Signal 2

### Air Temperature Actuator

#### Connector Part Information

- OEM: MG610203
- Service: N/A
- Description: WH

#### Air Temperature Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | -- | Air Temperature
3 | BN | -- | Low Reference
4 | -- | -- | Not Used
5 | YE | -- | Low Reference
6 | YE/BK | -- | Lower Mode Door Position Signal
7 | L-BU | -- | Air Temperature Door Control

### Ambient Air Temperature Sensor (C68)

--

#### Connector Part Information

- OEM: MG610327
- Service: N/A
- Description: 3-Way (BK)

#### Ambient Air Temperature Sensor (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Low Reference
2 | -- | -- | Not Used
3 | L-GN/BK | -- | Ambient Air Temperature Sensor Signal

### Ashtray Lamp

#### Connector Part Information

- OEM: JC 60-1257
- Service: N/A
- Description: 2-Way F (BK)

#### Ashtray Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Dimmer PWM Output
2 | D-GN | -- | Ground

### Automatic Transmission (M98)

#### Connector Part Information

- OEM: 7223-6509-40
- Service: N/A
- Description: 14-Way F RV Series, Sealed (GY)

#### Automatic Transmission (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Transmission Fluid Temperature Sensor Low Reference
2 | BU/WH | -- | Shift Pressure Control Solenoid Control
3 | PU/WH | -- | TCC Clutch Solenoid Control
4 | WH | -- | Line Pressure Control Solenoid Control
5 | -- | -- | Not Used
6 | WH | -- | Shift Solenoid 4 Supply Voltage
7 | YE | -- | Shift Solenoid 2 Supply Voltage
8 | BN/WH | -- | Transmission Fluid Temperature Sensor Signal
9 | PK/BK | -- | Shift Pressure Control Solenoid Supply Voltage
10 | GN | -- | TCC Clutch Solenoid Supply Voltage
11 | BU | -- | Line Pressure Control
12 | OG/WH | -- | Shift Solenoid 5 Supply Voltage
13 | WH | -- | Shift Solenoid 3 Supply Voltage
14 | L-GN | -- | Shift Solenoid 1 Supply Voltage

### Automatic Transmission (MH7/MH8)

#### Connector Part Information

- OEM: PE130755
- Service: N/A
- Description: 14-Way F GT 150 280 Series, Sealed (L-GY)

#### Automatic Transmission (MH7/MH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | 440 | Battery Positive Voltage
2 | BK | 250 | Ground
3 | OG/BK | 1786 | Transmission Park/Neutral Signal
4 | BN | 2501 | High Speed GMLAN Serial Data (-) (MH7)
WH | 2501 | High Speed GMLAN Serial Data (-) (MH8)
5 | BN/BK | 2500 | High Speed GMLAN Serial Data (+) (MH7)
YE | 2500 | High Speed GMLAN Serial Data (+) (MH8)
6 | BN/WH | 2500 | High Speed GMLAN Serial Data (+)
7 | BN/WH | 2500 | High Speed GMLAN Serial Data (+)
8 | L-GN | 2501 | High Speed GMLAN Serial Data (-) (MH7)
BN | 2501 | High Speed GMLAN Serial Data (-) (MH8)
9 | -- | -- | Not Used
10 | L-BU | 20 | Stop Lamp Supply Voltage
11 | -- | -- | Not Used
12 | PK/BK | 539 | Ignition 1 Voltage
13 | PK/BK | 539 | Ignition 1 Voltage
14 | L-GN | 2501 | High Speed GMLAN Serial Data (-) (MH7)
BN | 2501 | High Speed GMLAN Serial Data (-) (MH8)

### Automatic Transmission Control Indicator (MH7/MH8)

#### Connector Part Information

- OEM: PH845-09020
- Service: N/A
- Description: 9-Way F CDR09F Series (BK)

#### Automatic Transmission Control Indicator (MH7/MH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 1027 | Winter Mode Switch Signal
2 | -- | -- | Not Used
3 | BN/WH | 309 | Instrument Panel Lamps Supply Voltage
4 | GY | 773 | Transmission Position M Indicator Control
5 | D-BU/WH | 774 | Transmission Position D Indicator Control
6 | GY/BK | 773 | Transmission Position N Indicator Control
7 | L-GN | 775 | Transmission Position R Indicator Control
8 | WH/BK | 711 | Transmission Position P Indicator Control
9 | BK | 250 | Ground

### Automatic Transmission Shift Lever (M98)

#### Connector Part Information

- OEM: 7223-6508-30
- Service: N/A
- Description: 10-Way F DMS+RV Series, Sealed (BK)

#### Automatic Transmission Shift Lever (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BN | -- | A/T Shift Lock Solenoid Control
3 | BK | -- | Ground
4 | L-GN | -- | Park Position Signal
5 | -- | -- | Not Used
6 | BK | -- | Ground
7 | BN | -- | Tap Down Signal
8 | PU | -- | Tap Up Signal
9 | BN | -- | Driver Shift Control
10 | PK | -- | Ignition 1 Voltage

### Auxiliary Power Outlet

#### Connector Part Information

- OEM: MG630685-5
- Service: N/A
- Description: 2-Way F 2505 Series (BK)

#### Auxiliary Power Outlet

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Accessory Voltage
2 | BK/WH | -- | Ground

### Backup Lamp - Left

#### Connector Part Information

- OEM: 174463-1
- Service: N/A
- Description: 2-Way M 070 Multilock Series (WH)

#### Backup Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-GN | -- | Backup Lamp Supply Voltage

### Backup Lamp - Right

#### Connector Part Information

- OEM: 174463-1
- Service: N/A
- Description: 2-Way M 070 Multilock Series (WH)

#### Backup Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-GN | -- | Backup Lamp Supply Voltage

### Backup Lamp Switch (MFB/MFN)

#### Connector Part Information

- OEM: AK07207
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Backup Lamp Switch (MFB/MFN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-GN | -- | Backup Lamp Supply Voltage

### Blower Motor

#### Connector Part Information

- OEM: MG610281
- Service: N/A
- Description: 2-Way F .312 Series (NA)

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Blower Motor Speed Signal (C68)
BK | -- | Ground (C60/C66)
2 | YE | -- | Blower Motor Supply Voltage (C68)
RD | -- | Blower Motor Supply Voltage (C60/C66)

### Blower Motor Resistor (C60/C66)

#### Connector Part Information

- OEM: MG610047
- Service: N/A
- Description: 4-Way F 250 Series (NA)

#### Blower Motor Resistor (C60/C66)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | Blower Motor Speed Signal
2 | PK | -- | Blower Motor Speed Signal
3 | RD | -- | Blower Motor Supply Voltage
4 | D-BU | -- | Blower Motor Speed Signal

### Blower Motor Switch (C60/C66)

#### Connector Part Information

- OEM: MG610049
- Service: N/A
- Description: 6-Way F 250 Series (NA)

#### Blower Motor Switch (C60/C66)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Blower Relay Supply Voltage
2 | WH/RD | -- | Blower Switch Signal
3 | WH | -- | Blower Motor Speed Signal
4 | D-BU | -- | Blower Motor Speed Signal
5 | PK | -- | Blower Motor Speed Signal
6 | RD | -- | Blower Motor Speed Signal

### Body Control Module X1

#### Connector Part Information

- OEM: 98625-2001
- Service: N/A
- Description: 15-Way F HDX Series (GY)

#### Body Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | D-BU | 164 | Power Window Switch Driver Up Signal
4 | OG/BK | 737 | Rear Compartment Lid Ajar Switch Signal
5 | L-BU | 195 | Door Lock Signal
6 | WH | 194 | Door unlock Signal
7 | D-GN/BK | 2905 | Serial Data
8 | BN | 126 | Left Front Door Open Switch Signal
9 | WH | 156 | Courtesy Lamp Control
10 | OG | 2764 | Power Window Switch Drivers Express Down Signal
11 | BN | 41 | Ignition 2 Voltage
12 | BN | 165 | Driver Window Switch Driver Down Signal
13 | PK/D-BU | 638 | Power Window Motor Driver Down Control
14 | -- | -- | Not Used
15 | PK/BK | 109 | Hood Ajar Switch Signal

### Body Control Module X2

#### Connector Part Information

- OEM: 98631-2001
- Service: N/A
- Description: 30-Way F HDX Series (GY)

#### Body Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | 6985 | Windshield Wiper Switch Pulse Delay Signal
2 | BN/WH | 1434 | Immobilizer Signal
3 | L-GN | 1435 | Immobilizer Signal
4-5 | -- | -- | Not Used
6 | L-GN | 1845 | Chime Signal
7 | OG | 1000 | Crash Signal
8-11 | -- | -- | Not Used
12 | D-GN/WH | 817 | Vehicle Speed Signal
13 | D-BU/WH | 1315 | Right Front Turn Signal Lamp
14 | L-BU/WH | 1314 | Left Front Turn Supply Voltage
15 | WH | 193 | Rear Defog Relay Control
16-17 | -- | -- | Not Used
18 | PU | 1697 | Turn/Hazard Module Signal
19 | WH/BK | 5043 | Serial Data
20 | YE | 749 | Security Indicator Control
21 | -- | -- | Not Used
22 | YE/BK | 1436 | Immobilizer Signal
23 | L-GN | 80 | Key Ignition Switch Signal
24 | -- | -- | Not Used
25 | OG | 228 | Windshield Washer Pump Control
26 | BK/WH | 351 | Immobilizer Signal
27 | -- | -- | Not Used
28 | BN | 96 | Windshield Wiper Switch Pulse Delay Signal
29 | -- | -- | Not Used
30 | L-BU | 263 | Rear Compartment Lid Ajar Switch Signal

### Body Control Module X3

#### Connector Part Information

- OEM: 211 PC 122S0017
- Service: N/A
- Description: 12-Way F (BK)

#### Body Control Module X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 96 | Windshield Wiper Switch Pulse Delay Signal
2 | D-BU | -- | Interior Lamps Control
3 | L-BU | 97 | Windshield Wiper Switch MIST/OFF/LOW Signal
4 | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
5 | -- | -- | Not Used
6 | BN/WH | -- | Power Window Switch Drivers Express Up Signal
7 | -- | -- | Not Used
8 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
9 | -- | -- | Not Used
10 | RD/BK | -- | Power Window Switch Drivers Express Down Signal
11 | BN | 253 | Trunk Release Relay Control
12 | YE | 261 | Siren Control

### Body Control Module X4

#### Connector Part Information

- OEM: 211 PC 083S0017
- Service: N/A
- Description: 8-Way F 2.8 Series (BK)

#### Body Control Module X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 750 | Ground
2 | -- | -- | Not Used
3 | PK | 639 | Ignition 1 Voltage
4 | BK | 750 | Ground
5 | BN | 294 | Door Lock Actuator Unlock Control
6 | GY | 295 | Door Lock Actuator Lock Control
7 | PU | 1293 | Rear Defog Element Supply Voltage
8 | PU | 1293 | Rear Defog Element Supply Voltage

### Body Control Module X5

#### Connector Part Information

- OEM: UTA 321600157
- Service: N/A
- Description: BK

#### Body Control Module X5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | 142 | Battery Positive Voltage

### Boost Pressure Actuator (LLW)

#### Connector Part Information

- OEM: 368162-1
- Service: N/A
- Description: 4-Way F JPT Series Sealed (BK)

#### Boost Pressure Actuator (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Battery Positive Voltage
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | PU | -- | Boost Pressure Actuator Control

### Boost Pressure Sensor (LLW)

#### Connector Part Information

- OEM: 368162-1
- Service: N/A
- Description: 4-Way F JPT Series Sealed (BK)

#### Boost Pressure Sensor (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BU | -- | Ground
2 | L-GN | -- | Intake Air Temperature Signal
3 | WH/BK | -- | 5-Volt Reference
4 | GY/BK | -- | Intake Air Pressure Signal

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: MG610320
- Service: N/A
- Description: 2-Way F SWP Series (NA)

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Brake Warning Indicator Control
2 | BK | -- | Ground

### Camshaft Position (CMP) Sensor

#### Connector Part Information

- OEM: 85205-1
- Service: N/A
- Description: 3-Way F JPT Series (BK)

#### Camshaft Position (CMP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Camshaft Position (CMP) Sensor Signal (LBK/LBML)
L-GN/BK | -- | Camshaft Position (CMP) Sensor Signal (LLW)
2 | PK/BK | -- | Low Reference (LBK/LBM)
D-BU/WH | -- | Ground (LLW)
3 | PK | -- | Ignition 1 Voltage (LBK/LBM)
PK/WH | -- | Battery Positive Voltage (LLW)

### CAN Test Connector (MH7/MH8)

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP02F-B Series (BK)

#### CAN Test Connector (MH7/MH8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 2500 | High Speed GMLAN Serial Data (+) (MH7)
YE | 2500 | High Speed GMLAN Serial Data (+) (MH8)
2 | L-GN | 2501 | High Speed GMLAN Serial Data (-) (MH7)
WH | 2501 | High Speed GMLAN Serial Data (-) (MH8)

### Center Dome Lamp

#### Connector Part Information

- OEM: 368500-1
- Service: N/A
- Description: 3-Way F 070 MLC Series (NA)

#### Center Dome Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Inadvertent Lamp Control
2 | OG | -- | Courtesy Lamp Control
3 | BK | -- | Ground

### Center High Mounted Stop Lamp (CHMSL)

#### Connector Part Information

- OEM: MG610392
- Service: N/A
- Description: 2-Way F SDL Series (WH)

#### Center High Mounted Stop Lamp (CHMSL)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Stop lamp Supply Voltage/Stop Lamp Switch Signal
2 | BK | -- | Ground

### Cigar Lighter

#### Connector Part Information

- OEM: 368021-1
- Service: N/A
- Description: WH

#### Cigar Lighter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | YE | -- | Accessory Voltage

### Clock

#### Connector Part Information

- OEM: MG651439
- Service: N/A
- Description: 6-Way

#### Clock

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | -- | Ground
3 | BN/WH | -- | Park Lamp Supply Voltage
4 | YE | -- | Accessory Voltage
5 | RD/WH | -- | Battery Voltage
6 | -- | -- | Not Used

### Clutch Switch (LBM/LBK w/MFB/MFN)

#### Connector Part Information

- OEM: PE107545
- Service: N/A
- Description: 4-Way F Micro 100 Series (BK)

#### Clutch Switch (LBM/LBK w/MFB/MFN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | YE | -- | Clutch Switch Signal
4 | BK | -- | Ground

### Cooling Fan - Auxiliary

#### Connector Part Information

- OEM: 176146-1
- Service: N/A
- Description: 2-Way F 187 Series, Sealed (BK)

#### Cooling Fan - Auxiliary

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | Ground (Gasoline)
YE | -- | Cooling Fan Motor Supply Voltage (Diesel)
2 | L-BU | -- | Cooling Fan Motor Supply Voltage (Gasoline)
BK | -- | Ground (Diesel)

### Cooling Fan - Main

#### Connector Part Information

- OEM: 176146-1
- Service: N/A
- Description: 2-Way F 187 Series, Sealed (BK)

#### Cooling Fan - Main

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | GY | -- | Cooling Fan Motor Supply Voltage

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: 85205-1
- Service: N/A
- Description: 3-Way F JPT Series (BK)

#### Crankshaft Position (CKP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | -- | Crankshaft Position (CKP) Sensor Signal (LBM/LBK)
D-BU/WH | -- | Crankshaft Position (CKP) Sensor Signal (LLW)
2 | D-BU/WH | -- | Low Reference (LBM/LBK)
YE/BK | -- | Low Reference (LLW)
3 | BN/WH | -- | Ground (LBM/LBK)
GY | -- | Ground (LLW)

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: MG610761
- Service: N/A
- Description: BK

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | D-BU/WH | 555 | Serial Data
4 | BK | 1250 | Ground
5 | BK/WH | 251 | Ground
6 | BN/WH | 2500 | Serial Data (LHD)
BN/BK | 2500 | Serial Data (RHD)
7 | WH/BK | 5043 | Serial Data
8-13 | -- | -- | Not Used
14 | BN | 2501 | Serial Data
15 | -- | -- | Not Used
16 | RD/WH | 1840 | Battery Positive Voltage

### Diesel Particulate Filter Pressure Sensor (LLW)

#### Connector Part Information

- OEM: 1J0973703
- Service: N/A
- Description: 3-Way F Micro Timer II Series Sealed (BK)

#### Diesel Particulate Filter Pressure Sensor (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | 3044 | 5-Volt Reference
2 | L-BU | 3037 | Low Reference
3 | YE/BK | 3064 | Signal

### Diode

#### Connector Part Information

- OEM: MG620102-5
- Service: N/A
- Description: 2-Way F DIODE Connector (BK)

#### Diode

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Lamp Control
2 | OG | -- | Ground

### Door Latch Switch - Driver

#### Connector Part Information

- OEM: PKI 15011 04F, PKI 832419
- Service: N/A
- Description: 4-Way F

#### Door Latch Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | All Contact Input
2 | GY | -- | Door Ajar Signal
3 | BN | -- | Driver Front Door Contact Input
4 | BK | -- | Ground

### Door Latch Switch - Left Rear

#### Connector Part Information

- OEM: PKI 15011 04F, PKI 832419
- Service: N/A
- Description: 4-Way F

#### Door Latch Switch - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | -- | All Contact Input
2 | -- | -- | Not Used
3 | BN | -- | Door Ajar Signal
4 | WH | -- | Courtesy Lamp Control

### Door Latch Switch - Passenger

#### Connector Part Information

- OEM: PKI 15011 04F, PKI 832419
- Service: N/A
- Description: 4-Way F

#### Door Latch Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | -- | -- | Not Used
3 | BN | -- | Door Ajar Signal
4 | WH | -- | All Contact Input

### Door Latch Switch - Right Rear

#### Connector Part Information

- OEM: PKI 15011 04F, PKI 832419
- Service: N/A
- Description: 4-Way F

#### Door Latch Switch - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | -- | -- | Not Used
3 | BN | -- | Door Ajar Signal
4 | WH | -- | All Contact Input

### Door Lock Actuator - Driver

#### Connector Part Information

- OEM: AK6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Door Lock Actuator Unlock Control
B | GY | -- | Door Lock Actuator Lock Control

### Door Lock Actuator - Left Rear

#### Connector Part Information

- OEM: AK6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Door Lock Actuator Unlock Control
B | GY | -- | Door Lock Actuator Lock Control

### Door Lock Actuator - Passenger

#### Connector Part Information

- OEM: AK6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Door Lock Actuator Unlock Control
B | GY | -- | Door Lock Actuator Lock Control

### Door Lock Actuator - Right Rear

#### Connector Part Information

- OEM: AK6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Door Lock Actuator - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Door Lock Actuator Unlock Control
B | GY | -- | Door Lock Actuator Lock Control

### Door Step Lamp - Driver

#### Connector Part Information

- OEM: MG610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series (WH)

#### Door Step Lamp - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Courtesy Lamp Control
2 | BK | -- | Ground

### Door Step Lamp - Passenger

#### Connector Part Information

- OEM: MG610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series (WH)

#### Door Step Lamp - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Courtesy Lamp Control
2 | BK | -- | Ground

### Door Tamper Switch - Driver

#### Connector Part Information

- OEM: 832421
- Service: N/A
- Description: 4-Way F

#### Door Tamper Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 263 | Tamper Switch Signal
B | WH | 194 | Door Unlock Control
C | BK | 50 | Ground
D | L-BU | 195 | Door Lock Control

### Door Tamper Switch - Passenger

#### Connector Part Information

- OEM: 832421
- Service: N/A
- Description: 4-Way F

#### Door Tamper Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | -- | Tamper Switch Signal (LHD)
B | BK | 750 | Ground
C | -- | -- | Not Used
D | L-BU | 263 | Tamper Switch Signal (RHD)

### Driver Information Center (DIC)

#### Connector Part Information

- OEM: 15394150
- Service: N/A
- Description: 16-Way F Micro-Pack 064 Series (BK)

#### Driver Information Center (DIC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | PK | -- | Ignition Voltage
4 | YE | -- | Accessory Voltage
5 | BN/WH | -- | Park Lamp Supply Voltage
6 | YE | -- | Ignition Voltage (C68)
7 | BK | -- | Ground
8 | RD/WH | -- | Battery Voltage
9 | BN/WH | -- | Serial Data
10 | -- | -- | Not Used
11 | BN | -- | Engine Running Signal
12-13 | -- | -- | Not Used
14 | OG | -- | Fuel Consumption Data
15 | D-GN/WH | -- | VSS Output
16 | OG | -- | Fuel Gage Signal (LBM/LBK)
D-BU | -- | Fuel Gage Signal (LLW)

### Electronic Brake Control Module (EBCM) (JL9/NW9)

#### Connector Part Information

- OEM: 368482-1
- Service: N/A
- Description: 25-Way F Micro-Pack 100W Series (BK)

#### Electronic Brake Control Module (EBCM) (JL9/NW9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Right Front Wheel Speed Sensor Signal
2 | D-BU/WH | -- | Right Front Wheel Speed Sensor Low Reference
3 | L-GN/BK | -- | Wheel Speed Signal-Left Front
4 | PK | -- | Ignition 1 Voltage
5 | BN | -- | Left Rear Wheel Speed Sensor Signal
6 | D-BU | -- | Left Rear Wheel Speed Sensor Low Reference
7 | WH/BK | -- | Serial Data
8 | BK | -- | Ground
9 | RD | -- | Battery Positive Voltage
10 | BN | -- | CAN Serial Data Low
11 | BN/BK | -- | CAN Serial Data High
12 | GY/WH | -- | Traction Control Off Indicator Control
13 | -- | -- | Not Used
14 | L-BU | -- | Traction Control Switch Signal
15 | -- | -- | Not Used
16 | D-GN/BK | -- | ABS Indicator Signal
17 | PU | -- | Traction Control Indicator Control
18 | L-BU | -- | Stop Lamp Switch Signal
19 | BN | -- | Right Front Wheel Speed Sensor Signal
20 | D-BU | -- | Left Front Wheel Speed Sensor Low Reference
21 | D-GN | -- | Traction Control Active Indicator Control
22 | D-BU/BK | -- | Right Rear Wheel Speed Sensor Low Reference
23 | BN/WH | -- | Right Rear Wheel Speed Sensor Signal
BN/BK | -- | Right Rear Wheel Speed Sensor Signal (Holden, Euro/Gen, Diesel)
24 | BK | -- | Ground
25 | RD | -- | Battery Positive Voltage

### Electronic Brake Control Module (EBCM) (F45)

#### Connector Part Information

- OEM: 1897088-2
- Service: N/A
- Description: 47-Way F060/187 Series (BK)

#### Electronic Brake Control Module (EBCM) (F45)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | 42 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | D-GN | 1656 | Electronic Stability Active Indicator Control
4-5 | -- | -- | Not Used
6 | L-BU | 20 | Stop Lamp Supply Voltage
7 | -- | -- | Not Used
8 | PK | 1339 | Ignition 1 Voltage
9 | -- | -- | Not Used
10 | WH/BK | 5043 | Serial Data
11 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
12 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
13 | BN | 2501 | High Speed GMLAN Serial Data (-)
14 | BN | 2501 | High Speed GMLAN Serial Data (-)
15 | -- | -- | Not Used
16 | BK | 50 | Ground
17 | -- | -- | Not Used
18 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
19 | BN | 2501 | High Speed GMLAN Serial Data (-)
20-21 | -- | -- | Not Used
22 | PK | 839 | 12V Reference
23-28 | -- | -- | Not Used
29 | BK | 650 | Ground
30 | -- | -- | Not Used
31 | D-GN/BK | 1867 | ABS Warning Lamp Indicator Control
32 | OG/BK | 740 | Battery Positive Voltage
33 | D-BU/WH | 873 | Right Front Wheel Speed Sensor Low Reference
34 | BN/WH | 833 | Right Front Wheel Speed Sensor Signal
35 | PU | 1681 | Traction Control System Passive Indicator Control
36 | BN | 884 | Wheel Speed Sensor Signal Left Rear
37 | D-BU | 885 | Wheel Speed Sensor Low Reference Left Rear
38 | L-BU | 6844 | Electronic Stability Control Switch Signal
39-41 | -- | -- | Not Used
42 | D-BU/BK | 883 | Wheel Speed Sensor Low Reference Right Rear
43 | BN/BK | 882 | Wheel Speed Sensor Signal Right Rear
44 | -- | -- | Not Used
45 | BN | 830 | Wheel Speed Sensor Signal Left Front
46 | D-BU | 872 | Left Front Wheel Speed Sensor Signal Right Front Low Reference
47 | BK | 150 | Motor Ground

### Electronic Brake Control Module (EBCM) (JL9/NW9-F45)

#### Connector Part Information

- OEM: 1897077-1
- Service: N/A
- Description: 26-Way F 060/187 Series (BK)

#### Electronic Brake Control Module (EBCM) (JL9/NW9-F45)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | 740 | Battery Positive Voltage
2 | D-BU | 885 | Wheel Speed Sensor Low Reference Left Rear
3 | BN | 884 | Wheel Speed Sensor Signal Left Rear
4 | D-GN/BK | 1867 | ABS Warning Lamp Indicator Control
5 | BN/WH | 833 | Wheel Speed Sensor Signal Right Front
6 | D-BU/WH | 873 | Right Front Wheel Speed Sensor Low Reference
7 | -- | -- | Not Used
8 | D-BU | 872 | Left Front Wheel Speed Sensor Low Reference
9 | BN | 830 | Wheel Speed Sensor Signal Left Front
10 | -- | -- | Not Used
11 | BN/BK | 882 | Wheel Speed Sensor Signal Right Rear
12 | D-BU/BK | 883 | Wheel Speed Sensor Low Reference Right Rear
13 | BK | 50 | Ground
14 | RD | 42 | Battery Positive Voltage
15 | -- | -- | Not Used
16 | L-BU | 20 | Stop Lamp Supply Voltage
17 | -- | -- | Not Used
18 | WH/BK | 5043 | Serial Data
19 | -- | -- | Not Used
20 | PK | 1339 | Ignition 1 Voltage
21 | BN | 2501 | High Speed GMLAN Serial Data (-)
22 | BN | 2501 | High Speed GMLAN Serial Data (-)
23 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
24 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
25 | PU | 1681 | Traction Control Warning Indicator Lamp Control
26 | BK | 150 | Motor Ground

### Electronic Stability Control Switch (F45)

#### Connector Part Information

- OEM: MG652999
- Service: N/A
- Description: 4-Way F 040 III Series (NA)

#### Electronic Stability Control Switch (F45)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | L-BU | 6844 | ESC Switch Signal
3 | BN/WH | 309 | Instrument Panel Lamps Supply Voltage
4 | D-GN | 44 | Instrument Panel Lamp Dimmer Switch Signal

### Engine Control Module (ECM) X1

#### Connector Part Information

- OEM: 2-1355123-3
- Service: N/A
- Description: 60-Way F 064 MQS Series Sealed (WH)

#### Engine Control Module (ECM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Ignition Coil 6 Control (LBK/LBM)
L-BU | -- | Fuel injector 3 High (LLW)
2 | OG | -- | Ignition Coil 2 Control (LBK/LBM)
L-GN | -- | Fuel Injector 2 High (LLW)
3 | D-BU | -- | Ignition Coil 4 Control (LBK/LBM)
4 | BN/WH | -- | Fuel Rail Pressure Regulator Supply Voltage (LLW)
5 | L-GN/WH | -- | HO2S1 Bank 2 Sensor 1 Heater Control (LBK/LBM)
6 | PU | -- | HO2S1 Bank 2 Sensor 1 Signal (LBK/LBM)
GY | -- | Cruise Switch Ground (LLW)
7 | D-GN | -- | Low Reference (LBK/LBM)
GY | -- | CKP Ground (LLW)
8 | BN | -- | HO2S2 Bank 2 Sensor 2 Signal (LBK/LBM)
D-GN/WH | -- | Fuel Rail Pressure Sensor Ground (LLW)
9 | GY | -- | EGR Position Sensor Signal (LBK/LBM)
10 | -- | -- | Not Used
11 | BN | -- | Low Reference (LBK/LBM)
12 | D-BU | -- | Low Reference (LBK/LBM)
YE/BK | -- | CKP Low Reference (LLW)
13 | BN | -- | Low Reference (LBK/LBM)
WH/BK | -- | 5-Volt Reference (LLW)
14 | L-GN | -- | MAP Sensor Signal (LBK/LBM)
15 | PU/WH | -- | Boost Pressure Actuator Control (LLW)
16 | PU | -- | EVAP Canister Vent Solenoid Valve Control (LBK/LBM)
YE/BK | -- | Fuel Injector 1 High (LLW)
17 | D-GN/WH | -- | EVAP Canister Purge Solenoid Valve Control (LBK/LBM)
D-GN | -- | Fuel Injector 4 High (LLW)
18 | -- | -- | Not Used
19 | L-GN | -- | HO2S Bank 2 Sensor 2 Heater Control (LBK/LBM)
PU/WH | -- | High Pressure Pump Supply Voltage (LLW)
20 | D-BU/WH | -- | CMP Ground (LLW)
21-22 | -- | -- | Not Used
23 | YE/D-BU | -- | Ground (LLW)
24-25 | -- | -- | Not Used
26 | D-GN | -- | Cooling Fan Low Relay Control (LBK/LBM)
27 | D-BU/WH | -- | CKP High (LLW)
28 | WH | -- | Engine RPM Signal (LBK/LBM)
L-BU | -- | Fuel Rail Pressure Sensor 5-Volt Reference (LLW)
29-30 | -- | -- | Not Used
31 | PU | -- | Ignition Coil 1 Control (LBK/LBM)
PU | -- | Fuel Injector 2 Low (LLW)
32 | D-GN | -- | Ignition Coil 5 Control (LBK/LBM)
33 | YE | -- | Ignition Coil 3 Control (LBK/LBM)
BN | -- | Fuel Injector 4 Low (LLW)
34 | BK | -- | Shield Ground (LBK/LBM)
L-BU/BK | -- | Fuel Rail Pressure Regulator Control (LLW)
35-36 | -- | -- | Not Used
37 | D-BU/WH | -- | IAT Signal (LLW)
OG | -- | Fuel Consumption Signal (LBK/LBM)
38 | BN/WH | -- | Low Reference (LBK/LBM)
39 | D-BU/WH | -- | Fuel Level Sensor Signal (LBK/LBM)
40 | PU | -- | Low Reference (LBK/LBM)
GY/BK | -- | Boost Pressure Actuator Intake Air Pressure Signal (LLW)
41 | -- | -- | Not Used
42 | PU/WH | -- | MAF Signal (LLW)
43 | GY/BK | -- | Fuel Rail Pressure Sensor Signal (LLW)
44 | YE/BK | -- | IAT, MAF Ground (LLW)
45 | WH | -- | Cruise Indicator Control (LLW)
46 | GY | -- | EGR Solenoid Control (LBK/LBM)
BN/WH | -- | Fuel Injector 3 Low (LLW)
47 | WH/BK | -- | Intake Manifold Tuning (IMT) Valve Solenoid Control (LBK/LBM)
WH | -- | Fuel Injector 1 Low (LLW)
48 | -- | -- | Not Used
49 | D-GN | -- | High Pressure Pump Control (LLW)
50 | L-GN/BK | -- | CMP Signal (LLW)
51 | D-BU | -- | Cooling Fan Hi Relay Control (LBK/LBM)
52 | GY/BK | -- | Throttle Plate Actuator Feedback Signal (LLW)
53 | WH | -- | Cruise Indicator Control (LBK/LBM)
L-GN | -- | Boost Pressure Actuator IAT Signal (LLW)
54 | L-BU | -- | APP Sensor 2 Signal (LBK/LBM)
55 | BN | -- | Low Reference (LBK/LBM)
56 | D-BU | -- | APP Sensor 1 Signal (LBK/LBM)
L-BU/BK | -- | Cruise Switch (LLW)
57 | PU | -- | TP Sensor 2 Signal (LBK/LBM)
58 | BK | -- | Low Reference (LBK/LBM)
59 | D-BU | -- | TP Sensor 1 Signal (LBK/LBM)
WH/BK | -- | Throttle Plate Actuator Control (LLW)
60 | D-GN/WH | -- | EGR Control (LLW)

### Engine Control Module (ECM) X2

#### Connector Part Information

- OEM: 3-1355136-3
- Service: N/A
- Description: 94-Way F MQS 1.5/2.8 MCP Series, Sealed (BK)

#### Engine Control Module (ECM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground (LBK/LBM)
PK/BK | -- | Battery Positive Voltage (LLW)
2 | PK | -- | Ignition 1 Voltage (LBK/LBM)
BK | -- | Ground (LLW)
3 | BK | -- | Ground (LBK/LBM)
PK/BK | -- | Battery Positive Voltage (LLW)
4 | PK | -- | Ignition 1 Voltage (LBK/LBM)
BK | -- | Ground (LLW)
5 | BK | -- | Ground (LBK/LBM)
PK | -- | Battery Positive Voltage (LLW)
6 | RD/WH | -- | Battery Positive Voltage (LBK/LBM)
BK | -- | Ground (LLW)
7 | -- | -- | Not Used
8 | PU | -- | APP Sensor Low Reference (2) (LLW)
9 | D-BU/WH | -- | Low Reference (LBK/LBM)
D-BU | -- | APP Sensor Signal (1) (LLW)
10 | D-GN/WH | -- | HO2S2 Bank 1 Sensor 2 Signal (LBK/LBM)
YE/BK | -- | Fuel Temperature Sensor Ground (LLW)
11 | PU/WH | -- | HO2S2 Bank 1 Sensor 1 Signal (LBK/LBM)
L-GN/BK | -- | Fuel Temperature Signal (LLW)
12 | D-GN/WH | -- | Low Reference (LBK/LBM)
BK/WH | -- | Ground (LLW)
13 | PU/WH | -- | Knock Sensor 1 Signal (LBK/LBM)
OG/BK | -- | A/C Refrigerant Pressure Sensor Signal (LLW)
14 | YE/BK | -- | Knock Sensor 1 Ground (LBK/LBM)
15 | L-GN/BK | -- | Rough Road Sensor Signal (LBK/LBM)
16 | GY | -- | Cruise Switch Ground (LBK/LBM)
17 | D-GN/WH | -- | A/C Request Signal (LBK/LBM)
L-BU | -- | Stop Lamp Switch Signal (LLW)
18 | GY/BK | -- | ECT Ground (LLW)
19 | BK | -- | Low Reference (LBK/LBM)
BN | -- | Generator Voltage Signal (LLW)
20 | YE | -- | Intake Manifold Tuning (IMT) Valve Sensor Signal (LLW)
D-GN/WH | -- | Fuel Pump Relay Control (LLW)
21 | D-BU/WH | -- | Knock Sensor 2 Signal (LBK/LBM)
D-BU | -- | Change Oil Soon Indicator Control (LLW)
22 | YE/BK | -- | Knock Sensor 2 Ground (LBK/LBM)
BN/WH | -- | 5-Volt Reference (LLW)
23 | GY | -- | 5-Volt Reference 3 (LBK/LBM)
24 | WH/BK | -- | 5-Volt Reference 3 (LBK/LBM)
25 | -- | -- | Not Used
26 | D-GN | 135 | ECT Signal (LLW)
27 | -- | -- | Not Used
28 | PK/BK | -- | Ignition 1 Voltage (LLW)
29 | PU/WH | -- | A/C Compressor Control (LLW)
30 | GY/BK | -- | Low Reference (LBK/LBM)
BN | -- | APP Sensor Low Reference (1) (LLW)
31 | YE | -- | MAF Sensor Signal (LBK/LBM)
L-BU | -- | APP Sensor Signal (2) (LLW)
32 | PK/BK | -- | CMP Sensor Ground (LBK/LBM)
L-BU/BK | -- | Exhaust Gas Temperature Sensor Signal 2 (LLW)
33 | BN/WH | -- | CMP Sensor Signal (LBK/LBM)
YE/WH | -- | Exhaust Gas Temperature Sensor 2 Ground (LLW)
34 | BK | -- | Low Reference (LBK/LBM)
PU/WH | -- | Exhaust Gas Temperature Sensor Signal 1 (LLW)
35 | D-GN | -- | FTP Sensor Signal (LBK/LBM)
D-BU/WH | -- | Exhaust Gas Temperature Sensor 1 Ground (LLW)
36 | -- | -- | Not Used
37 | BN | -- | Low Reference (LBK/LBM)
L-BU | -- | Diesel Particulate Filter Pressure Sensor Ground (LLW)
38 | D-GN/WH | 817 | Vehicle Speed Signal (LBK/LBM w/MFB/MFN)
39 | L-GN/BK | -- | Ground (LBK/LBM)
40 | L-BU/BK | -- | Cruise Switch Positive (LBK/LBM)
41 | OG/BK | -- | Refrigerant Pressure Signal (LBK/LBM)
42 | BN | -- | Ground (RHD LBK/LBM)
GY | -- | Ground (LHD LBK/LBM)
43 | -- | -- | Not Used
44 | PU/WH | -- | Diesel Particulate Filter Pressure Sensor 5-Volt Reference (LLW)
45 | WH/BK | -- | APP Sensor 5-Volt Reference (1) (LLW)
46 | D-GN | -- | APP Sensor 5-Volt Reference (2) (LLW)
47 | L-BU | -- | 5-Volt Reference (RHDLBK/LBM)
GY | -- | 5-Volt Reference (LHDLBK/LBM)
48 | OG/BK | -- | 5-Volt Reference 1 (LBK/LBM)
WH | -- | Engine Speed Signal (LLW)
49 | D-GN | -- | 5-Volt Reference 3 (LBK/LBM)
BN | -- | Charge Indicator Control (LLW)
50 | YE | -- | Clutch Switch Signal (Holden)
51 | -- | -- | Not Used
52 | L-GN/BK | -- | Glow Plug Diagnosis (LLW)
53 | PU | -- | Stop Lamp Switch Signal (LBK/LBM)
54 | BN | -- | Brake Pedal Switch Signal (LLW)
55 | YE/BK | -- | CKP Sensor Reference High (LBK/LBM)
56 | D-BU/WH | -- | CKP Sensor Reference Low (LBK/LBM)
57 | BN/WH | -- | CKP Sensor Ground (LBK/LBM)
WH/BK | -- | PTC Request Signal (LLW)
58 | L-BU | -- | Intake Air Temperature (IAT) Sensor Signal (LBK/LBM)
59 | YE/BK | -- | Low Reference (LBK/LBM)
60-61 | -- | -- | Not Used
62 | YE | -- | ECT Sensor Signal (LBK/LBM)
63 | -- | -- | Not Used
64 | BN | -- | Engine Main Relay Control (LBK/LBM)
YE/BK | -- | Diesel Particulate Filter Pressure Sensor Signal (LLW)
65 | -- | -- | Not Used
66 | L-BU/BK | -- | Fuel Injector 4 Control (LBK/LBM)
BN | -- | ECT Signal (LLW)
67 | L-GN/BK | -- | Fuel Injector 2 Control (LBK/LBM)
GY/BK | -- | ECT Indicator Control (LLW)
68 | YE/BK | -- | Fuel Injector 6 Control (LBK/LBM)
D-BU | -- | Fuel Heater Relay Control (LLW)
69 | D-GN | -- | Cooling Fan Low Speed Relay Control (LLW)
70 | D-GN/WH | -- | Fuel Pump Relay Control (LBK/LBM)
YE | -- | Diesel Particulate Filter Indicator Control (LLW)
71 | D-BU | -- | TAC Motor Control 1 (LBK/LBM)
PU/WH | -- | MIL Control (LLW)
72 | L-BU | -- | TAC Motor Control 2 (LBK/LBM)
GY/BK | -- | Engine Main Relay Coil Control (LLW)
73-74 | -- | -- | Not Used
75 | D-BU | -- | Generator Field Duty Cycle Signal (LLW)
76 | WH/BK | -- | Serial Data (LBK/LBM)
77 | BN/WH | -- | CAN Serial Data High (LBK/LBM)
78 | BN | -- | CAN Serial Data Low (LBK/LBM)
79 | D-GN/WH | -- | A/C Request Signal (LLW)
80 | YE | -- | Clutch Switch Signal (Except Holden)
81-82 | -- | -- | Not Used
83 | L-BU | -- | Stop Lamp Switch Signal (LBK/LBM)
L-GN | -- | CAN Low (LLW)
84 | BN/WH | -- | CAN High (LLW)
85 | -- | -- | Not Used
86 | D-GN | -- | Engine Temperature Gage Output (LBK/LBM)
87 | PU/WH | -- | A/C Compressor Control (LBK/LBM)
88 | YE | -- | Fuel Gage Signal (LBK/LBM)
WH | -- | Cooling Fan Control Relay Control (LLW)
89 | BN | -- | Fuel Injector 1 Control (LBK/LBM)
90 | BN/WH | -- | Fuel Injector 5 Control (LBK/LBM)
D-BU | 473 | Cooling Fan High Speed Relay Control (LLW)
91 | PK/BK | -- | Fuel Injector 3 Control (LBK/LBM)
L-GN/WH | -- | PTC Relay 2, 3 Control (LLW)
92 | D-BU | -- | MIL Control (LBK/LBM)
L-BU | -- | Glow Plug Indicator Control (LLW)
93 | GY | -- | HO2S1 Bank 1 Sensor 1 Heater Control (LBK/LBM)
WH | -- | Glow Plug Control (LLW)
94 | GY/WH | -- | HO2S2 Bank 1 Heater Control (LBK/LBM)
YE | -- | PTC Relay Control (LLW)

### Engine Coolant Temperature (ECT) Sensor (LBK/LBM)

#### Connector Part Information

- OEM: AK0442
- Service: N/A
- Description: 2-Way Connector F (BK)

#### Engine Coolant Temperature (ECT) Sensor (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Engine Coolant Temperature (ECT) Sensor Signal
2 | BK/WH | -- | Ground

### Engine Coolant Temperature (ECT) Sensor (LLW)

#### Connector Part Information

- OEM: 12040753
- Service: N/A
- Description: 2-Way F 150 Series Sealed

#### Engine Coolant Temperature (ECT) Sensor (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Engine Coolant Temperature (ECT) Sensor Signal
B | GY/BK | -- | Ground

### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LBK/LBM)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series (BK)

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | D-GN/WH | -- | EVAP Canister Purge Valve Solenoid Control

### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LBK/LBM)

#### Connector Part Information

- OEM: AK32229
- Service: N/A
- Description: 2-Way F (BN)

#### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | EVAP Canister Vent Solenoid Control
2 | PK/BK | -- | Ignition 1 Voltage

### Exhaust Gas Recirculation (EGR) Valve (LBK/LBM)

#### Connector Part Information

- OEM: 12129946
- Service: N/A
- Description: 5-Way F Metri-Pack 150 Series Sealed (GY)

#### Exhaust Gas Recirculation (EGR) Valve (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | GY | -- | Exhaust Gas Recirculation (EGR) Solenoid Control
B | BN | -- | Low Reference
C | GY | -- | Exhaust Gas Recirculation (EGR) Valve Position Sensor Signal
D | OG/BK | -- | 5-Volt Reference
E | PK | -- | Ignition 1 Voltage

### Exhaust Gas Recirculation (EGR) Valve (LLW)

#### Connector Part Information

- OEM: 827551-3
- Service: N/A
- Description: 2-Way F Timer Sealed

#### Exhaust Gas Recirculation (EGR) Valve (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/WH | -- | Battery Positive Voltage
2 | D-GN/WH | -- | EGR Solenoid Control

### Exhaust Gas Temperature Sensor 1 (LLW)

#### Connector Part Information

- OEM: 621-02020
- Service: N/A
- Description: 2-Way M Sealed (BK)

#### Exhaust Gas Temperature Sensor 1 (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Signal
2 | BU/WH | -- | Ground

### Exhaust Gas Temperature Sensor 2 (LLW)

#### Connector Part Information

- OEM: 621-02020
- Service: N/A
- Description: 2-Way M, Sealed (BK)

#### Exhaust Gas Temperature Sensor 2 (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Signal
2 | YE/WH | -- | Ground

### Fog Lamp - Left Front

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP 04F-B Series

#### Fog Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Front Fog Lamp Supply Voltage
2 | BK | -- | Ground

### Fog Lamp - Left Rear

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP 04F-B Series

#### Fog Lamp - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | OG | -- | Rear Fog Lamp Supply Voltage

### Fog Lamp - Right Front

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP 04F-B Series

#### Fog Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Front Fog Lamp Supply Voltage
2 | BK | -- | Ground

### Fog Lamp - Right Rear

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP 04F-B Series

#### Fog Lamp - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | OG | -- | Rear Fog Lamp Supply Voltage

### Front Defogger

#### Connector Part Information

- OEM: PB621-02020
- Service: N/A
- Description: 2-Way M Sealed (BK)

#### Front Defogger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | D-BU | 2293 | Front Defogger Supply Voltage

### Fuel Filter Heater/Temperature Sensor (LLW)

#### Connector Part Information

- OEM: 17260406A
- Service: N/A
- Description: 6-Way F 280 Series Sealed

#### Fuel Filter Heater/Temperature Sensor (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | BK | -- | Ground
4 | PU | -- | Fuel Filter Heater Supply Voltage
5 | L-GN/BK | -- | Fuel Temperature Signal
6 | YE/BK | -- | Fuel Temperature Ground

### Fuel Injector 1 (LBK/LBM)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series (BK)

#### Fuel Injector 1 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | BN | -- | Fuel Injector 1 Control

### Fuel Injector 1 (LLW)

#### Connector Part Information

- OEM: 1928403874
- Service: N/A
- Description: 2-Way F Kompakt 2.8 Series, Sealed (BK)

#### Fuel Injector 1 (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | -- | High
2 | WH | -- | Low

### Fuel Injector 2 (LBK/LBM)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series (BK)

#### Fuel Injector 2 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-GN/BK | -- | Fuel Injector 2 Control

### Fuel Injector 2 (LLW)

#### Connector Part Information

- OEM: 1928403874
- Service: N/A
- Description: 2-Way F Kompakt 2.8 Series, Sealed (BK)

#### Fuel Injector 2 (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | High
2 | BU | -- | Low

### Fuel Injector 3 (LBK/LBM)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series (BK)

#### Fuel Injector 3 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | PK/BK | -- | Fuel Injector 3 Control

### Fuel Injector 3 (LLW)

#### Connector Part Information

- OEM: 1928403874
- Service: N/A
- Description: 2-Way F Kompakt 2.8 Series, Sealed (BK)

#### Fuel Injector 3 (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | High
2 | BN/WH | -- | Low

### Fuel Injector 4 (LBK/LBM)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series (BK)

#### Fuel Injector 4 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-BU/BK | -- | Fuel Injector 4 Control

### Fuel Injector 4 (LLW)

#### Connector Part Information

- OEM: 1928403874
- Service: N/A
- Description: 2-Way F Kompakt 2.8 Series, Sealed (BK)

#### Fuel Injector 4 (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | High
2 | BN | -- | Low

### Fuel Injector 5 (LBK/LBM)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series (BK)

#### Fuel Injector 5 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | BN/WH | -- | Fuel Injector 5 Control

### Fuel Injector 6 (LBK/LBM)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series (BK)

#### Fuel Injector 6 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | YE/BK | -- | Fuel Injector 6 Control

### Fuel Pump (LBM/LBK)

#### Connector Part Information

- OEM: KAFUS B06009A
- Service: N/A
- Description: 6-Way F

#### Fuel Pump (LBM/LBK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Low Fuel Indicator Signal
2 | BK | -- | Ground
3 | GY | -- | Fuel Pump Supply Voltage
4 | PK | -- | Ignition 1 Voltage
5 | YE | -- | Fuel Level Sensor Signal
6 | BN | -- | Low Reference 2.5L
PU | -- | Low Reference 2.0L

### Fuel Pump Module (LLW)

#### Connector Part Information

- OEM: MG641521
- Service: N/A
- Description: 5-Way F 090-II Sealed

#### Fuel Pump Module (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | D-BU | -- | Fuel Sensor Signal
3 | PU | -- | Ground
4 | GY | -- | Fuel Pump Supply Voltage
5 | BK | -- | Ground

### Fuel Rail Pressure Control Valve (LLW)

#### Connector Part Information

- OEM: 1928403874
- Service: N/A
- Description: 2-Way F Kompakt 2.8 Series, Sealed (BK)

#### Fuel Rail Pressure Control Valve (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Low
2 | BN/WH | -- | Ground

### Fuel Rail Pressure Sensor (LLW)

#### Connector Part Information

- OEM: 1928403968
- Service: N/A
- Description: 2-Way F Kompakt 2.8 Series, Sealed (BK)

#### Fuel Rail Pressure Sensor (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | -- | Ground
2 | GY/BK | -- | Signal
3 | L-BU | -- | 5-Volt Reference

### Fuel Tank Pressure (FTP) Sensor (LBK/LBM)

#### Connector Part Information

- OEM: AK32311
- Service: N/A
- Description: 3-Way F (BK)

#### Fuel Tank Pressure (FTP) Sensor (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Low Reference
2 | D-GN | -- | Fuel Tank Pressure (FTP) Signal
3 | GY | -- | 5-Volt Reference

### Generator

#### Connector Part Information

- OEM: 12186568
- Service: N/A
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Generator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BN | -- | Charge Indicator Control/Charge Indicator Signal
C | PK | -- | Ignition 1 Voltage (LBK/LBM)
D-BU | -- | Generator Power Control (LLW)
D | -- | -- | Not Used

### Glow Plug Control Unit (LLW)

#### Connector Part Information

- OEM: 60432001
- Service: N/A
- Description: 11-Way F Mixed Series, Sealed (BK)

#### Glow Plug Control Unit (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Glow Plug Supply Voltage
2 | PU | -- | Glow Plug Supply Voltage
3 | PU | -- | Glow Plug Supply Voltage
4 | PU | -- | Glow Plug Supply Voltage
5 | -- | -- | Not Used
6 | PK/WH | -- | Ignition Voltage
7 | BK | -- | Ground
8 | -- | -- | Not Used
9 | L-GN/BK | -- | Diagnosis
10 | RD/WH | -- | Battery Positive Voltage
11 | WH | -- | Glow Plug Control

### Hazard Switch

#### Connector Part Information

- OEM: MG651056
- Service: N/A
- Description: 10-Way F 090-II Series (WH)

#### Hazard Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | GN | -- | Ground
3 | BN/WH | -- | Dimmer PWM Output
4-6 | -- | -- | Not Used
7 | BK | -- | Ground
8 | PU | -- | Hazard Switch Signal
9-10 | -- | -- | Not Used

### Headlamp - Left (TR6)

#### Connector Part Information

- OEM: PB625-06027
- Service: N/A
- Description: 6-Way F NMWP 06F-B Series, Sealed (BK)

#### Headlamp - Left (TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | PU | -- | Park Lamp Supply Voltage
3 | GN | -- | Headlamp Levelling
4 | GN/WH | -- | High Beam Supply Voltage
5 | YE | -- | Low Beam Supply Voltage
6 | BK | -- | Ground

### Headlamp - Left (-TR6)

#### Connector Part Information

- OEM: PB625-04027
- Service: N/A
- Description: 4-Way F NMWP 04F-B Series, Sealed (BK)

#### Headlamp - Left (-TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | -- | Ground
3 | GN/WH | -- | High Beam Supply Voltage
4 | YE | -- | Low Beam Supply Voltage

### Headlamp - Right (TR6)

#### Connector Part Information

- OEM: PB625-06027
- Service: N/A
- Description: 6-Way F NMWP 06F-B Series, Sealed (BK)

#### Headlamp - Right (TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | BN/WH | -- | Park Lamp Supply Voltage
3 | GN | -- | Headlamp Levelling
4 | L-GN/BK | -- | High Beam Supply Voltage
5 | BN/WH | -- | Low Beam Supply Voltage
6 | BK | -- | Ground

### Headlamp - Right (-TR6)

#### Connector Part Information

- OEM: PB625-04027
- Service: N/A
- Description: 4-Way F NMWP 04F-B Series, Sealed (BK)

#### Headlamp - Right (-TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | -- | Ground
3 | L-GN/BK | -- | High Beam Supply Voltage
4 | BN/WH | -- | Low Beam Supply Voltage

### Headlamp Switch

#### Connector Part Information

- OEM: 936271-1
- Service: N/A
- Description: 6-Way M 090 Series (NA)

#### Headlamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | 2185 | Park Lamp Switch Signal
2 | BK | 1250 | Ground
3 | L-GN/BK | 2184 | Off Switch (T82)
4 | BK | 1250 | Ground
5 | YE | 317 | Front Fog Lamp Switch Signal
6 | GY/BK | 1798 | Head Lamp Switch Signal

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LBK/LBM)

#### Connector Part Information

- OEM: 174257-2
- Service: N/A
- Description: 4-Way M 070 Series Econoseal J MK-2 Series (BK)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 Signal
2 | PK | -- | Ignition 1 Voltage
3 | D-GN/WH | -- | Low Reference
4 | GY | -- | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 Heater Control

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LBK/LBM)

#### Connector Part Information

- OEM: PB625-04027
- Service: N/A
- Description: 4-Way F NMWP 02F-B Series (BK)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | -- | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 Signal
2 | PK | -- | Ignition 1 Voltage
3 | D-BU/WH | -- | Low Reference
4 | GY/WH | -- | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 Heater Control

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LBK/LBM)

#### Connector Part Information

- OEM: 174257-2
- Service: N/A
- Description: 4-Way M 070 Series Econoseal J MK-2 Series (BK)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 Signal
2 | PK | -- | Ignition 1 Voltage
3 | D-GN | -- | Low Reference
4 | L-GN/WH | -- | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 Heater Control

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LBK/LBM)

#### Connector Part Information

- OEM: PB625-04027
- Service: N/A
- Description: 4-Way F NMWP 02F-B Series (BK)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 Signal
2 | PK | -- | Ignition 1 Voltage
3 | D-BU | -- | Low Reference
4 | L-GN | -- | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 Heater Control

### Heated Seat - Driver (C37)

#### Connector Part Information

- OEM: MG610263
- Service: N/A
- Description: N/A

#### Heated Seat - Driver (C37)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Ground
2 | D-GN | -- | Heated Seat Supply Voltage

### Heated Seat - Passenger (C38)

#### Connector Part Information

- OEM: MG610263
- Service: N/A
- Description: N/A

#### Heated Seat - Passenger (C38)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Heated Seat Supply Voltage
2 | BK | -- | Ground

### Heated Seat Switch - Driver (C37)

#### Connector Part Information

- OEM: MG651044-2
- Service: N/A
- Description: 6-Way F 090 II Series (NA)

#### Heated Seat Switch - Driver (C37)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Accessory Voltage
BN | -- | Accessory Voltage
2 | BK | -- | Ground
3 | BK | -- | Ground (LHD)
4 | L-BU | -- | Heated Seat Supply Voltage (LHD)
BN | -- | Accessory Voltage (RHD)
5 | BN | -- | Accessory Voltage (LHD)
L-BU | -- | Heated Seat Supply Voltage (RHD)
6 | BK | -- | Ground (RHD)

### Heated Seat Switch - Passenger (C38)

#### Connector Part Information

- OEM: MG651044
- Service: N/A
- Description: 6-Way F 090 II Series (NA)

#### Heated Seat Switch - Passenger (C38)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Accessory Voltage
2 | BK | -- | Ground
3 | BK | -- | Ground (RHD)
4 | GY | -- | Accessory Voltage (LHD)
GY | -- | Accessory Voltage (LHD)
D-BU/WH | -- | Heated Seat Supply Voltage (RHD)
5 | D-BU/WH | -- | Heated Seat Supply Voltage (LHD)
GY | -- | Accessory Voltage (RHD)
GY | -- | Accessory Voltage (RHD)
6 | BK | -- | Ground (LHD)

### High Pressure Pump (LLW)

#### Connector Part Information

- OEM: 1928403874
- Service: N/A
- Description: 2-Way F Kompakt 2.8 Series, Sealed (BK)

#### High Pressure Pump (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Battery Positive Voltage
2 | D-GN | -- | Control

### High Speed Blower Motor Relay (C68)

#### Connector Part Information

- OEM: AK5443-R
- Service: N/A
- Description:

#### High Speed Blower Motor Relay (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
30 | PK | -- | Blower Motor Speed Signal
85 | BN | -- | Ignition Voltage
86 | D-BU/BK | -- | High Speed Blower Motor Control
87 | BK | -- | Ground

### Hood Ajar Switch

#### Connector Part Information

- OEM: MG611530
- Service: N/A
- Description: 3-Way F (WH)

#### Hood Ajar Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | PK/BK | -- | Hood Ajar Switch Signal
3 | -- | -- | Not Used

### Horn - High

#### Connector Part Information

- OEM: MG641156
- Service: N/A
- Description: 2-Way F 090 WP Series (GY)

#### Horn - High

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | Horn Control
2 | BK | -- | Ground

### Horn - Low

#### Connector Part Information

- OEM: MG641156
- Service: N/A
- Description: 2-Way F WP Series (GY)

#### Horn - Low

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | Horn Control
2 | BK | -- | Ground

### HVAC Control Module (C60/C66)

#### Connector Part Information

- OEM: MG610363
- Service: N/A
- Description: WH

#### HVAC Control Module (C60/C66)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Ground
2 | L-BU | -- | Air Mix Door Motor Control
3 | YE | -- | Air Mix Door Motor Signal
4 | -- | -- | Not Used
5 | BN | -- | Ignition Voltage
6 | D-GN/WH | -- | A/C Request Signal
7 | BN | -- | Air Mix Door Motor Control
8 | YE/BK | -- | Air Mix Door Motor Signal
9-10 | -- | -- | Not Used
11 | D-GN/BK | -- | Recirc Door Control
12 | PK/WH | -- | Recirc Door Control
13 | -- | -- | Not Used
14 | OG | -- | Battery Voltage
15 | D-GN/BK | -- | Mode Actuator Signal
16 | PK | -- | Mode Actuator Signal
17 | YE/D-BU | -- | Mode Actuator Signal
18 | WH/BK | -- | Mode Actuator Signal
19 | PK/BK | -- | Mode Actuator Signal
20 | WH/RD | -- | Blower Switch Signal

### HVAC Control Module X1 (C68)

#### Connector Part Information

- OEM: MG610360
- Service: N/A
- Description: 16-Way F SP Series (NA)

#### HVAC Control Module X1 (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-BU | -- | Air Temperature Door Control
3 | -- | -- | Not Used
4 | BN/WH | -- | Instrument Panel Lamps Dimmer Switch Control
5 | BN | -- | Ignition 2 Voltage
6 | D-GN/WH | -- | A/C Request Signal
7 | -- | -- | Not Used
8 | YE | -- | Air Temperature Door Control
9-13 | -- | -- | Not Used
14 | OG | -- | Battery Positive Voltage
15 | YE | -- | Ground
16 | D-BU/BK | -- | Blower High Relay Control

### HVAC Control Module X2 (C68)

#### Connector Part Information

- OEM: MG610363
- Service: N/A
- Description: WH

#### HVAC Control Module X2 (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | GY/BK | -- | Blower Motor Power Transistor Control
3 | -- | -- | Not Used
4 | BN | -- | Air Temp Actuator Reference Voltage
5 | YE/BK | -- | Air Temp Actuator Signal
6 | BK | -- | Ground
7 | D-GN | -- | Wiper Signal
8 | L-GN/BK | -- | Ambient Air Temperature Sensor Signal
9 | -- | -- | Not Used
10 | L-BU/BK | -- | Sunload Sensor Signal
11 | BK | -- | Ground
12 | D-BU | -- | Blower Feedback
13 | PK/WH | -- | Recirc Door Control A
14 | D-GN/BK | -- | Recirc Door Control B
15 | -- | -- | Not Used
16 | D-GN/BK | -- | Mode Actuator
17 | PK | -- | Mode Actuator
18 | YE/D-BU | -- | Mode Actuator
19 | WH/BK | -- | Mode Actuator
20 | PK/BK | -- | Mode Actuator

### Ignition Coil Module 1 (LBK/LBM)

#### Connector Part Information

- OEM: AK32325
- Service: N/A
- Description: 3-Way F (GY)

#### Ignition Coil Module 1 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | -- | Ignition Coil 1 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 2 (LBK/LBM)

#### Connector Part Information

- OEM: AK32325
- Service: N/A
- Description: 3-Way F (GY)

#### Ignition Coil Module 2 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | -- | Ignition Coil 2 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 3 (LBK/LBM)

#### Connector Part Information

- OEM: AK32325
- Service: N/A
- Description: 3-Way F (GY)

#### Ignition Coil Module 3 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | -- | Ignition Coil 3 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 4 (LBK/LBM)

#### Connector Part Information

- OEM: AK32325
- Service: N/A
- Description: 3-Way F (GY)

#### Ignition Coil Module 4 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-BU | -- | Ignition Coil 4 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 5 (LBK/LBM)

#### Connector Part Information

- OEM: AK32325
- Service: N/A
- Description: 3-Way F (GY)

#### Ignition Coil Module 5 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-GN | -- | Ignition Coil 5 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Coil Module 6 (LBK/LBM)

#### Connector Part Information

- OEM: AK32325
- Service: N/A
- Description: 3-Way F (GY)

#### Ignition Coil Module 6 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | GY | -- | Ignition Coil 6 Control
B | BK | -- | Ground
C | PK/BK | -- | Ignition 1 Voltage

### Ignition Switch

#### Connector Part Information

- OEM: MG650887
- Service: N/A
- Description: 6-Way F 250 III Series (NA)

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 300 | Ignition Voltage
2 | RD/BK | 642 | Battery Positive Voltage
3 | YE | 5 | Crank Voltage
4 | PK | 3 | Ignition Voltage
5 | RD/WH | 1642 | Battery Positive Voltage
6 | BN | 4 | Accessory Voltage

### Immobilizer

#### Connector Part Information

- OEM:
- Service: N/A
- Description: 6-Way F (BK)

#### Immobilizer

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 1435 | Immobilizer Signal
2 | BN/WH | 1434 | Immobilizer Signal
3 | YE/BK | 1436 | Immobilizer Signal
4 | BK/WH | 351 | Immobilizer Signal
5-6 | -- | -- | Not Used

### Inflatable Restraint I/P Module

#### Connector Part Information

- OEM: 160201704
- Service: N/A
- Description: 2-Way (YE)

#### Inflatable Restraint I/P Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH/BK | -- | I/P Module High Control
2 | GN/WH | -- | I/P Module Low Control

### Inflatable Restraint Roof Rail Module - Left (AY0)

#### Connector Part Information

- OEM: MG651201-4
- Service: N/A
- Description: 2-Way F 090 II Series (GY)

#### Inflatable Restraint Roof Rail Module - Left (AY0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Roof Rail Module High Control
2 | PK | -- | Roof Rail Module Low Control

### Inflatable Restraint Roof Rail Module - Right (AY0)

#### Connector Part Information

- OEM: MG651201-4
- Service: N/A
- Description: 2-Way F 090 II Series (GY)

#### Inflatable Restraint Roof Rail Module - Right (AY0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | -- | Roof Rail Module High Control
2 | WH/BK | -- | Roof Rail Module Low Control

### Inflatable Restraint Sensing and Diagnostic Module (SDM)

#### Connector Part Information

- OEM: 1-1411096-1
- Service: N/A
- Description: 75-Way (YE)

#### Inflatable Restraint Sensing and Diagnostic Module (SDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-25 | -- | -- | Not Used
26 | PK | 1139 | Ignition 1 Voltage
27 | YE | 358 | Air Bag Indicator Control
28 | BK/WH | 251 | Ground
29 | D-GN | 348 | Steering Wheel Module Low Control (AJ3)
BN/WH | 3020 | Steering Wheel Module Stage 1 Low Control
30 | WH | -- | Steering Wheel Module High Control (AJ3)
BN | 3021 | Steering Wheel Module Stage 1 High Control
31 | YE | 3025 | Passenger IP Module Stage 1 High Control
32 | OG | 3024 | Passenger IP Module Stage 1 Low Control
33 | OG/BK | 2119 | Seat Belt Pretensioner Left Low Control
34 | BN/WH | 2118 | Seat Belt Pretensioner Right High Control
35 | L-GN | 2116 | Seat Belt Pretensioner Right High Control
36 | OG | 2117 | Seat Belt Pretensioner Right Low Control
37 | OG/BK | 5224 | Side Impact Module Driver Low Control (AY0)
38 | BN/WH | 5223 | Side Impact Module Driver High Control (AY0)
39 | PU/WH | 5225 | Side Impact Module Passenger High Control (AY0)
40 | GY | 5228 | Side Impact Module Passenger Low Control (AY0)
41-44 | -- | -- | Not Used
45 | PU/WH | 5019 | Roof Rail Impact Module Left High Control (AY0)
46 | PK | 5020 | Roof Rail Impact Module Left Low Control (AY0)
47 | YE/BK | 5021 | Roof Rail Impact Module Right High Control (AY0)
48 | WH/BK | 5022 | Roof Rail Impact Module Right Low Control (AY0)
49-51 | -- | -- | Not Used
52 | BN/WH | 238 | Driver Seat Belt Indicator Control
53 | PU/WH | 5234 | Passenger Seat Belt Indicator Control (LHD LLW)
PU | -- | Passenger Seat Belt Indicator Control
54 | WH/BK | 5043 | Serial Data
55 | -- | -- | Not Used
56 | L-BU | -- | Passenger Air Bag OFF Indicator Control (LHD LLW)
D-GN/WH | 2308 | Passenger Air Bag OFF Indicator Control
57 | D-GN/WH | 817 | Vehicle Speed Sensor
58 | OG | 1000 | Post Crash Unlock Signal
59 | L-GN | 1845 | Chime Signal
60 | -- | -- | Not Used
61 | D-GN | 5016 | Driver Seat Belt Switch Signal
62 | OG | 1362 | Passenger Seat Belt Switch Signal
63 | PK/BK | 5861 | Passenger Presence System Signal (AL5)
64 | PK/BK | 5861 | Passenger Presence System Signal (AL5)
65-66 | -- | -- | Not Used
67 | D-BU/WH | 2307 | Passenger Air Bag On Indicator Control
68 | D-BU | 2104 | Side Impact Sensor Right Low (AY0)
69 | GY | 2103 | Side Impact Sensor Right High (AY0)
70 | D-GN | 2105 | Side Impact Sensor Left High (AY0)
71 | BN | 2106 | Side Impact Sensor Left Low (AY0)
72 | D-GN | 2134 | Right Front Side Impact Sensing Module Signal
73 | RD | 2133 | Right Front Side Impact Sensing Module Supply Voltage
74 | BK | 2131 | Left Front Side Impact Sensing Module Supply Voltage
75 | PU | 2132 | Left Front Side Impact Sensing Module Signal

### Inflatable Restraint Side Impact Module - Driver (AY0)

#### Connector Part Information

- OEM: V23540-M5302-Y22
- Service: N/A
- Description: 2-Way Connector (YE)

#### Inflatable Restraint Side Impact Module - Driver (AY0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Side Impact Module Driver Low Control
2 | BN/WH | -- | Side Impact Module Driver High Control

### Inflatable Restraint Side Impact Module - Passenger (AY0)

#### Connector Part Information

- OEM: V23540-M5302-Y22
- Service: N/A
- Description: 2-Way (YE)

#### Inflatable Restraint Side Impact Module - Passenger (AY0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Side Impact Module Passenger Low Control
2 | PU/WH | -- | Side Impact Module Passenger High Control

### Inflatable Restraint Side Impact Sensor - Left (AY0)

#### Connector Part Information

- OEM: FC 160301118
- Service: N/A
- Description: 2-Way

#### Inflatable Restraint Side Impact Sensor - Left (AY0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN | -- | Side Impact Sensing Module Left High
2 | BN | -- | Side Impact Module Left Low

### Inflatable Restraint Side Impact Sensor - Right (AY0)

#### Connector Part Information

- OEM: FC 160301118
- Service: N/A
- Description: 2-Way

#### Inflatable Restraint Side Impact Sensor - Right (AY0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Side Impact Sensing Module Right High
2 | BU | -- | Side Impact Module Right Low

### Inflatable Restraint Steering Wheel Module

#### Connector Part Information

- OEM: 54560210
- Service: N/A
- Description: 2-Way F ABX-3 (YE)

#### Inflatable Restraint Steering Wheel Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Steering Wheel Module High Control
B | -- | -- | Steering Wheel Module Low Control

### Inflatable Restraint Steering Wheel Module Coil X1

#### Connector Part Information

- OEM: 936271
- Service: N/A
- Description: 6-Way M 090 III Series

#### Inflatable Restraint Steering Wheel Module Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Remote Radio Switch Signal
2 | BN | -- | Remote Radio Switch Ground
3 | BN | -- | Horn Relay Control
4 | -- | -- | Not Used
5 | WH/BK | -- | Cruise Switch +
6 | GY | -- | Cruise Switch Ground

### Inflatable Restraint Steering Wheel Module Coil X2

#### Connector Part Information

- OEM: MG 651201-4
- Service: N/A
- Description: 2-Way F 090 II Series (GY)

#### Inflatable Restraint Steering Wheel Module Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GN | -- | Steering Wheel Module Low Control
2 | WH | -- | Steering Wheel Module High Control

### Input Speed Sensor (M98)

#### Connector Part Information

- OEM: 7283-8125-30
- Service: N/A
- Description: 2-Way F 090 Series, Sealed (BK)

#### Input Speed Sensor (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/BK | -- | Input Shaft Speed Sensor Low
2 | PU/WH | -- | Input Shaft Speed Sensor High

### Inside Rearview Mirror

#### Connector Part Information

- OEM: MG610026
- Service: N/A
- Description: 3-Way F L3 Series (WH)

#### Inside Rearview Mirror

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Backup Lamp Supply Voltage
2 | BK | -- | Ground
3 | PK | -- | Ignition 1 Voltage

### Instrument Panel Cluster (IPC) X1

#### Connector Part Information

- OEM: 175967-2
- Service: N/A
- Description: 20-Way M 040 Hybrid MK-II Series (BK)

#### Instrument Panel Cluster (IPC) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/BK | 1555 | SSPS Warning Indicator Control (Except Holden/NV8)
2-8 | -- | -- | Not Used
9 | L-GN | 5053 | Winter Mode Indicator Control
10 | L-BU | 14 | Left Turn Signal Supply
11 | -- | -- | Not Used
12 | OG | -- | Fuel PWM Output (Diesel)
13 | PU | 1681 | Traction Control System Warning Indicator Control (NW9)
14 | WH | 629 | Daytime Running Lamp (DRL) Indicator Control (TQE)
15 | GY/WH | 1657 | TCS OFF Indicator control (NW9)
16 | D-GN | 1656 | TCS Active Indicator Control (NW9)
17 | D-GN/BK | 1867 | ABS Indicator Control (JL9)
18 | L-BU/BK | 3145 | Cruise Indicator Control
19 | YE | 172 | Low Fuel Indicator Control
20 | OG | 55 | Fuel Level Signal (LBK/LBM)
D-BU/WH | 55 | Fuel Level Signal (LLW)

### Instrument Panel Cluster (IPC) X2

#### Connector Part Information

- OEM: 175966-1
- Service: N/A
- Description: 16-Way M 040 Multilock Series (GY)

#### Instrument Panel Cluster (IPC) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 15 | Right Turn Signal Supply
2 | BN | 358 | AIR BAG Warning Indicator Control
3 | GY | 157 | Door Ajar Indicator Control
4 | BK | 2250 | Turn Indicator Ground
5 | RD/WH | 640 | Door/Trunk Ajar Indicator Supply
6 | D-GN | 135 | Coolant Temp Gage Signal
7 | D-GN | 817 | VSS Input
8 | D-GN/WH | 817 | VSS Output
9 | RD/WH | 1140 | Battery Voltage
10 | PK | 239 | Ignition Voltage
11 | BK | 2250 | Ground
12 | BN/WH | 309 | Park Lamp Supply
13 | D-GN | 44 | Illumination Dimming Control
14 | YE | 749 | Theft Deterrent Indicator Control
15 | -- | -- | Not Used
16 | WH | 121 | Engine Speed Signal

### Instrument Panel Cluster (IPC) X3

#### Connector Part Information

- OEM: 174046-2
- Service: N/A
- Description: 16-Way F 040 Multilock Series (BK)

#### Instrument Panel Cluster (IPC) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | 1885 | MIL Control
2 | BN/WH | 33 | Park Brake Indicator Control
3 | YE | 234 | Seatbelt Warning Indicator Control
4 | YE | 183 | Front Fog Indicator Control
5 | BN | -- | Tach Output (LLW)
6 | BN | 25 | Charge Indicator Control
7 | BN | 31 | Oil Pressure Indicator Control
8 | D-BU | 3021 | Change Oil Indicator Control (LLW)
9 | GY | 2555 | Parking Assist Indicator Control
10 | OG/BK | 737 | Trunk Ajar Indicator Control
11 | YE/BK | 317 | Rear Fog Indicator Control
12-13 | -- | -- | Not Used
14 | BN/WH | 99 | Washer Fluid Indicator Control
15 | -- | -- | Not Used
16 | L-GN/BK | 1360 | Hi Beam Indicator Control

### Instrument Panel Cluster (IPC) X4 (M98)

#### Connector Part Information

- OEM: 174045-4
- Service: N/A
- Description: 12-Way M 040 Multilock Series (GN)

#### Instrument Panel Cluster (IPC) X4 (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-7 | -- | -- | Not Used
8 | D-GN | 1373 | TCM Serial Data
9-12 | -- | -- | Not Used

### Instrument Panel Cluster (IPC) X4 (MH7/MH8)

#### Connector Part Information

- OEM: 936201-1
- Service: N/A
- Description: 16-Way F 090 III Series (NA)

#### Instrument Panel Cluster (IPC) X4 (MH7/MH8)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | GY | 773 | Transmission Position M Indicator Control
3 | D-BU/WH | 774 | Transmission Position D Indicator Control
4 | GY/BK | 773 | Transmission Position N Indicator Control
5 | L-GN | 775 | Transmission Position R Indicator Control
6 | WH/BK | 711 | Transmission Position P Indicator Control
7 | BN | 141 | Ignition 2 Voltage
8 | L-GN | 24 | Backup Lamp Supply Voltage
9 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
10 | BN | 2501 | High Speed GMLAN Serial Data (-)
11-16 | -- | -- | Not Used

### Intake Air Temperature (IAT) Sensor (LBK/LBM)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series (BK)

#### Intake Air Temperature (IAT) Sensor (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Intake Air Temperature (IAT) Sensor Signal
2 | YE/BK | -- | Low Reference

### Intake Manifold Tuning Valve Solenoid (LBK/LBM)

#### Connector Part Information

- OEM: 174352-2
- Service: N/A
- Description: 2-Way F Econoseal J Mark II Series (BK)

#### Intake Manifold Tuning Valve Solenoid (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | WH/BK | -- | Intake Manifold Tuning Valve Solenoid Control

### I/P Compartment Lamp

#### Connector Part Information

- OEM: AK36277
- Service: N/A
- Description: 2-Way F (GY)

#### I/P Compartment Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Inadvertent Power Control
2 | PU | -- | I/P Compartment Lamp Control

### I/P Compartment Lamp Switch

#### Connector Part Information

- OEM: AK5306
- Service: N/A
- Description: 2-Way F (BK)

#### I/P Compartment Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | I/P Compartment Lamp Control
2 | BK | -- | Ground

### Key Reminder Switch

#### Connector Part Information

- OEM: MG610489-5
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### Key Reminder Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/WH | -- | Key In Signal
2 | BN | -- | Battery Positive Voltage

### Knock Sensor (KS) 1 (LBK/LBM)

#### Connector Part Information

- OEM: 368215-1
- Service: N/A
- Description: 3-Way F JPT Series (GY)

#### Knock Sensor (KS) 1 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | -- | Knock Sensor (KS) 1 Signal
2 | YE/BK | -- | Low Reference
3 | GY | -- | Shield Ground

### Knock Sensor (KS) 2 (LBK/LBM)

#### Connector Part Information

- OEM: 368215-1
- Service: N/A
- Description: 3-Way F JPT Series (GY)

#### Knock Sensor (KS) 2 (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Knock Sensor (KS) 2 Signal
2 | YE/BK | -- | Low Reference
3 | GY | -- | Shield Ground

### License Lamp

#### Connector Part Information

- OEM: MG610489-5
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### License Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | License Plate Lamp Supply Voltage
2 | BK | -- | Ground

### Magnetic Steering Actuator (N40/NV8)

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP 04F-B Series (BK)

#### Magnetic Steering Actuator (N40/NV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU/BK | -- | Variable Effort Steering Actuator Control - High
2 | L-BU/BK | -- | Variable Effort Steering Actuator Control - Low

### Manifold Absolute Pressure (MAP) Sensor (LBK/LBM)

#### Connector Part Information

- OEM: 12129946
- Service: N/A
- Description: 3-Way F Metri-Pack 150 Series Sealed (GY)

#### Manifold Absolute Pressure (MAP) Sensor (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | -- | Low Reference
B | L-GN | -- | Manifold Absolute Pressure (MAP) Sensor Signal
C | OG/BK | -- | 5-Volt Reference

### Mass Air Flow (MAF) Sensor (LBK/LBM)

#### Connector Part Information

- OEM: 85205-1
- Service: N/A
- Description: 3-Way F JPT Series (BK)

#### Mass Air Flow (MAF) Sensor (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | -- | Low Reference
2 | YE | -- | Mass Air Flow (MAF) Sensor Signal
3 | PK | -- | Ignition 1 Voltage

### Mass Air Flow (MAF) Sensor (LLW)

#### Connector Part Information

- OEM: 1928403736
- Service: N/A
- Description: 4-Way F Kompakt Series, Sealed (BK)

#### Mass Air Flow (MAF) Sensor (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Ignition 1 Voltage
2 | YE/BK | -- | Ground
3 | D-BU/WH | -- | IAT Signal
4 | PU/WH | -- | MAF Signal

### Mode Actuator

#### Connector Part Information

- OEM: MG610203
- Service: N/A
- Description: 7-Way F 118 Series (NA)

#### Mode Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/D-BU | -- | Lower Mode Valve Solenoid Control
2 | PK | -- | Defrost Mode Valve Solenoid Control
3 | D-GN/BK | -- | Upper Mode Valve Solenoid Control
4 | BN | -- | Ignition 3 Voltage
5 | BK | -- | Ground
6 | PK/BK | -- | Mode Valve Signal
7 | WH/BK | -- | Mode Valve Signal

### Multifunction Control Module X1

#### Connector Part Information

- OEM: 368136-1
- Service: N/A
- Description: 26-Way F 070 Series, Sealed (NA)

#### Multifunction Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | 737 | Trunk Contact Signal
2 | L-BU | 20 | Brake Switch Signal
3 | BN | 25 | Engine Running Signal
4 | L-GN | 80 | Key In Signal
5 | L-GN | 275 | Park Position Signal
6 | -- | -- | Not Used
7 | BN/WH | 230 | Reference Voltage
8 | D-GN | 144 | Dimmer Switch Signal
9 | YE | 43 | Accessory Voltage
10 | L-GN | 24 | Back Up Switch Signal
11 | WH | -- | Sun Load Sensor Signal (T82)
12 | RD/WH | 1140 | Battery Positive Voltage
13 | PK | 239 | Ignition 1 Voltage
14 | D-GN/BK | 1798 | Head Lamp Switch Signal
15 | GY/BK | 2185 | Park Lamp Switch Signal
16 | L-GN/BK | 2184 | Light Switch Signal
17 | BN | 126 | Driver Door Contact Signal
18 | WH | 156 | All Doors Contact Signal
19 | OG/WH | 881 | Up/Down Switch Signal
20 | BN | 1890 | COM
21 | PU/WH | 889 | Left/Right Switch Signal
22 | D-GN/WH | 1788 | 5-Volt Reference
23 | D-GN | 1784 | Vertical Sensor Signal
24 | D-BU | 1729 | Sensor Ground
25 | BK | 250 | Ground
26 | -- | -- | Not Used

### Multifunction Control Module X2

#### Connector Part Information

- OEM: 368135-1
- Service: N/A
- Description: 22-Way F

#### Multifunction Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | 1785 | Horizontal Sensor Signal
2 | YE | 183 | Front Fog Indicator Control
3 | YE/BK | 317 | Rear Fog Indicator Control
4 | L-GN/BK | 1360 | High Beam Indicator Control
5 | WH | 629 | DRL Indicator
6 | GY | 1890 | Passenger Common Control
7 | RD/WH | 1881 | Up/Down Passenger Control
8 | PU | 1889 | Left/Right Passenger Control
9 | GY/BK | 179 | Folding Mirror Switch Signal
10 | -- | -- | Not Used
11 | OG | 122 | Rear Fog Lamp Control
12 | BN/WH | 309 | Dimmer PWM Output Control
13 | WH | 1080 | Park Lamp Control
14 | D-GN/BK | 1798 | Head Lamp Low Beam Control
15 | RD/WH | 140 | Head Lamp High Beam Control
16 | D-GN/WH | 1317 | Fog Lamp Control
17 | YE | 317 | Fog Lamp Switch Signal
18 | OG | 122 | Rear Fog Lamp Switch Signal
19 | PU | 524 | Head Lamp High Switch Signal
20 | YE/BK | 307 | Head Lamp Passing Switch Signal
21 | L-BU | 191 | Mirror Unfolding Control
22 | YE | 190 | Mirror Folding Control

### Multifunction Control Module X3

#### Connector Part Information

- OEM: 929504-3
- Service: N/A
- Description: 8-Way F JPT Series (BK)

#### Multifunction Control Module X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | PK/D-BU | 145 | Ignition 2 Voltage
3 | D-BU/WH | 1640 | Courtesy Lamp Power Control
4 | BK | 351 | Ground
5 | BN | 186 | BTSI Solenoid Control
6 | -- | -- | Not Used
7 | RD/WH | 640 | Inadvertent Lamp Power Control
8 | RD/WH | 1340 | Battery Positive Voltage

### Multifunction Switch

#### Connector Part Information

- OEM: 15394150
- Service: N/A
- Description: 16-Way F (BK)

#### Multifunction Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Right Mirror Up/Down Motor
OG/WH | -- | Right Mirror Up/Down Motor (DL7)
2 | GY/BK | 179 | Folding Mirror Switch Signal
3 | YE | -- | Left Mirror Up/Down Motor
4 | BN | 1890 | Mirror Motor Common
5 | PU | -- | Right Mirror Left/Right Motor
PU/WH | -- | Right Mirror Left/Right Motor (DL7)
6 | BK | 2250 | Ground
7 | -- | -- | Not Used
8 | BK | 450 | Ground
9 | WH | -- | Left Mirror Left/Right Motor
10 | BN | 1739 | Ignition 1 Voltage
11 | BN/WH | 309 | Dimmer PWM Output
12 | D-GN | 144 | Dimmer Switch Signal
13 | BN/WH | 230 | Reference Voltage
14 | BN | 312 | Headlamp Levelling Switch Control (LBK/LBM)
BN/WH | 189 | Headlamp Levelling Switch Signal (LLW)
15 | L-GN | 189 | Headlamp Levelling Switch Signal (LBK/LBM)
OG | 312 | Headlamp Levelling Switch Control (LLW)
16 | OG | 122 | Rear Fog Lamp Switch Signal

### Multifunction/Turn Signal Switch

#### Connector Part Information

- OEM: 929504-3
- Service: N/A
- Description: 8-Way F JPT Series (BK)

#### Multifunction/Turn Signal Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | YE/BK | -- | Passing Switch Signal
3 | PU | -- | Dimmer Switch Signal
4 | BK | -- | Ground
5-6 | -- | -- | Not Used
7 | D-BU/WH | -- | Right Turn Switch Signal
8 | L-BU/WH | -- | Left Turn Switch Signal

### Object Detection Alarm (UD7)

#### Connector Part Information

- OEM: MG610209
- Service: N/A
- Description: 3-Way F

#### Object Detection Alarm (UD7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU | -- | Alarm Power
2 | YE | -- | Alarm Signal
3 | GY | -- | Alarm Ground

### Object Detection Module (UD7)

#### Connector Part Information

- OEM: 15394150
- Service: N/A
- Description: 16-Way Micro-Pack 064 Series (BK)

#### Object Detection Module (UD7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Right Corner Sensor Signal
2 | OG/BK | -- | Right Middle Sensor Signal
3 | BU | -- | Left Middle Sensor
4 | YE | -- | Left Corner Sensor Signal
5 | L-GN | -- | Back Up Lamp Switch Signal
6 | BU | -- | Alarm Power
7 | GY | -- | Alarm Ground
8 | PK | -- | Ignition 1 Voltage
9 | BN | -- | Right Sensor Ground
10 | GY | -- | Indicator Control
11 | -- | -- | Not Used
12 | BN/WH | -- | Left Sensor Ground
13 | L-BU | -- | Park Brake Switch Signal
14 | YE | -- | Alarm Signal
15 | -- | -- | Not Used
16 | BK | -- | Ground

### Object Detection Sensor - Left Corner (UD7)

#### Connector Part Information

- OEM: MG642273
- Service: N/A
- Description: 2-Way

#### Object Detection Sensor - Left Corner (UD7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Ground
2 | YE | -- | Signal

### Object Detection Sensor - Left Middle (UD7)

#### Connector Part Information

- OEM: MG642273
- Service: N/A
- Description: 2-Way

#### Object Detection Sensor - Left Middle (UD7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Ground
2 | BU | -- | Signal

### Object Detection Sensor - Right Corner (UD7)

#### Connector Part Information

- OEM: MG642273
- Service: N/A
- Description: 2-Way

#### Object Detection Sensor - Right Corner (UD7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Ground
2 | GY | -- | Signal

### Object Detection Sensor - Right Middle (UD7)

#### Connector Part Information

- OEM: MG642273
- Service: N/A
- Description: 2-Way

#### Object Detection Sensor - Right Middle (UD7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Ground
2 | OG/BK | -- | Signal

### Oil Feeding Connector (JL9-F45)

#### Connector Part Information

- OEM: MG640329
- Service: N/A
- Description: 3-Way M SWP Series (BK)

#### Oil Feeding Connector (JL9-F45)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | WH/BK | -- | Serial Data
3 | PK | -- | Ignition 1 Voltage

### Oil Feeding Connector (JL9+F45)

#### Connector Part Information

- OEM: MG640333-5
- Service: N/A
- Description: 4-Way M SWP Series (BK)

#### Oil Feeding Connector (JL9+F45)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
3 | BN | 2501 | High Speed GNLAN Serial Data (-)
4 | PK | 1339 | Ignition 1 Voltage

### Oil Pressure Switch

#### Connector Part Information

- OEM: AK32104
- Service: N/A
- Description: 1-Way F Metri-Pack 150 Series, Sealed

#### Oil Pressure Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Oil Pressure Indicator Control

### Output Speed Sensor (M98)

#### Connector Part Information

- OEM: 7283-8125-30
- Service: N/A
- Description: 2-Way F 090 Series, Sealed (BK)

#### Output Speed Sensor (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Input Shaft Speed Sensor Low
2 | YE | -- | Input Shaft Speed Sensor High

### Outside Rearview Mirror - Driver

#### Connector Part Information

- OEM: 174045-2
- Service: N/A
- Description: 12-Way M 40 Multilock Series (BK)

#### Outside Rearview Mirror - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Turn Signal Lamp
2 | YE | -- | Folding Mirror Motor Extend Control
3 | L-BU | -- | Folding Mirror Motor Retract Control
4 | YE | -- | Mirror Motor Vertical Control
5 | BN | -- | Motor Common
6 | WH | -- | Mirror Motor Horizontal Control
7-10 | -- | -- | Not Used
11 | OG | -- | Heated Mirror Element Supply Voltage
12 | BK | -- | Ground

### Outside Rearview Mirror - Passenger

#### Connector Part Information

- OEM: 174045-2
- Service: N/A
- Description: 12-Way M 040 Multilock Series (BK)

#### Outside Rearview Mirror - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU | -- | Turn Signal Lamp
2 | YE | -- | Folding Mirror Motor Extend Control
3 | L-BU | -- | Folding Mirror Motor Retract Control
4 | BN | -- | Mirror Motor Vertical Control
5 | GY | -- | Motor Common
6 | PU | -- | Mirror Motor Horizontal Control
7 | D-GN | -- | Vertical Signal
8 | RD | -- | Horizontal Signal
9 | D-BU | -- | Ground
10 | GN/WH | -- | 5-Volt Reference
11 | OG | -- | Heated Mirror Element Supply Voltage
12 | BK | -- | Ground

### Park/Neutral Position Switch (M98)

#### Connector Part Information

- OEM: 7223-6508-30
- Service: N/A
- Description: 10-Way F DMS+RV Series, Sealed (BK)

#### Park/Neutral Position Switch (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | L-GN | -- | Reverse Signal
3 | BK/WH | -- | Ground
4 | PK/BK | -- | Park/Neutral Signal
5 | GY | -- | C Signal
6 | YE | -- | B Signal
7 | -- | -- | Not Used
8 | WH | -- | PA Signal
9 | PK | -- | Ignition 1 Voltage
10 | BN/WH | -- | A Signal

### Park Brake Switch

#### Connector Part Information

- OEM: MG651194
- Service: N/A
- Description: 1-Way F 090-II Series

#### Park Brake Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Brake Warning Indicator Control

### Passenger Airbag/Seat Belt Warning Lamp

#### Connector Part Information

- OEM: PHB845-07010
- Service: N/A
- Description: 7-Way F CDR07F Series (WH)

#### Passenger Airbag/Seat Belt Warning Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | PU | -- | Passenger Seat Belt Indicator Control
3-4 | -- | -- | Not used
5 | PK | -- | Ignition 1 Voltage
6 | GN/WH | -- | Passenger Air Bag OFF Indicator Control
7 | -- | -- | Not Used

### Passenger Presence System Sensor (AL5)

#### Connector Part Information

- OEM: 1-967640-1
- Service: N/A
- Description: 4-Way F MQS Socket Housing, Sealed (BK)

#### Passenger Presence System Sensor (AL5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | PK/BK | -- | Passenger Presence Signal
3 | BK/WH | -- | Ground
4 | -- | -- | Not Used

### Power Amplifier (U63)

#### Connector Part Information

- OEM: 173853-1
- Service: N/A
- Description: 18-Way F 070 Multilock Series (WH)

#### Power Amplifier (U63)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 550 | Ground
2 | OG | 340 | Battery Voltage
3 | YE | 116 | Speaker Return Left Rear
4 | WH | 119 | Speaker Feed Left Rear
5 | D-GN | 117 | Speaker Return Right Front (LHD)
GY | 118 | Speaker Return Right Front (RHD)
6 | L-GN | 200 | Speaker Feed Left Front (LHD)
BN | 201 | Speaker Feed Left Front (RHD)
7-8 | -- | -- | Not Used
9 | BK | 550 | Ground
10 | OG | 340 | Battery Voltage
11 | -- | -- | Not Used
12 | L-BU | 115 | Speaker Return Right Rear
13 | D-BU | 46 | Speaker Feed Right Rear
14 | GY | 118 | Speaker Return Left Front (LHD)
D-GN | 117 | Speaker Return Right Front (RHD)
15 | BN | 201 | Speaker Feed Left Front (LHD)
L-GN | 200 | Speaker Feed Right Front (RHD)
16-18 | -- | -- | Not Used

### Power Seat Switch (AH5)

#### Connector Part Information

- OEM: MG610404
- Service: N/A
- Description: 10-Way F 070 Series (NA)

#### Power Seat Switch (AH5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | -- | Battery Positive Voltage
2 | BK | -- | Ground
3 | D-BU | -- | Sliding Motor Control
4 | D-BU/WH | -- | Sliding Motor Control
5 | YE | -- | Front Lift Motor Control
6 | YE/RD | -- | Front Lift Motor Control
7 | WH | -- | Rear Lift Motor Control
8 | WH/RD | -- | Rear Lift Motor Control
9 | D-GN | -- | Recline Motor Control
10 | L-GN | -- | Recline Motor Control

### Power Seat Test Connector (AH5)

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: 2-Way F 250 Series (NA)

#### Power Seat Test Connector (AH5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Battery Positive Voltage
2 | BK | -- | Ground

### Power Steering Control Module (N40/NV8)

#### Connector Part Information

- OEM: MG651050
- Service: N/A
- Description: 8-Way F 090-II Series (WH)

#### Power Steering Control Module (N40/NV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | -- | Variable Effort Steering Actuator Control - Low
2 | D-BU/BK | -- | Variable Effort Steering Actuator Control - High
3 | -- | -- | Not Used
4 | D-BU/WH | -- | Serial Data
5 | L-GN/BK | -- | Variable Effort Steering Actuator Indicator Lamp Control
6 | D-GN/WH | -- | Vehicle Speed Signal
7 | BN | -- | Ignition 2 Voltage
8 | BK | -- | Ground

### PRNDL Lamp

#### Connector Part Information

- OEM: MG611857
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### PRNDL Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | Ground
2 | BN/WH | -- | Dimmer PWM Output

### PTC Heater (LLW)

#### Connector Part Information

- OEM: 15326878
- Service: N/A
- Description: 3-Way F GT 280 Series (BK)

#### PTC Heater (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | -- | PTC Heater Supply Voltage
2 | BN | -- | PTC Heater Supply Voltage
3 | D-BU/WH | -- | PTC Heater Supply Voltage

### Radio X1

#### Connector Part Information

- OEM: 15464950
- Service: N/A
- Description: 14-Way F GT ISO Micro 64 Modular Series (BK)

#### Radio X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 40 | Battery Voltage
2 | BN | -- | Speaker Feed Left Front (LHD)
L-GN | 200 | Speaker Feed Left Front (RHD)
3 | L-GN | -- | Speaker Feed Right Front (LHD)
BN | 201 | Speaker Feed Right Front (RHD)
4-5 | -- | -- | Not Used
6 | GY | 161 | Power Antenna Feed
7 | BN/WH | 309 | Illumination Feed
8 | BK | 350 | Ground
9 | GY | -- | Speaker Return Left Front (LHD)
D-GN | 117 | Speaker Return Left Front (RHD)
10 | D-GN | -- | Speaker Return Right Front (LHD)
GY | 118 | Speaker Return Right Front (RHD)
11 | -- | -- | Not Used
12 | BN | 180 | Remote Radio Return Ground
13 | -- | -- | Not Used
14 | D-GN | 44 | Instrument Panel Lamps Dimmer Control

### Radio X2

#### Connector Part Information

- OEM: 15394150
- Service: N/A
- Description: 16-Way F Micro-Pack 064 Series (BK)

#### Radio X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | PK/BK | 5755 | Remote On (U63)
3 | D-GN | 1795 | Amp Signal Feed (U63)
4 | -- | -- | Not Used
5 | WH | 119 | Speaker Feed Left Rear
6 | D-BU | 46 | Speaker Feed Right Rear
7-8 | -- | -- | Not Used
9 | PU/WH | 5754 | Amp Enable (U63)
10 | -- | -- | Not Used
11 | BK/WH | 315 | Amp Signal (U63)
12 | L-GN | 1011 | Radio Control Signal Steering Column
13 | YE | 116 | Speaker Return Left Rear
14 | L-BU | 115 | Speaker Return Right Rear
15 | -- | -- | Not Used
16 | YE | 243 | Ignition Voltage

### Radio Antenna Module

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: 2-Way F 250 Series (WH)

#### Radio Antenna Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | -- | Rear Defog Element Supply Voltage
2 | GY | -- | Antenna Enable Signal

### Rain Sensor (CEI)

#### Connector Part Information

- OEM: 43645-0800
- Service: N/A
- Description: 8-Way F Micro-Fit Series (BK)

#### Rain Sensor (CEI)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Low Speed
2 | BU | -- | High Speed
3 | BK | -- | Ground
4 | PK | -- | Ignition 1 Voltage
5 | BU/WH | -- | Auto Sensitivity
6 | OG | -- | Washer Switch Signal
7 | BN | -- | Wiper AUTO Output
8 | -- | -- | Not Used

### Rear Compartment Lamp

#### Connector Part Information

- OEM: AK5306
- Service: N/A
- Description: 2-Way F (BK)

#### Rear Compartment Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Inadvertent Power Control
2 | OG/BK | -- | Rear Compartment Lamp Control

### Rear Compartment Release Switch

#### Connector Part Information

- OEM: MG651201-4
- Service: N/A
- Description: 2-Way F 090 II Series (GY)

#### Rear Compartment Release Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 253 | Trunk Release Control
2 | RD | 1140 | Battery Positive Voltage

### Rear Window Defogger Grid X1

#### Connector Part Information

- OEM: 12092133
- Service: N/A
- Description: 1-Way F Metri-Pack 630 Series Self Lock (BK)

#### Rear Window Defogger Grid X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | -- | Rear Defogger Element Supply Voltage

### Rear Window Defogger Grid X2

#### Connector Part Information

- OEM: 12092133
- Service: N/A
- Description: 1-Way F Metri-Pack 630 Series Self Lock (BK)

#### Rear Window Defogger Grid X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | -- | Rear Defogger Ground

### Recirculation Actuator

#### Connector Part Information

- OEM: KET MG 610203
- Service: N/A
- Description: 7-Way F (BK)

#### Recirculation Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | BN | -- | Ignition 1 Voltage
5 | PK/WH | -- | Recirculation Door Control A
6 | -- | -- | Not Used
7 | D-GN/BK | -- | Recirculation Door Control B

### Seat Belt Pretensioner - Driver

#### Connector Part Information

- OEM: V23540-M5302-Y22
- Service: N/A
- Description: 2-Way F

#### Seat Belt Pretensioner - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Seat Belt Pretensioner Left High Control
2 | OG/BK | -- | Seat Belt Pretensioner Left Low Control

### Seat Belt Pretensioner - Passenger

#### Connector Part Information

- OEM: V23540-M5302-Y22
- Service: N/A
- Description: 2-Way F

#### Seat Belt Pretensioner - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Seat Belt Pretensioner Right High Control
2 | OG | -- | Seat Belt Pretensioner Right Low Control

### Seat Belt Switch - Driver

#### Connector Part Information

- OEM: MG610392
- Service: N/A
- Description: 2-Way F

#### Seat Belt Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | GN | -- | Driver Seat Belt Switch Signal

### Seat Belt Switch - Passenger

#### Connector Part Information

- OEM: MG610392
- Service: N/A
- Description: 2-Way F

#### Seat Belt Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | OG | -- | Passenger Seat Belt Switch Signal

### Speaker - Left Front

#### Connector Part Information

- OEM: MG610070
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### Speaker - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Left Front Speaker Return (LHD)
D-GN | -- | Left Front Speaker Return (RHD)
2 | BN | -- | Left Front Speaker Feed (LHD)
L-GN/BK | -- | Left Front Speaker Feed (RHD)

### Speaker - Left Rear

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: (WH)

#### Speaker - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Left Rear speaker Return
2 | WH | -- | Left Rear Speaker Feed

### Speaker - Right Front

#### Connector Part Information

- OEM: MG610070
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### Speaker - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | Right Front Return (LHD)
GY | -- | Right Front Return (RHD)
2 | L-GN/BK | -- | Right Front Speaker Feed (LHD)
BN | -- | Right Front Speaker Feed (RHD)

### Speaker - Right Rear

#### Connector Part Information

- OEM: MG610070
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### Speaker - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Right Rear Speaker Return
2 | WH | -- | Right Rear Speaker Feed

### Steering Angle Sensor (F45)

#### Connector Part Information

- OEM: 1488752-1
- Service: N/A
- Description: 6-Way F 064 GET Series (BK)

#### Steering Angle Sensor (F45)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 839 | 12V Reference
2 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
3 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
4 | BN | 2501 | High Speed GMLAN Serial Data (-)
5 | BN | 2501 | High Speed GMLAN Serial Data (-)
6 | BK | 650 | Ground

### Stop Lamp Switch

#### Connector Part Information

- OEM: MG610267
- Service: N/A
- Description: 4-Way F 250 Double Lock Series (NA)

#### Stop Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 839 | Ignition 1 Voltage
2 | OG | 540 | Battery Positive Voltage (LHD)
BN | 186 | Brake Pedal Position Switch Signal (RHD)
3 | BN | 186 | Brake Pedal Position Switch Signal (LHD)
OG | 540 | Battery Positive Voltage (RHD)
4 | L-BU/WH | 20 | Stop Lamp Switch Signal
L-BU | 20 | Stop Lamp Switch Signal

### Subwoofer Speaker

#### Connector Part Information

- OEM:
- Service: N/A
- Description:

#### Subwoofer Speaker

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | -- | Battery Voltage
2 | OG | -- | Battery Voltage
3 | D-GN | -- | Signal Feed
4 | BK | -- | Ground
5 | BK | -- | Ground
6 | PK | -- | Remote On
7 | PU | -- | Enable
8 | BK | -- | Signal Return

### Sunload Sensor (C68/T82)

#### Connector Part Information

- OEM: MG610159
- Service: N/A
- Description: 4-Way F 2.3 Series (NA)

#### Sunload Sensor (C68/T82)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Battery Positive Voltage
2 | WH | -- | Sunload Sensor Signal (T82)
3 | YE | -- | Sunload Sensor Signal (C68)
4 | BK | 351 | Ground

### Sunroof Module (CF5)

#### Connector Part Information

- OEM: 368502
- Service: N/A
- Description: WH

#### Sunroof Module (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | YE | -- | Accessory Voltage
5 | BN | -- | Sunroof Open Signal
6 | OG | -- | Sunroof Close Signal

### Sunroof Switch/Reading Lamp (CF5)

#### Connector Part Information

- OEM: 368174-1
- Service: N/A
- Description: WH

#### Sunroof Switch/Reading Lamp (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | M/F Module Output
2 | BK | -- | Ground
3 | -- | -- | Not Used
4 | BN | -- | Sunroof Open Signal
5 | OG | -- | Sunroof Close Signal
6 | YE | -- | Accessory Voltage

### Tail Lamp - Left

#### Connector Part Information

- OEM: MG610047
- Service: N/A
- Description: 4-Way F 250 Series (NA)

#### Tail Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Tail Lamp Supply Voltage
2 | L-BU/WH | -- | Stop Lamp Supply Voltage
3 | BK | -- | Ground
4 | L-BU | -- | Turn Signal Control

### Tail Lamp - Right

#### Connector Part Information

- OEM: MG610047
- Service: N/A
- Description: 4-Way F 250 Series (NA)

#### Tail Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Tail Lamp Supply Voltage
2 | L-BU/WH | -- | Stop Lamp Supply Voltage
3 | BK | -- | Ground
4 | L-BU | -- | Turn Signal Control

### Theft Deterrent Alarm

#### Connector Part Information

- OEM: PB625-02027
- Service: N/A
- Description: 2-Way F NMWP Series, Sealed (BK)

#### Theft Deterrent Alarm

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | YE | -- | Siren Control

### Throttle Body (LBK/LBM)

#### Connector Part Information

- OEM: KAFUS B06009A
- Service: N/A
- Description: 6-Way F

#### Throttle Body (LBK/LBM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | 5-Volt Reference 3
2 | PU | -- | Throttle Position (TP) Sensor 2 Signal
3 | BK | -- | Low Reference
4 | D-BU | -- | Throttle Position (TP) Sensor 1 Signal
5 | D-BU | -- | TAC Motor Control 1
6 | L-BU | -- | TAC Motor Control 2

### Throttle Plate Actuator (LLW)

#### Connector Part Information

- OEM: 42121400
- Service: N/A
- Description: 4-Way F Mini-Timer Series, Sealed (BK)

#### Throttle Plate Actuator (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | PK/WH | -- | Battery Positive Voltage
3 | WH/BK | -- | Throttle Valve Control
4 | GY/BK | -- | Feedback Signal

### Traction Control Switch (NW9)

#### Connector Part Information

- OEM: MG652999
- Service: N/A
- Description: 4-Way F 040 III Series (NA)

#### Traction Control Switch (NW9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | -- | Ignition 2 Voltage
2 | L-BU | -- | Traction Control Switch Signal
3 | BN/WH | -- | Instrument Panel Lamps Dimmer Switch Control
4 | D-GN | -- | Instrument Panel Lamps Dimmer Switch Signal

### Transmission Control Module (TCM) X1 (M98)

#### Connector Part Information

- OEM: 1318756-2
- Service: N/A
- Description: 24-Way F 025/090 Mixed Series Hybrid Series (BK)

#### Transmission Control Module (TCM) X1 (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/WH | -- | Ground
2 | WH | -- | Line Pressure Control Solenoid Control
3 | PU/WH | -- | TCC Clutch Solenoid Control
4 | BU | -- | Line Pressure Control Solenoid Supply Voltage
5 | GN | -- | TCC Clutch Solenoid Supply Voltage
6 | PK | -- | Ignition 1 Voltage
7 | BN | -- | High Speed GMLAN Serial Data (-)
8-10 | -- | -- | Not Used
11 | BN/WH | -- | Transmission Fluid Temperature Sensor Signal
12 | OG/BK | -- | Transmission Fluid Temperature Sensor Low Reference
13 | WH | -- | Shift Solenoid 4 Supply Voltage
14 | WH | -- | Shift Solenoid 3 Supply Voltage
15 | YE/BK | -- | Shift Solenoid 2 Supply Voltage
16 | L-GN | -- | Shift Solenoid 1 Supply Voltage
17 | BN/BK | -- | High Speed GMLAN Serial Data (+)
18 | -- | -- | Not Used
19 | BU/WH | -- | Shift Pressure Control Solenoid Control
20 | -- | -- | Not Used
21 | PK/BK | -- | Shift Pressure Control Solenoid Supply Voltage
22 | OG/WH | -- | Shift Solenoid 5 Supply Voltage
23 | BK/WH | -- | Ground
24 | OG | -- | Battery Positive Voltage (RHD)
RD/WH | -- | Battery Positive Voltage (LHD)

### Transmission Control Module (TCM) X2 (M98)

#### Connector Part Information

- OEM: 1318757-2
- Service: N/A
- Description: 26-Way F 090III Hybrid Series (BK)

#### Transmission Control Module (TCM) X2 (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Tap Up Signal
2 | -- | -- | Not Used
3 | L-GN | -- | Winter Mode Indicator Control
4 | L-GN/WH | -- | Winter Mode Switch Signal
5 | PU | -- | Output Shaft Speed Sensor Signal Low
6 | L-GN/BK | -- | Input Shaft Speed Sensor Signal Low
7 | YE | -- | B Signal
8 | BN/WH | -- | A Signal
9 | BN | -- | Driver Shift Control
10-13 | -- | -- | Not Used
14 | YE | -- | Output Shaft Speed Sensor Signal High
15 | D-GN | -- | Vehicle Speed Signal (LHD)
GN/WH | -- | Vehicle Speed Signal (RHD)
16 | PU/WH | -- | Input Shaft Speed Sensor Signal High
17 | GN | -- | Serial Data
18 | BN | -- | Tap Down Signal
19 | WH | -- | PA Signal
20 | GY | -- | C Signal
21 | -- | -- | Not Used
22 | L-BU | -- | Stop Lamp Switch Signal
23-26 | -- | -- | Not Used

### Trunk Latch

#### Connector Part Information

- OEM: MG651032
- Service: N/A
- Description: 3-Way F 090 II Series (NA)

#### Trunk Latch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-BU | -- | Trunk Latch Actuator Supply Voltage
3 | OG/BK | -- | Trunk Open Switch Signal

### Trunk Tamper Switch

#### Connector Part Information

- OEM: AK07207
- Service: N/A
- Description: 2-Way F

#### Trunk Tamper Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | -- | Tamper Switch Signal
2 | BK | -- | Ground

### Turn Signal Lamp - Left Front (TR6)

#### Connector Part Information

- OEM: 936184-1
- Service: N/A
- Description: 2-Way F 090 Series (WH)

#### Turn Signal Lamp - Left Front (TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage

### Turn Signal Lamp - Right Front (TR6)

#### Connector Part Information

- OEM: 936184-1
- Service: N/A
- Description: 2-Way F 090 Series (WH)

#### Turn Signal Lamp - Right Front (TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 150 | Ground
2 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage

### Turn Signal/Park Lamp - Left Front (-TR6)

#### Connector Part Information

- OEM: 936187-3
- Service: N/A
- Description: 3-Way F

#### Turn Signal/Park Lamp - Left Front (-TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | PU | 709 | Left Park Lamp Supply Voltage
3 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

### Turn Signal/Park Lamp - Right Front (-TR6)

#### Connector Part Information

- OEM: 936187-3
- Service: N/A
- Description: 3-Way F

#### Turn Signal/Park Lamp - Right Front (-TR6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 150 | Ground
2 | BN/WH | 309 | Right Park Lamp Supply Voltage
3 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage

### Tweeter - Left Front

#### Connector Part Information

- OEM: MG610070
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### Tweeter - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | -- | Left Front Speaker Return
2 | BN | -- | Left Front Speaker Feed

### Tweeter - Left Rear

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: 2-Way F 250 Series (NA)

#### Tweeter - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Left Rear Speaker Return
2 | WH | -- | Left Rear Speaker Feed

### Tweeter - Right Front

#### Connector Part Information

- OEM: MG610070
- Service: N/A
- Description: 2-Way F 090 Series (NA)

#### Tweeter - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | -- | Right Front Speaker Return
2 | L-GN | -- | Right Front Speaker Feed

### Tweeter - Right Rear

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: 2-Way F 250 Series (NA)

#### Tweeter - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Left Rear Speaker Return
2 | WH | -- | Left Rear Speaker Feed

### Vanity Lamp - Left

#### Connector Part Information

- OEM: AK36277
- Service: N/A
- Description: 2-Way F (BK)

#### Vanity Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Inadvertent Power Control
2 | BK | -- | Ground

### Vanity Lamp - Right

#### Connector Part Information

- OEM: AK36277
- Service: N/A
- Description: 2-Way F (BK)

#### Vanity Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Inadvertent Power Control
2 | BK | -- | Ground

### Vehicle Speed Sensor (MFB/MFN)

#### Connector Part Information

- OEM: AK32311
- Service: N/A
- Description: 3-Way F (BK)

#### Vehicle Speed Sensor (MFB/MFN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/BK | -- | Ground
2 | D-GN | -- | Vehicle Speed Signal
3 | PK | -- | Ignition 1 Voltage

### Water In Fuel Sensor (LLW)

#### Connector Part Information

- OEM: 85205-1
- Service: N/A
- Description: 3-Way F JPT Series, Sealed

#### Water In Fuel Sensor (LLW)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Signal
2 | BK | -- | Ground
3 | PK/WH | -- | Battery Positive Voltage

### Wheel Speed Sensor (WSS) - Left Front (JL9/NW9)

#### Connector Part Information

- OEM: 174352-2
- Service: N/A
- Description: 2-Way F Econoseal J Mark II Series (BK)

#### Wheel Speed Sensor (WSS) - Left Front (JL9/NW9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Left Front Wheel Speed Sensor Signal
2 | D-BU | -- | Left Front Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Left Rear (JL9/NW9)

#### Connector Part Information

- OEM: PB621-02020
- Service: N/A
- Description: 2-Way M (BK)

#### Wheel Speed Sensor (WSS) - Left Rear (JL9/NW9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Left Rear Wheel Speed Sensor Low Reference
2 | BN | -- | Left Rear Wheel Speed Sensor Signal

### Wheel Speed Sensor (WSS) - Right Front (JL9/NW9)

#### Connector Part Information

- OEM: 174352-2
- Service: N/A
- Description: 2-Way F Econoseal J Mark II Series (BK)

#### Wheel Speed Sensor (WSS) - Right Front (JL9/NW9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Right Front Wheel Speed Sensor Signal
2 | D-BU/WH | -- | Right Front Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Right Rear (JL9/NW9)

#### Connector Part Information

- OEM: PB621-02020
- Service: N/A
- Description: 2-Way M (BK)

#### Wheel Speed Sensor (WSS) - Right Rear (JL9/NW9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU/BK | -- | Right Rear Wheel Speed Sensor Low Reference
2 | BN/WH | -- | Right Rear Wheel Speed Sensor Signal

### Window/Door Lock Switch - Driver X1

#### Connector Part Information

- OEM: MG651056
- Service: N/A
- Description: 10-Way F 090-II Series (WH)

#### Window/Door Lock Switch - Driver X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Power Window Master Switch Right Rear Up Signal
2 | PU | -- | Power Window Master Switch Right Rear Down Signal
3 | D-GN | -- | Power Window Master Switch Left Rear Up Signal
4 | PU | -- | Power Window Master Switch Left Rear Down Signal
5 | L-BU | -- | Power Window Master Switch Passenger Front Down Signal (LHD)
BN | -- | Power Window Motor Driver Front Down Control (AA7, RHD w/ABZ)
6 | OG | -- | Power Window Supply Voltage Ground (LHD w/ABZ)
BK | -- | Ground (RHD)
7 | OG | -- | Power Window Supply Voltage (AA7, RHD w/ABZ)
BN | -- | Power Window Master Switch Passenger Front Down Signal (LHD)
8 | BN | -- | Power Window Motor Driver Front Down Control (LHD w/ABZ)
L-BU | -- | Power Window Master Switch Passenger Front Down Signal (RHD)
9 | PK/BK | -- | Power Window Master Switch Lockout Control (LHD)
BN | -- | Power Window Master Switch Passenger Front Down Signal (RHD
10 | BK | -- | Ground (LHD)
PK/BK | -- | Power Window Master Switch Lockout Control (RHD)

### Window/Door Lock Switch - Driver X2

#### Connector Part Information

- OEM: MG651044
- Service: N/A
- Description: 6-Way F 090 II Series (WH)

#### Window/Door Lock Switch - Driver X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Power Window Motor Driver Front Up Control
2 | L-GN | -- | Power Window Switch Driver Front Express Down Signal (ABZ)
OG | -- | Power Window Switch Driver Front Express Down Signal (AA7)
3 | -- | -- | Not Used
4 | L-BU | -- | Door Lock Control
5 | WH | -- | Door Unlock Control
6 | L-GN | -- | Auto Up (ABZ)

### Window/Door Lock Switch - Passenger

#### Connector Part Information

- OEM: MG651050
- Service: N/A
- Description: 8-Way F 090-II Series (WH)

#### Window/Door Lock Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | -- | Power Window Master Switch Passenger Front Up Signal
2 | D-BU | -- | Power Window Master Switch Lockout Control
3 | BN | -- | Power Window Master Switch Passenger Front Down Signal
4 | D-BU | -- | Power Window Motor Passenger Front Up Control
5 | L-BU | -- | Door Lock Control
6 | BK | -- | Ground
7 | WH | -- | Door Unlock Control
8 | BN | -- | Power Window Motor Passenger Front Down Control

### Window Motor - Driver (AA7)

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: 2-Way F 250 Series (WH)

#### Window Motor - Driver (AA7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Power Window Switch Drivers Up Signal
2 | D-BU/WH | -- | Power Window Switch Drivers Down Signal

### Window Motor - Driver (ABZ)

#### Connector Part Information

- OEM: PB625-06027
- Service: N/A
- Description: 6-Way F NMWP-06 Series (BK)

#### Window Motor - Driver (ABZ)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | -- | Auto Input
2 | BN | -- | Manual Down Input
3 | BK | -- | Ground
4 | -- | -- | Not Used
5 | YE | -- | Manual Up Input
6 | OG | -- | Window Relay Output

### Window Motor - Left Rear

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: 2-Way F 250 Series (WH)

#### Window Motor - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Power Window Motor Left Rear Up Control
2 | BN | -- | Power Window Motor Left Rear Down Control

### Window Motor - Passenger

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: 2-Way F 250 Series (WH)

#### Window Motor - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Power Window Motor Right Front Up Control
2 | BN | -- | Power Window Motor Right Front Down Control

### Window Motor - Right Rear

#### Connector Part Information

- OEM: MG610043
- Service: N/A
- Description: 2-Way F250 Series (WH)

#### Window Motor - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Power Window Motor Right Rear Up Control
2 | BN | -- | Power Window Motor Right Rear Down Control

### Window Switch - Left Rear

#### Connector Part Information

- OEM: MG610663
- Service: N/A
- Description: 8-Way F (WH)

#### Window Switch - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Power Window Master Switch Left Rear Up Signal
2 | D-GN | -- | Power Window Master Switch Left Rear Up Control
3 | PK/D-BU | -- | Power Window Master Switch Lockout Control
4 | BK | -- | Ground
5 | PU | -- | Power Window Motor Left Rear Down Control
6 | BN | -- | Power Window Master Switch Left Rear Down Signal
7-8 | -- | -- | Not Used

### Window Switch - Right Rear

#### Connector Part Information

- OEM: MG610663
- Service: N/A
- Description: 8-Way F (WH)

#### Window Switch - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | -- | Power Window Master Switch Right Rear Up Signal
2 | D-GN | -- | Power Window Master Switch Right Rear Up Control
3 | PK/D-BU | -- | Power Window Master Switch Lockout Control
4 | BK | -- | Ground
5 | PU | -- | Power Window Motor Master Switch Right Rear Down Control
6 | BN | -- | Power Window Master Switch Right Rear Down Signal
7-8 | -- | -- | Not Used

### Windshield Washer Fluid Pump - Front

#### Connector Part Information

- OEM: MG640605
- Service: N/A
- Description: 2-Way F 090 WP Series (WH)

#### Windshield Washer Fluid Pump - Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | -- | Windshield Washer Pump Control
2 | BK | -- | Ground

### Windshield Washer Fluid Switch

#### Connector Part Information

- OEM: 174352-2
- Service: N/A
- Description: 2-Way F Econoseal J-Mark II Series, Sealed (BK)

#### Windshield Washer Fluid Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 150 | Ground
2 | YE | 196 | Windshield Washer Fluid Level Signal

### Windshield Wiper Motor

#### Connector Part Information

- OEM: PB625-06027
- Service: N/A
- Description: 6-Way F NMWP 06F-B Series (BK)

#### Windshield Wiper Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BN/WH | -- | Windshield Wiper Switch Pulse Delay Signal
3 | PK | -- | Battery Positive Voltage
4 | BK | -- | Ground
5 | D-GN | -- | Windshield Wiper Switch Signal
6 | PU/WH | -- | Windshield Wiper Motor High Speed

### Windshield Wiper/Washer Switch X1

#### Connector Part Information

- OEM: MG610154
- Service: N/A
- Description: 9-Way F 118 (PA) Series (WH)

#### Windshield Wiper/Washer Switch X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | PK | 639 | Ignition 1 Voltage
4 | OG | 228 | Windshield Washer Pump Control
OG | 228 | Windshield Washer Switch Signal
5 | D-GN | 95 | Windshield Wiper Switch Signal
6 | L-BU | 97 | Windshield Wiper Switch MIST/OFF/LOW Signal
7 | D-GN/WH | 91 | Intermittent Windshield Wiper Switch Control
8 | PK | 939 | Battery Positive Voltage
9 | PU | 92 | Wiper Motor HI Signal

### Windshield Wiper/Washer Switch X2

#### Connector Part Information

- OEM: 174460-1
- Service: N/A
- Description: 2-Way F 070 Multilock Series (WH)

#### Windshield Wiper/Washer Switch X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 91 | Windshield Wiper Switch Pulse Delay Signal
2 | D-BU/WH | 6985 | Windshield Wiper Switch Signal 2

### Winter Mode Switch (M98)

#### Connector Part Information

- OEM: MG652999
- Service: N/A
- Description: 4-Way F 040 Series (NA)

#### Winter Mode Switch (M98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | -- | Ground
2 | L-GN | -- | Winter Mode Switch Signal
3 | BN/WH | -- | Illumination Control
4 | GN | -- | Ground

### Yaw Rate Sensor (F45)

#### Connector Part Information

- OEM: PH845-05010
- Service: N/A
- Description: 5-Way F CDR Series (WH)

#### Yaw Rate Sensor (F45)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/BK | 2500 | High Speed GMLAN Serial Data (+)
2 | -- | -- | Not Used
3 | BK | 650 | Ground
4 | PK | 839 | 12V Reference
5 | BN | 2501 | High Speed GMLAN Serial Data (-)