For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster. Refer to Instrument Cluster Replacement.
3. Press the clips down and remove the instrument cluster lens.
4. Remove the tachometer from the instrument cluster.

### Installation Procedure

1. Install the tachometer to the instrument cluster.
2. Install the instrument cluster lens.
3. Install the instrument cluster. Refer to Instrument Cluster Replacement.
4. Connect the negative battery cable.