For 1990-2009 cars

Scan Tool Output Control | Additional Menu Selections | Description
--- | --- | ---
Automated Bleed | -- | Used in order to bleed the ABS hydraulics
LF Inlet Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
LF Outlet Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
LF TCS Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
LR Inlet Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
LR Outlet Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
Pump Motor Test | -- | Commands the pump motor ON and OFF
RF Inlet Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
RF Outlet Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
RF TCS Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
RR Inlet Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF
RR Outlet Solenoid Valve Test | Solenoid Test | Commands the solenoid ON and OFF