For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Antilock Brake System (ABS) Main Relay Operation Voltage | 9-16 V
Antilock Brake System (ABS) Mode | 4 Channel 4 Sensor
Speed Ring

- Inside Diameter - Front

61.9 mm

2.4370 in

- Inside Diameter - Rear

28.1 mm

1.1063 in

- Outside Diameter - Front

70.4 mm

2.7716 in

- Outside Diameter - Rear

41.13 mm

1.6192 in

- Tooth Volume of the Speed Ring

47 EA

Wheel Speed Sensor - Resistance | 1,040-1,161 Ω