For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Bleeder Valve | 6 N·m | 53 lb in
Booster Pushrod Hex Nut | 18 N·m | 13 lb ft
Booster-to-Dash Panel Nuts | 22 N·m | 16 lb ft
Brake Lines Fittings | 16 N·m | 12 lb ft
Brake Pedal-to-Pedal Bracket Hex Nut | 18 N·m | 13 lb ft
Front Disc Brake Hose-to-Caliper Bolt | 40 N·m | 30 lb ft
Master Cylinder Brake Lines | 16 N·m | 12 lb ft
Master Cylinder Mounting Nuts | 13 N·m | 115 lb in
Proportioning Valve Brake Lines | 16 N·m | 12 lb ft
Proportioning Valve Nut | 10 N·m | 7 lb ft
Pushrod Clevis | 18 N·m | 13 lb ft
Rear Disc Brake Hose-to-Caliper Bolt | 32 N·m | 24 lb ft
Trim Panel Screws | 3 N·m | 27 lb in